{"text_format":"2","workbook":"xls","n_sheets":1,"sheets":["Products"],"not_rendered":{"charts":0,"images":0,"macros":0,"external_links":1,"defined_names":0,"comments":0,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"run_cost":"one","rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900","formulas":"cached_only"}

{"sheet":"Products","index":0,"n_rows":47,"n_cols":9,"rows_kept":47,"cut":false,"hidden":false,"merged":[],"flags":["formulas_cached_only"]}
["PRODUCT NAME","FTXF-C"]
[]
[]
[]
[]
["","","","","","FTXF20C5V1B","FTXF25C5V1B","FTXF35C5V1B","FTXF42C5V1B"]
["Elektromos bemenet","Hűtés","","Névl.","kW","0.023","0.023","0.029","0.04"]
["","Fűtés","","Névl.","kW","0.023","0.023","0.029","0.04"]
["Burkolat","Szín","","","","Fehér","Fehér","Fehér","Fehér"]
["Méretek","Egység","","Magasság","mm","286","286","286","286"]
["","","","Szélesség","mm","770","770","770","770"]
["","","","Mélység","mm","225","225","225","225"]
["Tömeg","Egység","","","kg","8","8","8.5","9"]
["Ventilátor","Légáramlási arány","Hűtés","Magas","m³/perc","8.3","8.5","11.8","12.6"]
["","Légszállítási sebesség","Hűtés","Közepes","m³/perc","6","6","8","9"]
["","","","Alacsony","m³/perc","4.6","4.6","6.4","6.9"]
["","","","Csendes működés","m³/perc","3.6","3.6","4.4","4.9"]
["","","Fűtés","Magas","m³/perc","9.7","9.7","11.9","12.8"]
["","Légszállítási sebesség","Fűtés","Közepes","m³/perc","7.8","7.9","8.6","8.8"]
["","","Fűtés","Alacsony","m³/perc","5.8","6","6.5","6.7"]
["","","","Csendes működés","m³/perc","4.6","4.6","5.3","5.2"]
["Hangteljesítményszint","Hűtés","","","dB(A)","53","54","54","59"]
["","Fűtés","","","dB(A)","55","55","56","59"]
["Hangnyomás szint","Hűtés","","Magas","dB(A)","39","40","43","45"]
["Hangnyomásszint","Hűtés","","Közepes","dB(A)","33","33","34","36"]
["Hangnyomás szint","Hűtés","","Alacsony","dB(A)","25","26","27","30"]
["","","","Csendes működés","dB(A)","20","20","20","22"]
["","Fűtés","","Magas","dB(A)","39","40","40","44"]
["Hangnyomásszint","Fűtés","","Közepes","dB(A)","34","34","35","34"]
["Hangnyomás szint","Fűtés","","Alacsony","dB(A)","28","28","29","28"]
["","","","Csendes működés","dB(A)","21","21","21","22"]
["Csőcsatlakozások","Folyadék","","Külső átm.","mm","6.35","6.35","6.35","6.35"]
["","Gáz","","Külső átm.","mm","9.5","9.5","9.5","9.5"]
["","Ürítés","","","","18","18","18","18"]
["Vezérlőrendszerek","Infravörös távszabályzó","","","","ARC470A1","ARC470A1","ARC470A1","ARC470A1"]
["","Vezetékes távszabályzó","","","","BRC073A1","BRC073A1","BRC073A1","BRC073A1"]
["Standard Accessories","Installation manual","","","","1","1","1","1"]
["","AAA dry-cell batteries","","","","2","2","2","2"]
["","Operation manual","","","","1","1","1","1"]
["","Batteries","","","","1","1","1","1"]
["","Indoor unit fixing screws","","","","2","2","2","2"]
["","Infrared remote control","","","","1","1","1","1"]
["","Mounting plate","","","","1","1","1","1"]
["","Remote control holder","","","","1","1","1","1"]
["Áramellátás","fázis","","","","1~","1~","1~","1~"]
["","Frekvencia","","","Hz","50","50","50","50"]
["","Feszültség","","","V","220-440","220-440","220-440","220-440"]