{"text_format":"2","workbook":"xls","n_sheets":1,"sheets":["Products"],"not_rendered":{"charts":0,"images":0,"macros":0,"external_links":1,"defined_names":0,"comments":0,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"run_cost":"one","rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900","formulas":"cached_only"}

{"sheet":"Products","index":0,"n_rows":90,"n_cols":12,"rows_kept":90,"cut":false,"hidden":false,"merged":[],"flags":["formulas_cached_only"]}
["PRODUCT NAME","FTXF-D"]
[]
[]
[]
[]
["","","","","","FTXF20D5V1B","FTXF25D5V1B","FTXF35D5V1B","FTXF42D5V1B","FTXF50D2V1B","FTXF60D2V1B","FTXF71D2V1B"]
["Áramfelvétel","Hűtés","","Névl.","kW","","","","","0.029","","0.032"]
["","Fűtés","","Névl.","kW","","","","","0.032","","0.035"]
["Burkolat","Colour","","","","","","","","Fehér","","Fehér"]
["Befoglaló méretek","Berendezés","","Magasság","mm","","","","","295","","295"]
["","","","Szélesség","mm","","","","","990","","990"]
["","","","Mélység","mm","","","","","263","","263"]
["Súly","Egység","","","kg","","","","","13.5","","13.5"]
["Ventilátor","Légáramlási arány","Hűtés","Magas","m³/perc","","","","","16.8","","17.3"]
["","","","Medium","m³/perc","","","","","14.4","","14.8"]
["","","","Alacsony","m³/perc","","","","","11.9","","12.2"]
["","","","Csendes működés","m³/perc","","","","","10.5","","10.7"]
["","","Fűtés","Magas","m³/perc","","","","","17.3","","17.9"]
["","","","Medium","m³/perc","","","","","14.8","","15.8"]
["","","","Alacsony","m³/perc","","","","","12.2","","12.8"]
["","","","Csendes működés","m³/perc","","","","","10.7","","11.3"]
["Hangteljesítmény szintje","Hűtés","","","dB(A)","","","","","59","","62"]
["","Fűtés","","","dB(A)","","","","","61","","62"]
["Hangnyomás szint","Hűtés","","Magas","dB(A)","","","","","43","","46"]
["","","","Medium","dB(A)","","","","","39","","42"]
["","","","Alacsony","dB(A)","","","","","34","","37"]
["","","","Csendes működés","dB(A)","","","","","31","","34"]
["","Fűtés","","Magas","dB(A)","","","","","42","","45"]
["","","","Közepes","dB(A)","","","","","38","","41"]
["","","","Alacsony","dB(A)","","","","","33","","36"]
["","","","Csendes működés","dB(A)","","","","","30","","33"]
["Csőcsatlakozások","Liquid","","OD","mm","","","","","6.35","","6.35"]
["","Gáz","","külső átm.","mm","","","","","12.7","","12.7"]
["","Ürítés","","","","","","","","18","","18"]
["Vezérlőrendszerek","Infravörös távszabályzó","","","","","","","","ARC470A1","","ARC470A1"]
["","Wired remote control","","","","","","","","BRC073A1","","BRC073A1"]
["Standard Accessories","AAA szárazelemek","","","","","","","","2","","2"]
["","Telepítési utasítás","","","","","","","","1","","1"]
["","Használati utasítás","","","","","","","","1","","1"]
["","Infravörös távirányító","","","","","","","","1","","1"]
["","Távirányító tartó","","","","","","","","1","","1"]
["","Szerelőlemez","","","","","","","","1","","1"]
["","Beltéri egység rögzítő csavarja","","","","","","","","2","","2"]
["Áramellátás","Név","","","","","","","","V1","","V1"]
["","Fázis","","","","","","","","1~","","1~"]
["","Frekvencia","","","Hz","","","","","50","","50"]
["","Feszültség","","","V","","","","","220-240","","220-240"]
["Elektromos bemenet","Hűtés","","Névl.","kW","0.023","0.023","0.029","0.040","","0.032"]
["","Fűtés","","Névl.","kW","0.023","0.023","0.029","0.040","","0.035"]
["Burkolat","Szín","","","","Fehér","Fehér","Fehér","Fehér","","Fehér"]
["Méretek","Egység","","Magasság","mm","286","286","286","286","","295"]
["","","","Szélesség","mm","770","770","770","770","","990"]
["","","","Mélység","mm","225","225","225","225","","263"]
["Tömeg","Egység","","","kg","8","8","8.5","9.00","","13.5"]
["Ventilátor","Légáramlási arány","Hűtés","Magas","m³/perc","9.8","10","11.5","12.6","","17.3"]
["","Légszállítási sebesség","Hűtés","Közepes","m³/perc","8","8","8","9","","14.8"]
["","","","Alacsony","m³/perc","6","6.2","6.4","6.9","","12.2"]
["","","","Csendes működés","m³/perc","4.3","4.3","4.4","4.9","","10.7"]
["","","Fűtés","Magas","m³/perc","10.4","10.4","11.9","12.8","","17.9"]
["","Légszállítási sebesség","Fűtés","Közepes","m³/perc","8.3","8.4","8.6","8.8","","15.8"]
["","","Fűtés","Alacsony","m³/perc","6.2","6.4","6.5","6.7","","12.8"]
["","","","Csendes működés","m³/perc","5.3","5.3","5.3","5.2","","11.3"]
["Hangteljesítményszint","Hűtés","","","dB(A)","53","54","54","59.0","","60"]
["","Fűtés","","","dB(A)","55","55","56","59.0","","62"]
["Hangnyomás szint","Hűtés","","Magas","dB(A)","39","40","43","45.0","","45"]
["Hangnyomásszint","Hűtés","","Közepes","dB(A)","33","33","34","36.0","","41"]
["Hangnyomás szint","Hűtés","","Alacsony","dB(A)","25","26","27","30.0","","36"]
["","","","Csendes működés","dB(A)","20","20","20","22.0","","33"]
["","Fűtés","","Magas","dB(A)","39","40","40","44.0","","44"]
["Hangnyomásszint","Fűtés","","Közepes","dB(A)","34","34","35","34.0","","40"]
["Hangnyomás szint","Fűtés","","Alacsony","dB(A)","28","28","29","28.0","","35"]
["","","","Csendes működés","dB(A)","21","21","21","22.0","","32"]
["Csőcsatlakozások","Folyadék","","Külső átm.","mm","6","6","6","6","","6.35"]
["","Gáz","","Külső átm.","mm","9.5","9.5","9.5","9.50","","12.7"]
["","Ürítés","","","","18","18","18","18","","18"]
["Vezérlőrendszerek","Infravörös távszabályzó","","","","ARC470A1","ARC470A1","ARC470A1","ARC470A1","","ARC470A1"]
["","Vezetékes távszabályzó","","","","BRC073A1","BRC073A1","BRC073A1","BRC073A1","","BRC073A1"]
["Standard Accessories","Installation manual","","","","1","1","1","1","","1"]
["","AAA dry-cell batteries","","","","2","2","2","2","","2"]
["","General safety precautions","","","","196","196","196","196"]
["","Operation manual","","","","1","1","1","1","","1"]
["","Batteries","","","","1","1","1","1"]
["","Indoor unit fixing screws","","","","2","2","2","2","","2"]
["","Infrared remote control","","","","1","1","1","1","","1"]
["","Mounting plate","","","","1","1","1","1","","1"]
["","Remote control holder","","","","1","1","1","1","","1"]
["Áramellátás","fázis","","","","1~","1~","1~","1~","","1~"]
["","Frekvencia","","","Hz","50","50","50","50","","50"]
["","Feszültség","","","V","220-440","220-440","220-440","220-440","","220-240"]
["","Megnevezés","","","","","","","","","V1"]