{"text_format":"2","workbook":"xls","n_sheets":1,"sheets":["Products"],"not_rendered":{"charts":0,"images":0,"macros":0,"external_links":1,"defined_names":0,"comments":0,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"run_cost":"one","rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900","formulas":"cached_only"}

{"sheet":"Products","index":0,"n_rows":34,"n_cols":8,"rows_kept":34,"cut":false,"hidden":false,"merged":[],"flags":["formulas_cached_only"]}
["PRODUCT NAME","FTXJ-AB / RXJ-M9"]
[]
[]
[]
[]
["","","","","FTXJ20A2V1BB / RXJ20M5V1B9","FTXJ25A2V1BB / RXJ25M5V1B9","FTXJ35A2V1BB  / RXJ35M5V1B9","FTXJ35A2V1BB / RXJ35M5V1B9"]
["Hűtési teljesítmény","Névl.","","kW","","","3.50"]
["Normál hatékonyság","Éves energiafogyasztás","","kWh","","","428"]
["","EER","","","","","4.09"]
["","COP","","","","","4.04"]
["","Energiacímkézés irányelve","Hűtés","","","","A"]
["","","Fűtés","","","","A"]
["Fűtőkapacitás","Névl.","","kW","","","4.00"]
["Notes","","","","","","(1) - Az üzemi tartomány tekintetében ld. az önálló ábrát"]
["","","","","","","(2) - Az elektromos adatokat lásd külön rajzokon"]
["","","","","","","(3) - A névleges hűtési teljesítmények a következő feltételekre vonatkoznak: belső hőmérséklet: 27 °C száraz hőm., 19 °C nedves hőm., kültéri hőmérséklet: 35°C száraz, a hűtőközeg egyenértékű csővezetékhossza: 5m, szintkülönbség: 0m."]
["","","","","","","(4) - A névleges fűtési kapacitás alapja: belső hőmérséklet: 20°C száraz, kültéri hőmérséklet: 7 °C száraz, 6 °C párás, a hűtőközeg egyenértékű csővezetékhossza: 5m, szintkülönbség: 0m."]
["Outdoor unit","","","","RXJ20M5V1B9","RXJ25M5V1B9","","RXJ35M5V1B9"]
["Hűtési teljesítmény","Névl.","","kW","2.30","2.40","","3.50"]
["Fűtőkapacitás","Névl.","","kW","2.50","3.20","","4.00"]
["Névleges hatékonyság","EER","","","4.64","4.73","","4.09"]
["","COP","","","5.00","4.57","","4.04"]
["","Éves energiafogyasztás","","kWh","248","254","","428"]
["Normál hatékonyság","Energiacímkézés irányelve","Hűtés","","A","A","","A"]
["","","Fűtés","","A","A","","A"]
["Felülethűtés","Energiatakarékossági osztály","","","A+++","A+++","","A++"]
["","Kapacitás","Pdesign","kW","2.30","2.40","","3.50"]
["","SEER","","","8.73","8.64","","7.19"]
["","Éves energiafogyasztás","","kWh/a","92","97","","170"]
["Felülethűtés (Mérsékelt éghajlat)","Energiatakarékossági osztály","","","A++","A++","","A++"]
["","Kapacitás","Pdesign","kW","2.10","2.70","","3.00"]
["","SCOP/A","","","4.61","4.60","","4.60"]
["","Pdh fűtőteljesítmény -10 ° hőmérsékleten","","kW","1.80","2.18","","2.61"]
["","Éves energiafogyasztás","","kWh/a","638","822","","913"]