{"text_format":"2","workbook":"xls","n_sheets":1,"sheets":["Products"],"not_rendered":{"charts":0,"images":0,"macros":0,"external_links":1,"defined_names":0,"comments":0,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"run_cost":"one","rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900","formulas":"cached_only"}

{"sheet":"Products","index":0,"n_rows":54,"n_cols":9,"rows_kept":54,"cut":false,"hidden":false,"merged":[],"flags":["formulas_cached_only"]}
["PRODUCT NAME","FTXJ-MS"]
[]
[]
[]
[]
["","","","","","FTXJ20MV1BS","FTXJ25MV1BS","FTXJ35MV1BS","FTXJ50MV1BS"]
["Elektromos bemenet","Hűtés","","Névl.","kW","0.023","0.023","0.033","0.033"]
["","Fűtés","","Névl.","kW","0.031","0.033","0.042","0.043"]
["Burkolat","Szín","","","","Ezüst","Ezüst","Ezüst","Ezüst"]
["Méretek","Egység","","Magasság","pp","303","303","303","303"]
["","","","Szélesség","pp","998","998","998","998"]
["","","","Mélység","pp","212","212","212","212"]
["Tömeg","Egység","","","kg","12","12","12","12"]
["Ventilátor","Légáramlási arány","Hűtés","Magas","m³/perc","8.9","8.9","10.9","10.9"]
["","Légszállítási sebesség","Hűtés","Közepes","m³/perc","6.6","6.6","7.8","8.9"]
["","","","Alacsony","m³/perc","4.4","4.4","4.8","6.8"]
["","","","Csendes működés","m³/perc","2.6","2.6","2.9","3.6"]
["","","Fűtés","Magas","m³/perc","10.2","11.0","12.4","12.6"]
["","Légszállítási sebesség","Fűtés","Közepes","m³/perc","8.4","8.6","9.6","10.5"]
["","","Fűtés","Alacsony","m³/perc","6.3","6.3","6.9","8.1"]
["","","","Csendes működés","m³/perc","3.8","3.8","4.1","5.0"]
["Hangteljesítményszint","Hűtés","","","dB(A)","54","54","59","60"]
["","Fűtés","","","dB(A)","56","56","59","60"]
["Hangnyomás szint","Hűtés","","Magas","dB(A)","38","38","45","46"]
["Hangnyomásszint","Hűtés","","Közepes","dB(A)","32","32","34","40"]
["Hangnyomás szint","Hűtés","","Alacsony","dB(A)","25","25","26","35"]
["","","","Csendes működés","dB(A)","19","19","20","25"]
["","Fűtés","","Magas","dB(A)","40","41","45","47"]
["Hangnyomásszint","Fűtés","","Közepes","dB(A)","34","34","37","41"]
["Hangnyomás szint","Fűtés","","Alacsony","dB(A)","28","28","29","35"]
["","","","Csendes működés","dB(A)","19","19","20","25"]
["Csőcsatlakozások","Folyadék","","Külső átm.","pp","6.35","6.35","6.35","6.35"]
["","Gáz","","Külső átm.","pp","9.50","9.50","9.50","12.70"]
["","Ürítés","","","","18","18","18","18"]
["Vezérlőrendszerek","Infravörös távszabályzó","","","","ARC466A9","ARC466A9","ARC466A9","ARC466A9"]
["Standard Accessories","Installation manual","","","","1","1","1","1"]
["","Wireless remote control","","","","1","1","1","1"]
["","Screw cover","","","","2","2","2","2"]
["","AAA dry-cell batteries","","","","2","2","2","2"]
["","Fixing screw for remote controller holder","","","","2","2","2","2"]
["","WLAN adapter kit","","","","1","1","1","1"]
["","Operation manual","","","","1","1","1","1"]
["","Titanium apatite deodorizing filter","","","","2","2","2","2"]
["","Fixing screws for mounting plate","","","","5","5","5","5"]
["","Indoor unit fixing screws","","","","2","2","2","2"]
["","Mounting plate","","","","1","1","1","1"]
["","Remote control holder","","","","1","1","1","1"]
["Áramellátás","Megnevezés","","","","V1","V1","V1","V1"]
["","fázis","","","","1~","1~","1~","1~"]
["","Frekvencia","","","Hz","50","50","50","50"]
["","Feszültség","","","V","220-240","220-240","220-240","220-240"]
["Notes","","","","","(1) - 220V","(1) - 220V","(1) - 220V","(1) - 220V"]
["","","","","","(2) - 230V","(2) - 230V","(2) - 230V","(2) - 230V"]
["","","","","","(3) - 240V","(3) - 240V","(3) - 240V","(3) - 240V"]