{"text_format":"2","workbook":"xls","n_sheets":1,"sheets":["Products"],"not_rendered":{"charts":0,"images":0,"macros":0,"external_links":1,"defined_names":0,"comments":0,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"run_cost":"one","rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900","formulas":"cached_only"}

{"sheet":"Products","index":0,"n_rows":22,"n_cols":8,"rows_kept":22,"cut":false,"hidden":false,"merged":[],"flags":["formulas_cached_only"]}
["PRODUCT NAME","FTXN-L / RXN-L"]
[]
[]
[]
[]
["","","","","FTXN25LV1B / RXN25LV1B","FTXN35LV1B / RXN35LV1B","FTXN50LV1B / RXN50LV1B","FTXN60LV1B / RXN60LV1B"]
["Hűtési teljesítmény","Min.","","kW","1.30","1.30","1.88","2.00"]
["","Max.","","kW","2.80","3.50","6.20","6.50"]
["","Névl.","","kW","2.50","3.20","5.45","6.21"]
["Csőcsatlakozások","Folyadék","Külső átm.","mm","6.35","6.35","6.35","6.35"]
["","Gáz","Külső átm.","mm","9.52","9.52","12.70","15.90"]
["","Ürítés","külső átm.","mm","16.5","16.5","16.5","16.5"]
["Normál hatékonyság","Éves energiafogyasztás","","kWh","390","498","850","965"]
["","EER","","","3.21","3.22","3.21","3.22"]
["","COP","","","3.61","3.61","3.61","3.62"]
["","Energiacímkézés irányelve","Hűtés","","A","A","A","A"]
["","","Fűtés","","A","A","A","A"]
["Fűtőkapacitás","Névl.","","kW","2.80","3.50","5.62","6.40"]
["","Min.","","kW","1.30","1.30","1.32","1.56"]
["","Max.","","kW","3.70","4.00","6.60","7.10"]
["Notes","","","","(1) - EER/COP értékek az Eurovent 2012 szerint, csak EU-n kívüli országokra vonatkozóan","(1) - EER/COP értékek az Eurovent 2012 szerint, csak EU-n kívüli országokra vonatkozóan","(1) - EER/COP értékek az Eurovent 2012 szerint, csak EU-n kívüli országokra vonatkozóan","(1) - EER/COP értékek az Eurovent 2012 szerint, csak EU-n kívüli országokra vonatkozóan"]
["","","","","(2) - Névleges hatékonyság: hűtés 35°/27° névleges terhelésen, fűtés 7°/20° névleges terhelésen","(2) - Névleges hatékonyság: hűtés 35°/27° névleges terhelésen, fűtés 7°/20° névleges terhelésen","(2) - Névleges hatékonyság: hűtés 35°/27° névleges terhelésen, fűtés 7°/20° névleges terhelésen","(2) - Névleges hatékonyság: hűtés 35°/27° névleges terhelésen, fűtés 7°/20° névleges terhelésen"]