{"text_format":"2","workbook":"xls","n_sheets":1,"sheets":["Products"],"not_rendered":{"charts":0,"images":0,"macros":0,"external_links":1,"defined_names":0,"comments":0,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"run_cost":"one","rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900","formulas":"cached_only"}

{"sheet":"Products","index":0,"n_rows":55,"n_cols":11,"rows_kept":55,"cut":false,"hidden":false,"merged":[],"flags":["formulas_cached_only"]}
["PRODUCT NAME","FTXP-N"]
[]
[]
[]
[]
["","","","","","FTXP35N5V1B","FTXP50N2V1B","FTXP60N2V1B","FTXP71N2V1B","FTXP20N5V1B (Archived)","FTXP25N5V1B (Archived)"]
["Elektromos bemenet","Hűtés","","Névl.","kW","0.032","0.029","0.032","0.032","0.019","0.02"]
["","Fűtés","","Névl.","kW","0.032","0.032","0.035","0.035","0.023","0.023"]
["Burkolat","Szín","","","","Fehér","Fehér","Fehér","Fehér","Fehér","Fehér"]
["Méretek","Egység","","Magasság","pp","286","295","295","295","286","286"]
["","","","Szélesség","pp","770","990","990","990","770","770"]
["","","","Mélység","pp","225","263","263","263","225","225"]
["Tömeg","Egység","","","kg","9","13.5","13.5","13.5","8.5","8.5"]
["Ventilátor","Légáramlási arány","Hűtés","Magas","m³/perc","11.5","16.3","16.8","16.8","9.5","9.7"]
["","Légszállítási sebesség","Hűtés","Közepes","m³/perc","8.3","14","14.4","14.4","7.4","7.7"]
["","","","Alacsony","m³/perc","6.3","11.5","11.8","11.8","5.6","5.8"]
["","","","Csendes működés","m³/perc","4.5","8.3","9.2","10.1","4.2","4.2"]
["","","Fűtés","Magas","m³/perc","11.5","17.3","17.9","17.9","10.4","10.4"]
["","Légszállítási sebesség","Fűtés","Közepes","m³/perc","9","14.4","15.3","15.3","8.1","8.1"]
["","","Fűtés","Alacsony","m³/perc","7","11.8","12.4","12.4","6.2","6.4"]
["","","","Csendes működés","m³/perc","5.3","10.4","11","11","5.2","5.2"]
["Hangteljesítményszint","Hűtés","","","dB(A)","58","59","60","62","55","55"]
["","Fűtés","","","dB(A)","58","61","62","62","55","55"]
["Hangnyomás szint","Hűtés","","Magas","dB(A)","43","43","45","46","39","40"]
["Hangnyomásszint","Hűtés","","Közepes","dB(A)","34","39","41","42","33","33"]
["Hangnyomás szint","Hűtés","","Alacsony","dB(A)","27","34","36","37","25","26"]
["","","","Csendes működés","dB(A)","20","27","30","32","19","19"]
["","Fűtés","","Magas","dB(A)","40","42","44","45","39","40"]
["Hangnyomásszint","Fűtés","","Közepes","dB(A)","35","38","40","41","34","34"]
["Hangnyomás szint","Fűtés","","Alacsony","dB(A)","29","33","35","36","28","28"]
["","","","Csendes működés","dB(A)","21","30","32","33","21","21"]
["Csőcsatlakozások","Folyadék","","Külső átm.","pp","6","6.4","6.4","6.4","6","6"]
["","Gáz","","Külső átm.","pp","9.5","12.7","12.7","12.7","9.5","9.5"]
["","Ürítés","","","","18","18","18","18","18","18"]
["Vezérlőrendszerek","Infrared remote control","","","","ARC480A78","ARC480A53","ARC480A53","ARC480A53"]
["Vezérlőrendszerek","Vezetékes távszabályzó","","","","BRC944B2, BRC073A1","","","","BRC944B2, BRC073A1","BRC944B2, BRC073A1"]
["Standard Accessories","Installation manual","","","","1","1","1","1","1","1"]
["","AAA dry-cell batteries","","","","2","2","2","2","2","2"]
["","General safety precautions","","","","1","","","","1","1"]
["","Operation manual","","","","1","1","1","1","1","1"]
["","Titanium apatite deodorizing filter","","","","1","1","1","1","1","1"]
["","Silver particle filter","","","","1","1","1","1","1","1"]
["","Indoor unit fixing screws","","","","2","2","2","2","2","2"]
["","Infrared remote control","","","","1","1","1","1","1","1"]
["","Mounting plate","","","","1","1","1","1","1","1"]
["","Remote control holder","","","","1","1","1","1","1","1"]
["Áramellátás","Megnevezés","","","","","V1","V1","V1"]
["","fázis","","","","1~","1~","1~","1~","1~","1~"]
["","Frekvencia","","","Hz","50","50","50","50","50","50"]
["","Feszültség","","","V","220-240","220-240","220-240","220-240","220-240","220-240"]
["Standard Accessories","WLAN adapter kit","","","","","1","1","1"]
["Vezérlőrendszerek","Infravörös távszabályzó","","","","","","","","ARC480A78","ARC480A78"]
["Notes","","","","","","","","","(1) - Hűtés: belső hőm. 27 °C száraz, 19 °C nedves hőm.; kültéri hőm. 35°C száraz hőmérséklet; egyenlő csőhossz: 5 m; szintkülönbség: 0m","(1) - Hűtés: belső hőm. 27 °C száraz, 19 °C nedves hőm.; kültéri hőm. 35°C száraz hőmérséklet; egyenlő csőhossz: 5 m; szintkülönbség: 0m"]
["","","","","","","","","","(2) - Fűtés: belső hőm. 20°C száraz hőm.; külső hőm. 7 °C száraz hőm., 6 °C nedves hőm.; a hűtőközeg egyenértékű csővezetékhossza: 5m (vízszintes)","(2) - Fűtés: belső hőm. 20°C száraz hőm.; külső hőm. 7 °C száraz hőm., 6 °C nedves hőm.; a hűtőközeg egyenértékű csővezetékhossza: 5m (vízszintes)"]
["","","","","","","","","","(3) - Az elektromos adatokat lásd külön rajzokon","(3) - Az elektromos adatokat lásd külön rajzokon"]