{"text_format":"2","workbook":"xls","n_sheets":1,"sheets":["Products"],"not_rendered":{"charts":0,"images":0,"macros":0,"external_links":1,"defined_names":0,"comments":0,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"run_cost":"one","rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900","formulas":"cached_only"}

{"sheet":"Products","index":0,"n_rows":26,"n_cols":6,"rows_kept":26,"cut":false,"hidden":false,"merged":[],"flags":["formulas_cached_only"]}
["PRODUCT NAME","FTXQ-A / RXQ-A"]
[]
[]
[]
[]
["","","","","FTXQ25AMV1B / RXQ25AMV1B","FTXQ35AMV1B / RXQ35AMV1B"]
["Hűtési teljesítmény","Min.","","kW","1.30","1.30"]
["","Névl.","","kW","2.50","3.50"]
["","Max.","","kW","3.00","3.80"]
["Fűtőkapacitás","Min.","","kW","1.30","1.30"]
["","Névl.","","kW","3.00","3.90"]
["","Max.","","kW","3.90","4.80"]
["Névleges hatékonyság","EER","","","3.24","3.24"]
["","COP","","","3.71","3.71"]
["","Éves energiafogyasztás","","kWh","386","540"]
["Normál hatékonyság","Energiacímkézés irányelve","Hűtés","","A","A"]
["","","Fűtés","","A","A"]
["Felülethűtés","Energiatakarékossági osztály","","","A++","A++"]
["","Kapacitás","Pdesign","kW","2.50","3.50"]
["","SEER","","","6.22","6.21"]
["","Éves energiafogyasztás","","kWh/a","141","197"]
["Felülethűtés (Mérsékelt éghajlat)","Energiatakarékossági osztály","","","A+","A+"]
["","Kapacitás","Pdesign","kW","2.30","2.40"]
["","SCOP/A","","","4.22","4.12"]
["","Pdh fűtőteljesítmény -10 ° hőmérsékleten","","kW","1.81","1.90"]
["","Éves energiafogyasztás","","kWh/a","764","815"]