{"text_format":"2","workbook":"xls","n_sheets":1,"sheets":["Products"],"not_rendered":{"charts":0,"images":0,"macros":0,"external_links":1,"defined_names":0,"comments":0,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"run_cost":"one","rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900","formulas":"cached_only"}

{"sheet":"Products","index":0,"n_rows":86,"n_cols":7,"rows_kept":86,"cut":false,"hidden":false,"merged":[],"flags":["formulas_cached_only"]}
["PRODUCT NAME","FTXQ-A"]
[]
[]
[]
[]
["","","","","","FTXQ25AMV1B","FTXQ35AMV1B"]
["Hangnyomás szint","Fűtés","","Magas","dB(A)","","42.0"]
["","","","Közepes","dB(A)","","35.0"]
["","","","Csendes működés","dB(A)","","25.0"]
["","","","Alacsony","dB(A)","","30.0"]
["","Hűtés","","Közepes","dB(A)","","35.0"]
["","","","Csendes működés","dB(A)","","24.0"]
["","","","Alacsony","dB(A)","","28.0"]
["","","","Magas","dB(A)","","41.0"]
["Standard Accessories","Telepítési utasítás","","","","","1"]
["","Használati utasítás","","","","","1"]
["","AAA szárazelemek","","","","","2"]
["","Szerelőlemez","","","","","1"]
["","Beltéri egység rögzítő csavarja","","","","","2"]
["","Általános biztonsági óvintézkedések","","","","","1"]
["","Infravörös távirányító","","","","","1"]
["","Távirányító tartó","","","","","1"]
["Vezérlőrendszerek","Infrared remote control","","","","","ARC470A1"]
["Csőcsatlakozások","Folyadék","","Külső átm.","mm","","6.35"]
["","Gáz","","Külső átm.","mm","","9.50"]
["","Ürítés","","","","","18"]
["Áramfelvétel","Hűtés","","Névl.","kW","","0.025"]
["","Fűtés","","Névl.","kW","","0.031"]
["Sound power level","Hűtés","","","dB(A)","","55"]
["Méretek","Egység","","Szélesség","mm","","770"]
["","","","Mélység","mm","","232"]
["","","","Magasság","mm","","291"]
["Burkolat","Szín","","","","","Fehér"]
["Tömeg","Egység","","","kg","","9.00"]
["Ventilátor","Légáramlási arány","Fűtés","Magas","m³/perc","","12.0"]
["","","","Alacsony","m³/perc","","8.3"]
["","","","Medium","m³/perc","","10.0"]
["","","","Csendes működés","m³/perc","","6.9"]
["","","Hűtés","Alacsony","m³/perc","","7.0"]
["","","","Medium","m³/perc","","8.5"]
["","","","Magas","m³/perc","","10.5"]
["","","","Csendes működés","m³/perc","","6.0"]
["Power supply","fázis","","","","","1~"]
["","Frekvencia","","","Hz","","50"]
["","Feszültség","","","V","","220-240"]
["Notes","","","","","","(1) - Hűtés: belső hőm. 27°CDB, 19,0°CWB; kültéri hőm. 35°C száraz hőm., 24°C nedves hőm.; egyenlő csőhossz: 5m"]
["","","","","","","(2) - Fűtés: belső hőm. 20°C száraz hőm.; külső hőm. 7 °C száraz hőm., 6 °C nedves hőm.; a hűtőközeg egyenértékű csővezetékhossza: 5m"]
["Elektromos bemenet","Hűtés","","Névl.","kW","0.023"]
["","Fűtés","","Névl.","kW","0.027"]
["Burkolat","Szín","","","","Fehér"]
["Méretek","Egység","","Magasság","mm","291"]
["","","","Szélesség","mm","770"]
["","","","Mélység","mm","232"]
["Tömeg","Egység","","","kg","9"]
["Ventilátor","Légáramlási arány","Hűtés","Magas","m³/perc","10.2"]
["","Légszállítási sebesség","Hűtés","Közepes","m³/perc","8.1"]
["","","","Alacsony","m³/perc","6.5"]
["","","","Csendes működés","m³/perc","5"]
["","","Fűtés","Magas","m³/perc","11.1"]
["","Légszállítási sebesség","Fűtés","Közepes","m³/perc","9.6"]
["","","Fűtés","Alacsony","m³/perc","8.1"]
["","","","Csendes működés","m³/perc","6.8"]
["Hangteljesítményszint","Hűtés","","","dB(A)","55"]
["Hangnyomás szint","Hűtés","","Magas","dB(A)","40"]
["Hangnyomásszint","Hűtés","","Közepes","dB(A)","34"]
["Hangnyomás szint","Hűtés","","Alacsony","dB(A)","26"]
["","","","Csendes működés","dB(A)","23"]
["","Fűtés","","Magas","dB(A)","40"]
["Hangnyomásszint","Fűtés","","Közepes","dB(A)","34"]
["Hangnyomás szint","Fűtés","","Alacsony","dB(A)","29"]
["","","","Csendes működés","dB(A)","25"]
["Csőcsatlakozások","Folyadék","","Külső átm.","mm","6.35"]
["","Gáz","","Külső átm.","mm","9.5"]
["","Ürítés","","","","18"]
["Vezérlőrendszerek","Infravörös távszabályzó","","","","ARC470A1"]
["Standard Accessories","Installation manual","","","","1"]
["","AAA dry-cell batteries","","","","2"]
["","General safety precautions","","","","1"]
["","Operation manual","","","","1"]
["","Indoor unit fixing screws","","","","2"]
["","Infrared remote control","","","","1"]
["","Mounting plate","","","","1"]
["","Remote control holder","","","","1"]
["Áramellátás","fázis","","","","1~"]
["","Frekvencia","","","Hz","50"]
["","Feszültség","","","V","220-240"]