{"text_format":"2","workbook":"xls","n_sheets":1,"sheets":["Products"],"not_rendered":{"charts":0,"images":0,"macros":0,"external_links":1,"defined_names":0,"comments":0,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"run_cost":"one","rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900","formulas":"cached_only"}

{"sheet":"Products","index":0,"n_rows":85,"n_cols":12,"rows_kept":85,"cut":false,"hidden":false,"merged":[],"flags":["formulas_cached_only"]}
["PRODUCT NAME","FTXS-G"]
[]
[]
[]
[]
["","","","","","FTXS20G2V1B","FTXS25G2V1B","FTXS35G2V1B","FTXS42G2V1B","FTXS50G2V1B","FTXS60GV1B","FTXS71GV1B"]
["Hangnyomás szint","Fűtés","","Magas","dB(A)","38","39","42","42","44","","46"]
["","","","Csendes működés","dB(A)","25","25","26","30","31","","34"]
["","","","Alacsony","dB(A)","28","28","29","33","34","","37"]
["","Hűtés","","Csendes működés","dB(A)","22","22","23","30","31","","34"]
["","","","Alacsony","dB(A)","25","25","26","33","34","","37"]
["","","","Magas","dB(A)","38","38","42","42","43","","46"]
["","","","Névl.","dB(A)","33","34","36","38","39","","42"]
["","Hűtés","","Névl.","dB(A)","32","32","34","38","39","","42"]
["Standard Accessories","Titánium apatit fotokatalitikus légtisztító szűrő","","","","2","2","2","2","2"]
["","Használati utasítás","","","","1","1","1","1","1","","1"]
["","Telepítési utasítás","","","","1","1","1","1","1","","1"]
["","Vezeték nélküli távirányító","","","","1","1","1","1","1","","1"]
["","Elemek","","","","2","2","2","2","2","","2"]
["","Távirányító tartó","","","","1","1","1","1","1","","1"]
["","Beltéri egység rögzítő csavarja","","","","2","2","2","2","2","","2"]
["","Szerelőlemez","","","","1","1","1","1","1","","1"]
["Vezérlőrendszerek","Infrared remote control","","","","","","","","","","ARC452A3"]
["Csőcsatlakozások","Folyadék","","Külső átm.","mm","6.35","6.35","6.35","6.35","6.35","","6.35"]
["","Gáz","","Külső átm.","mm","9.52","9.52","9.52","9.52","12.70","","15.9"]
["","Ürítés","","","","18","18","18","18","18","","18"]
["Power input","Hűtés","","Névl.","kW","","","","","","","0.045 (2), 0.045 (3), 0.045 (4)"]
["","Fűtés","","Névl.","kW","","","","","","","0.060 (2), 0.060 (3), 0.060 (4)"]
["Sound power level","Hűtés","","","dB(A)","54","54","58","58","59","","63"]
["","Fűtés","","","dB(A)","54","55","58","58","60","","62"]
["Méretek","Egység","","Szélesség","mm","800","800","800","800","800","","1,050"]
["","","","Mélység","mm","215","215","215","215","215","","250"]
["","","","Magasság","mm","295","295","295","295","295","","290"]
["Burkolat","Szín","","","","Fehér","Fehér","Fehér","Fehér","Fehér","","Fehér"]
["Tömeg","Egység","","","kg","9","9","10","10","10","","12"]
["Power supply","fázis","","","","1~","1~","1~","1~","1~","","1~"]
["","Frekvencia","","","Hz","50","50","50","50","50","","50"]
["","Megnevezés","","","","V1","V1","V1","V1","V1","","V1"]
["","Feszültség","","","V","220-240","220-240","220-240","220-240","220-240","","220-240"]
["Notes","","","","","(1) - 220V","(1) - 220V","(1) - 220V","(1) - 220V","(1) - 220V","(1) - 220V","(1) - SL: A Légszállítási sebesség beállításának néma ventilátorszintje"]
["","","","","","(2) - 230V","(2) - 230V","(2) - 230V","(2) - 230V","(2) - 230V","(2) - 230V","(2) - 220V"]
["","","","","","(3) - 240V","(3) - 240V","(3) - 240V","(3) - 240V","(3) - 240V","(3) - 240V","(3) - 230V"]
["Ventilátor","Légáramlási arány","Hűtés","Névl.","m³/perc","","","","","","16.0"]
["Hangnyomás szint","Hűtés","","Névl.","dB(A)","","","","","","41"]
["Ventilátor","Légáramlási arány","Fűtés","Névl.","m³/perc","","","","","","14.9"]
["Hangnyomás szint","Fűtés","","Névl.","dB(A)","","","","","","40"]
["Elektromos bemenet","Hűtés","","Névl.","kW","","","","","","0.040 (4) (2) (3), 0.040 (4) (2) (3), 0.040 (4) (2) (3)"]
["","Fűtés","","Névl.","kW","","","","","","0.045 (4) (2) (3), 0.045 (4) (2) (3), 0.045 (4) (2) (3)"]
["Burkolat","Szín","","","","","","","","","Fehér"]
["Méretek","Egység","","Magasság","mm","","","","","","290"]
["","","","Szélesség","mm","","","","","","1050"]
["","","","Mélység","mm","","","","","","250"]
["Tömeg","Egység","","","kg","","","","","","12"]
["Ventilátor","Légáramlási arány","Hűtés","Magas","m³/perc","","","","","","16.0"]
["","","","Alacsony","m³/perc","","","","","","11.3"]
["","","","Csendes működés","m³/perc","","","","","","10.1"]
["","","Fűtés","Magas","m³/perc","","","","","","17.2"]
["","","","Alacsony","m³/perc","","","","","","12.6"]
["","","","Csendes működés","m³/perc","","","","","","11.3"]
["Hangteljesítményszint","Hűtés","","","dB(A)","","","","","","60"]
["","Fűtés","","","dB(A)","","","","","","59"]
["Hangnyomás szint","Hűtés","","Magas","dB(A)","","","","","","45"]
["","","","Alacsony","dB(A)","","","","","","36"]
["","","","Csendes működés","dB(A)","","","","","","33"]
["","Fűtés","","Magas","dB(A)","","","","","","44"]
["","","","Alacsony","dB(A)","","","","","","35"]
["","","","Csendes működés","dB(A)","","","","","","32"]
["Csőcsatlakozások","Folyadék","","Külső átm.","mm","","","","","","6.35"]
["","Gáz","","Külső átm.","mm","","","","","","12.7"]
["","Ürítés","","","","","","","","","18"]
["Vezérlőrendszerek","Infravörös távszabályzó","","","","","","","","","ARC452A3"]
["Standard Accessories","Installation manual","","","","","","","","","1"]
["","Wireless remote control","","","","","","","","","1"]
["","Operation manual","","","","","","","","","1"]
["","Batteries","","","","","","","","","2"]
["","Indoor unit fixing screws","","","","","","","","","2"]
["","Mounting plate","","","","","","","","","1"]
["","Remote control holder","","","","","","","","","1"]
["","Titanium apatite photocatalytic air purification filter","","","","","","","","","2"]
["Áramellátás","Megnevezés","","","","","","","","","V1"]
["","fázis","","","","","","","","","1~"]
["","Frekvencia","","","Hz","","","","","","50"]
["","Feszültség","","","V","","","","","","220-240"]
["Standard Accessories","Titánium apatit fotokatalitikus légtisztító szűrő keret nélkül","","","","","","","","","","2"]
["Notes","","","","","","","","","","","(4) - 240V"]