{"text_format":"2","workbook":"xls","n_sheets":1,"sheets":["Products"],"not_rendered":{"charts":0,"images":0,"macros":0,"external_links":1,"defined_names":0,"comments":0,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"run_cost":"one","rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900","formulas":"cached_only"}

{"sheet":"Products","index":0,"n_rows":48,"n_cols":11,"rows_kept":48,"cut":false,"hidden":false,"merged":[],"flags":["formulas_cached_only"]}
["PRODUCT NAME","FTXS-K / RXS-L"]
[]
[]
[]
[]
["","","","","FTXS20K2V1B / RXS20L2V1B","FTXS25K2V1B / RXS25L2V1B","FTXS35K2V1B / RXS35L2V1B","FTXS42K2V1B / RXS42L2V1B","FTXS42K3V1B / RXS42L2V1B","FTXS50K2V1B / RXS50L2V1B","FTXS50K3V1B / RXS50L2V1B"]
["Hűtési teljesítmény","Min.","","kW","1.3","1.3","1.4","1.7","","1.7"]
["","Max.","","kW","2.8","3.2","4.0","5.0","","5.3"]
["","Névl.","","kW","2.00","2.5","3.5","4.20","","5.00"]
["Csőcsatlakozások","Folyadék","Külső átm.","mm","6.35","6.35","6.35","6.35","","6.35"]
["","Gáz","Külső átm.","mm","9.5","9.5","9.5","9.5","","12.7"]
["","Ürítés","külső átm.","mm","18","18","18","18","","18"]
["Normál hatékonyság","Éves energiafogyasztás","","kWh","215","285","430","590","","705"]
["","EER","","","4.65","4.39","4.07","3.56","","3.55"]
["","COP","","","4.72","4.67","4.76","4.12","","4.00"]
["","Energiacímkézés irányelve","Hűtés","","A","A","A","A","","A"]
["","","Fűtés","","A","A","A","A","","A"]
["Fűtőkapacitás","Névl.","","kW","2.5","2.8","4.00","5.40","","5.80"]
["","Min.","","kW","1.3","1.3","1.4","1.7","","1.7"]
["","Max.","","kW","4.3","4.7","5.2","6.0","","6.5"]
["Notes","","","","(1) - EER/COP értékek az Eurovent 2012 szerint, csak EU-n kívüli országokra vonatkozóan","(1) - EER/COP értékek az Eurovent 2012 szerint, csak EU-n kívüli országokra vonatkozóan","(1) - EER/COP értékek az Eurovent 2012 szerint, csak EU-n kívüli országokra vonatkozóan","(1) - EER/COP értékek az Eurovent 2012 szerint, csak EU-n kívüli országokra vonatkozóan","(1) - EER/COP értékek az Eurovent 2012 szerint, csak EU-n kívüli országokra vonatkozóan","(1) - EER/COP értékek az Eurovent 2012 szerint, csak EU-n kívüli országokra vonatkozóan","(1) - EER/COP értékek az Eurovent 2012 szerint, csak EU-n kívüli országokra vonatkozóan"]
["","","","","(2) - 220V","(2) - 220V","(2) - 220V","(2) - 220V","(2) - Névleges hatékonyság: hűtés 35°/27° névleges terhelésen, fűtés 7°/20° névleges terhelésen","(2) - 220V","(2) - Névleges hatékonyság: hűtés 35°/27° névleges terhelésen, fűtés 7°/20° névleges terhelésen"]
["","","","","(3) - 230V","(3) - 230V","(3) - 230V","(3) - 230V","(3) - 220V","(3) - 230V","(3) - 220V"]
["","","","","(4) - 240V","(4) - 240V","(4) - 240V","(4) - 240V","(4) - 230V","(4) - 240V","(4) - 230V"]
["","","","","(5) - Névleges hatékonyság: hűtés 35°/27° névleges terhelésen, fűtés 7°/20° névleges terhelésen","(5) - Névleges hatékonyság: hűtés 35°/27° névleges terhelésen, fűtés 7°/20° névleges terhelésen","(5) - Névleges hatékonyság: hűtés 35°/27° névleges terhelésen, fűtés 7°/20° névleges terhelésen","(5) - Névleges hatékonyság: hűtés 35°/27° névleges terhelésen, fűtés 7°/20° névleges terhelésen","(5) - 240V","(5) - Névleges hatékonyság: hűtés 35°/27° névleges terhelésen, fűtés 7°/20° névleges terhelésen","(5) - 240V"]
["Outdoor unit","","","","","","","","RXS42L","","RXS50L"]
["Hűtési teljesítmény","Min.","","kW","","","","","1.7","","1.7"]
["","Névl.","","kW","","","","","4.20","","5.00"]
["","Max.","","kW","","","","","5.0","","5.3"]
["Fűtőkapacitás","Min.","","kW","","","","","1.7","","1.7"]
["","Névl.","","kW","","","","","5.40","","5.80"]
["","Max.","","kW","","","","","6.0","","6.5"]
["Névleges hatékonyság","EER","","","","","","","3.35","","3.32"]
["","COP","","","","","","","4.12","","4.00"]
["","Éves energiafogyasztás","","kWh","","","","","627","","753"]
["Normál hatékonyság","Energiacímkézés irányelve","Hűtés","","","","","","A","","A"]
["","","Fűtés","","","","","","A","","A"]
["Csőcsatlakozások","Ürítés","külső átm.","mm","","","","","18","","18"]
["","Gáz","Külső átm.","mm","","","","","12.7","","12.7"]
["","Folyadék","Külső átm.","mm","","","","","6.35","","6.35"]
["Felülethűtés","Energiatakarékossági osztály","","","","","","","A++","","A++"]
["","Kapacitás","Pdesign","kW","","","","","4.20","","5.00"]
["","SEER","","","","","","","6.80","","6.80"]
["","Éves energiafogyasztás","","kWh/a","","","","","216","","257"]
["Felülethűtés (Mérsékelt éghajlat)","Energiatakarékossági osztály","","","","","","","A+","","A+"]
["","Kapacitás","Pdesign","kW","","","","","4.00","","4.60"]
["","SCOP/A","","","","","","","4.20","","4.20"]
["","Éves energiafogyasztás","","kWh/a","","","","","1334","","1535"]