{"text_format":"2","workbook":"xls","n_sheets":1,"sheets":["Products"],"not_rendered":{"charts":0,"images":0,"macros":0,"external_links":1,"defined_names":0,"comments":0,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"run_cost":"one","rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900","formulas":"cached_only"}

{"sheet":"Products","index":0,"n_rows":25,"n_cols":10,"rows_kept":25,"cut":false,"hidden":false,"merged":[],"flags":["formulas_cached_only"]}
["PRODUCT NAME","FTXS-K / RXS-L3"]
[]
[]
[]
[]
["","","","","FTXS20K2V1B / RXS20L3V1B","FTXS20K3V1B / RXS20L3V1B","FTXS25K2V1B / RXS25L3V1B","FTXS25K3V1B / RXS25L3V1B","FTXS35K2V1B / RXS35L3V1B","FTXS35K3V1B / RXS35L3V1B"]
["Hűtési teljesítmény","Min.","","kW","","","","","","1.4"]
["","Max.","","kW","","","","","","4.0"]
["","Névl.","","kW","2.0","2.00 (2)","2.5","2.5 (2)","3.5","3.5 (2)"]
["Csőcsatlakozások","Folyadék","Külső átm.","mm","","6.35","","6.35","","6.35"]
["","Gáz","Külső átm.","mm","","9.5","","9.5","","9.5"]
["","Ürítés","külső átm.","mm","","18","","18","","18"]
["Normál hatékonyság","Éves energiafogyasztás","","kWh","228","228","297","297","450","450"]
["","EER","","","4.39","4.39 (1)","4.21","4.21 (1)","3.89","3.89 (1)"]
["","COP","","","4.72","4.72 (1)","4.67","4.67 (1)","4.76","4.76 (1)"]
["","Energiacímkézés irányelve","Hűtés","","A","A","A","A","A","A"]
["","","Fűtés","","A","A","A","A","A","A"]
["Fűtőkapacitás","Névl.","","kW","2.5","2.5 (2)","2.8","2.8 (2)","4.0","4.00 (2)"]
["","Min.","","kW","","1.3","","1.3","","1.4"]
["","Max.","","kW","","4.3","","4.7","","5.2"]
["Notes","","","","(1) - EER/COP értékek az Eurovent 2012 szerint, csak EU-n kívüli országokra vonatkozóan","(1) - EER/COP értékek az Eurovent 2012 szerint, csak EU-n kívüli országokra vonatkozóan","(1) - EER/COP értékek az Eurovent 2012 szerint, csak EU-n kívüli országokra vonatkozóan","(1) - EER/COP értékek az Eurovent 2012 szerint, csak EU-n kívüli országokra vonatkozóan","(1) - EER/COP értékek az Eurovent 2012 szerint, csak EU-n kívüli országokra vonatkozóan","(1) - EER/COP értékek az Eurovent 2012 szerint, csak EU-n kívüli országokra vonatkozóan"]
["","","","","(2) - Névleges hatékonyság: hűtés 35°/27° névleges terhelésen, fűtés 7°/20° névleges terhelésen","(2) - Névleges hatékonyság: hűtés 35°/27° névleges terhelésen, fűtés 7°/20° névleges terhelésen","(2) - Névleges hatékonyság: hűtés 35°/27° névleges terhelésen, fűtés 7°/20° névleges terhelésen","(2) - Névleges hatékonyság: hűtés 35°/27° névleges terhelésen, fűtés 7°/20° névleges terhelésen","(2) - Névleges hatékonyság: hűtés 35°/27° névleges terhelésen, fűtés 7°/20° névleges terhelésen","(2) - Névleges hatékonyság: hűtés 35°/27° névleges terhelésen, fűtés 7°/20° névleges terhelésen"]
["","","","","","(3) - 220V","","(3) - 220V","","(3) - 220V"]
["","","","","","(4) - 230V","","(4) - 230V","","(4) - 230V"]
["","","","","","(5) - 240V","","(5) - 240V","","(5) - 240V"]