{"text_format":"2","workbook":"xls","n_sheets":1,"sheets":["Products"],"not_rendered":{"charts":0,"images":0,"macros":0,"external_links":1,"defined_names":0,"comments":0,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"run_cost":"one","rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900","formulas":"cached_only"}

{"sheet":"Products","index":0,"n_rows":91,"n_cols":15,"rows_kept":91,"cut":false,"hidden":false,"merged":[],"flags":["formulas_cached_only"]}
["PRODUCT NAME","FTXS-K"]
[]
[]
[]
[]
["","","","","","FTXS20K2V1B","FTXS20K3V1B","FTXS25K2V1B","FTXS25K3V1B","FTXS35K2V1B","FTXS35K3V1B","FTXS42K2V1B","FTXS42K3V1B","FTXS50K2V1B","FTXS50K3V1B"]
["Hangnyomás szint","Fűtés","","Magas","dB(A)","40","","","","","","45"]
["","","","Csendes működés","dB(A)","19","","","","","","22"]
["","","","Alacsony","dB(A)","27","","","","","","33"]
["","Hűtés","","Csendes működés","dB(A)","19","","","","","","21"]
["","","","Alacsony","dB(A)","24","","","","","","33"]
["","","","Magas","dB(A)","40","","","","","","45"]
["","","","Névl.","dB(A)","34","","","","","","39"]
["","Hűtés","","Névl.","dB(A)","32","","","","","","39"]
["Standard Accessories","Telepítési utasítás","","","","1","","","","","","1"]
["","Használati utasítás","","","","1","","","","","","1"]
["","Vezeték nélküli távirányító","","","","1","","","","","","1"]
["","Elemek","","","","2","","","","","","2"]
["","Távirányító tartó","","","","1","","","","","","1"]
["","Szerelőlemez","","","","1","","","","","","1"]
["","Beltéri egység rögzítő csavarja","","","","2","","","","","","2"]
["","Titánium apatit fotokatalitikus légtisztító szűrő","","","","2","","","","","","2"]
["Vezérlőrendszerek","Infravörös távszabályzó","","","","ARC466A6","","","","","","ARC466A6"]
["Csőcsatlakozások","Folyadék","","Külső átm.","mm","6.35","","","","","","6.35"]
["","Gáz","","Külső átm.","mm","9.5","","","","","","9.5"]
["","Drain","","","","18","","","","","","18"]
["Elektromos bemenet","Hűtés","","Névl.","kW","0.04","","","","","","0.024 (2), 0.024 (3), 0.024 (4)"]
["","Fűtés","","Névl.","kW","0.04","","","","","","0.030 (2), 0.030 (3), 0.030 (4)"]
["Sound power level","Hűtés","","","dB(A)","58","","","","","","59"]
["","Fűtés","","","dB(A)","58","","","","","","59"]
["Méretek","Egység","","Szélesség","mm","780","","","","","","900"]
["","","","Mélység","mm","215","","","","","","215"]
["","","","Magasság","mm","289","","","","","","298"]
["Burkolat","Szín","","","","Fehér","","","","","","Fehér"]
["Tömeg","Egység","","","kg","8","","","","","","11"]
["Power supply","fázis","","","","1~","","","","","","1~"]
["","Frekvencia","","","Hz","50","","","","","","50"]
["","Megnevezés","","","","V1","","","","","","V1"]
["","Feszültség","","","V","220-240","","","","","","220-240"]
["Notes","","","","","(1) - 220V","(1) - 220V","(1) - 220V","(1) - 220V","(1) - 220V","(1) - 220V","(1) - Multi rendszerű kültéri egységhez való csatlakoztatás esetén lásd a csatlakoztatandó multi kültéri egység műszaki jellemzőit","(1) - 220V","(1) - 220V","(1) - 220V"]
["","","","","","(2) - 230V","(2) - 230V","(2) - 230V","(2) - 230V","(2) - 230V","(2) - 230V","(2) - 220V","(2) - 230V","(2) - 230V","(2) - 230V"]
["","","","","","(3) - 240V","(3) - 240V","(3) - 240V","(3) - 240V","(3) - 240V","(3) - 240V","(3) - 230V","(3) - 240V","(3) - 240V","(3) - 240V"]
["Elektromos bemenet","Hűtés","","Névl.","kW","","0.040, 0.040, 0.040","0.04","0.040 (3) (1) (2), 0.040 (3) (1) (2), 0.040 (3) (1) (2)","0.026 (3) (4) (2), 0.026 (3) (4) (2), 0.026 (3) (4) (2)","0.026 (1) (3) (2), 0.026 (1) (3) (2), 0.026 (1) (3) (2)","","0.024, 0.024, 0.024","0.026 (4) (2) (3), 0.026 (4) (2) (3), 0.026 (4) (2) (3)","0.026 (1) (2) (3), 0.026 (1) (2) (3), 0.026 (1) (2) (3)"]
["","Fűtés","","Névl.","kW","","0.040, 0.040, 0.040","0.04","0.040 (2) (3) (1), 0.040 (2) (3) (1), 0.040 (2) (3) (1)","0.028 (2) (4) (3), 0.028 (2) (4) (3), 0.028 (2) (4) (3)","0.028 (1) (3) (2), 0.028 (1) (3) (2), 0.028 (1) (3) (2)","","0.030, 0.030, 0.030","0.032 (2) (4) (3), 0.032 (2) (4) (3), 0.032 (2) (4) (3)","0.032 (2) (1) (3), 0.032 (2) (1) (3), 0.032 (2) (1) (3)"]
["Burkolat","Szín","","","","","Fehér","Fehér","Fehér","Fehér","Fehér","","Fehér","Fehér","Fehér"]
["Méretek","Egység","","Magasság","mm","","215","289","215","298","215","","215","298","215"]
["","","","Szélesség","mm","","780","780","780","900","900","","900","900","900"]
["","","","Mélység","mm","","289","215","289","215","298","","298","215","298"]
["Tömeg","Egység","","","kg","","8.00","8","8.00","11","11.0","","11.0","11","11.0"]
["Ventilátor","Légáramlási arány","Hűtés","Magas","m³/perc","","8.8","9.1","9.1","11.2","11.2","","11.2","11.9","11.9"]
["","Légszállítási sebesség","Hűtés","Közepes","m³/perc","","6.7","7.0","7.0","","8.5","","9.1","","9.6"]
["","","","Alacsony","m³/perc","","4.7","5.0","5.0","5.8","5.8","","7.0","7.4","7.4"]
["","","","Csendes működés","m³/perc","","3.9","3.9","3.9","4.1","4.1","","4.1","4.5","4.5"]
["","","Fűtés","Magas","m³/perc","","9.5","10.0","10.0","12.1","12.1","","12.4","13.3","13.3"]
["","Légszállítási sebesség","Fűtés","Közepes","m³/perc","","7.8","8.0","8.0","","9.3","","10.0","","10.8"]
["","","Fűtés","Alacsony","m³/perc","","6.0","6.0","6.0","6.5","6.5","","7.8","8.4","8.4"]
["","","","Csendes működés","m³/perc","","4.3","4.3","4.3","4.2","4.2","","5.2","5.5","5.5"]
["Hangteljesítményszint","Hűtés","","","dB(A)","","58","58","58","59","59","","59","60","60"]
["","Fűtés","","","dB(A)","","58","58","58","59","59","","59","60","60"]
["Hangnyomás szint","Hűtés","","Magas","dB(A)","","40","41","41","45","45","","45","46","46"]
["Hangnyomásszint","Hűtés","","Közepes","dB(A)","","32","33","33","","37","","39","","40"]
["Hangnyomás szint","Hűtés","","Alacsony","dB(A)","","24","25","25","29","29","","33","34","34"]
["","","","Csendes működés","dB(A)","","19","19","19","19","19","","21","23","23"]
["","Fűtés","","Magas","dB(A)","","40","41","41","45","45","","45","47","47"]
["Hangnyomásszint","Fűtés","","Közepes","dB(A)","","34","34","34","","39","","39","","40"]
["Hangnyomás szint","Fűtés","","Alacsony","dB(A)","","27","27","27","29","29","","33","34","34"]
["","","","Csendes működés","dB(A)","","19","19","19","19","19","","22","24","24"]
["Csőcsatlakozások","Folyadék","","Külső átm.","mm","","6.35","6.35","6.35","6.35","6.35","","6.35","6.35","6.35"]
["","Gáz","","Külső átm.","mm","","9.50","9.5","9.50","9.5","9.50","","9.50","12.7","12.7"]
["","Ürítés","","","","","18","18","18","18","18","","18","18","18"]
["Vezérlőrendszerek","Infravörös távszabályzó","","","","","ARC466A6","","","","","","ARC466A9"]
["Standard Accessories","Installation manual","","","","","1","1","1","1","1","","1","1","1"]
["","Wireless remote control","","","","","1","1","1","1","1","","1","1","1"]
["","AAA dry-cell batteries","","","","","2","","2","","2","","2","","2"]
["","Operation manual","","","","","1","1","1","1","1","","1","1","1"]
["","Titanium apatite deodorizing filter","","","","","2","","2","","2","","2","","2"]
["","Indoor unit fixing screws","","","","","2","2","2","2","2","","2","2","2"]
["","Mounting plate","","","","","1","1","1","1","1","","1","1","1"]
["","Remote control holder","","","","","1","1","1","1","1","","1","1","1"]
["Áramellátás","Megnevezés","","","","","V1","V1","V1","V1","V1","","V1","V1","V1"]
["","fázis","","","","","1~","1~","1~","1~","1~","","1~","1~","1~"]
["","Frekvencia","","","Hz","","50","50","50","50","50","","50","50","50"]
["","Feszültség","","","V","","220-240","220-240","220-240","220-240","220-240","","220-240","220-240","220-240"]
["Ventilátor","Légáramlási arány","Hűtés","Névl.","m³/perc","","","9.1","","11.2","","","","11.9"]
["Hangnyomás szint","Hűtés","","Névl.","dB(A)","","","33","","37","","","","40"]
["Ventilátor","Légáramlási arány","Fűtés","Névl.","m³/perc","","","8.0","","9.3","","","","10.8"]
["Hangnyomás szint","Fűtés","","Névl.","dB(A)","","","34","","39","","","","40"]
["Vezérlőrendszerek","Infravörös távszabályzó","","","","","","ARC466A6","ARC466A6","ARC466A6","ARC466A9","","","ARC466A6","ARC466A9"]
["Standard Accessories","Batteries","","","","","","2","","2","","","","2"]
["","Titanium apatite photocatalytic air purification filter","","","","","","2","","2","","","","2"]
["Notes","","","","","","","","","","","(4) - 240V"]