{"text_format":"2","workbook":"xls","n_sheets":1,"sheets":["Products"],"not_rendered":{"charts":0,"images":0,"macros":0,"external_links":1,"defined_names":0,"comments":0,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"run_cost":"one","rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900","formulas":"cached_only"}

{"sheet":"Products","index":0,"n_rows":42,"n_cols":5,"rows_kept":42,"cut":false,"hidden":false,"merged":[],"flags":["formulas_cached_only"]}
["PRODUCT NAME","FTXTA-AW"]
[]
[]
[]
[]
["","","","","FTXTA30A2V1BW"]
["Hangnyomás szint","Fűtés","Magas","dB(A)","41"]
["","","Közepes","dB(A)","31"]
["","","Csendes működés","dB(A)","19"]
["","","Alacsony","dB(A)","24"]
["","Hűtés","Medium","dB(A)","32"]
["","","Csendes működés","dB(A)","20"]
["","","Alacsony","dB(A)","25"]
["","","Magas","dB(A)","43"]
["Standard Accessories","Telepítési utasítás","","","1"]
["","Használati utasítás","","","1"]
["","Légszűrő","","","2"]
["","Infravörös távirányító","","","1"]
["","A távirányító rögzítésére szolgáló lap","","","1"]
["","Csavarzsák","","","1"]
["","Csavarfedél","","","2"]
["","AAA szárazelemek","","","2"]
["","Általános biztonsági óvintézkedések","","","1"]
["Refrigerant","GWP","","","675.0"]
["Control systems","Wired remote control","","","BRC073A4"]
["","Infrared remote control","","","ARC466A59"]
["Csőcsatlakozások","Folyadék","Külső átm.","pp","6.35"]
["","Gáz","Külső átm.","pp","9.50"]
["","Ürítés","","","18"]
["Elektromos bemenet","Hűtés","Névl.","kW","0.023"]
["","Fűtés","Névl.","kW","0.022"]
["Sound power level","Hűtés","","dB(A)","60"]
["","Fűtés","","dB(A)","60"]
["Méretek","Egység","Szélesség","pp","798"]
["","","Mélység","pp","189"]
["","","Magasság","pp","295"]
["Burkolat","Szín","","","Fehér"]
["Tömeg","Egység","","kg","11.5"]
["Power supply","fázis","","","1~"]
["","Frekvencia","","Hz","50"]
["","Megnevezés","","","V1"]
["","Feszültség","","V","220-240"]