{"text_format":"2","workbook":"xls","n_sheets":1,"sheets":["Products"],"not_rendered":{"charts":0,"images":0,"macros":0,"external_links":1,"defined_names":0,"comments":0,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"run_cost":"one","rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900","formulas":"cached_only"}

{"sheet":"Products","index":0,"n_rows":53,"n_cols":6,"rows_kept":53,"cut":false,"hidden":false,"merged":[],"flags":["formulas_cached_only"]}
["PRODUCT NAME","FTXTA-BW"]
[]
[]
[]
[]
["","","","","","FTXTA30B2V1BW"]
["Hangnyomás szint","Fűtés","","Magas","dB(A)","41"]
["","","","Közepes","dB(A)","31"]
["","","","Csendes működés","dB(A)","19"]
["","","","Alacsony","dB(A)","24"]
["","Hűtés","","Medium","dB(A)","32"]
["","","","Csendes működés","dB(A)","20"]
["","","","Alacsony","dB(A)","25"]
["","","","Magas","dB(A)","43"]
["Standard Accessories","Telepítési utasítás","","","","1"]
["","Használati utasítás","","","","1"]
["","Légszűrő","","","","2"]
["","Infravörös távirányító","","","","1"]
["","A távirányító rögzítésére szolgáló lap","","","","1"]
["","Csavarzsák","","","","1"]
["","Csavarfedél","","","","2"]
["","AAA szárazelemek","","","","2"]
["","Általános biztonsági óvintézkedések","","","","1"]
["Refrigerant","GWP","","","","675.0"]
["Vezérlőrendszerek","Vezetékes távszabályzó","","","","BRC073A4"]
["","Infravörös távszabályzó","","","","ARC466A59"]
["Csőcsatlakozások","Folyadék","","Külső átm.","mm","6.35"]
["","Gáz","","Külső átm.","mm","9.50"]
["","Drain","","","","18"]
["Elektromos bemenet","Hűtés","","Névl.","kW","0.023"]
["","Fűtés","","Névl.","kW","0.022"]
["Hangteljesítmény szintje","Hűtés","","","dB(A)","60"]
["","Fűtés","","","dB(A)","60"]
["Méretek","Berendezés","","Szélesség","mm","798"]
["","","","Mélység","mm","189"]
["","","","Magasság","mm","295"]
["Burkolat","Colour","","","","Fehér"]
["Súly","Berendezés","","","kg","11.5"]
["Fan","Légszállítási sebesség","Fűtés","Magas","m³/perc","11.5"]
["","","","Alacsony","m³/perc","6.0"]
["","","","Közepes","m³/perc","8.0"]
["","","","Csendes működés","m³/perc","5.1"]
["","","Hűtés","Alacsony","m³/perc","5.7"]
["","","","Közepes","m³/perc","8.3"]
["","","","Magas","m³/perc","11.9"]
["","","","Csendes működés","m³/perc","4.6"]
["Power supply","Phase","","","","1~"]
["","Frekvencia","","","Hz","50"]
["","Name","","","","V1"]
["","Feszültség","","","V","220-240"]
["Notes","","","","","(1) - Hűtés: belső hőm. 27°CDB, 19,0°CWB; kültéri hőm. 35°C száraz hőm., 24°C nedves hőm.; egyenlő csőhossz: 5m"]
["","","","","","(2) - Fűtés: belső hőm. 20°C száraz hőm.; külső hőm. 7 °C száraz hőm., 6 °C nedves hőm.; a hűtőközeg egyenértékű csővezetékhossza: 5m"]
["","","","","","(3) - Az elektromos adatokat lásd külön rajzokon"]