{"text_format":"2","workbook":"xls","n_sheets":1,"sheets":["Products"],"not_rendered":{"charts":0,"images":0,"macros":0,"external_links":1,"defined_names":0,"comments":0,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"run_cost":"one","rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900","formulas":"cached_only"}

{"sheet":"Products","index":0,"n_rows":21,"n_cols":5,"rows_kept":21,"cut":false,"hidden":false,"merged":[],"flags":["formulas_cached_only"]}
["PRODUCT NAME","FTXTA-CB / RXTA-B"]
[]
[]
[]
[]
["","","","","FTXTA30C2V1BB / RXTA30B2V1B"]
["Hűtési teljesítmény","Min.","","kW","0.70"]
["","Névl.","","kW","3.00"]
["","Max.","","kW","4.50"]
["Fűtőkapacitás","Min.","","kW","0.80"]
["","Névl.","","kW","3.20"]
["","Max.","","kW","6.90"]
["Normál hatékonyság","Éves energiafogyasztás","","kWh","357"]
["","COP","","","4.87"]
["","EER","","","4.20"]
["","Energiacímkézés irányelve","Hűtés","","A"]
["","","Fűtés","","A"]
["Notes","","","","(1) - A névleges hűtési teljesítmények a következő feltételekre vonatkoznak: belső hőmérséklet: 27 °C száraz hőm., 19 °C nedves hőm., kültéri hőm.: 35°C száraz, a hűtőközeg egyenértékű csővezetékhossza: 5m, szintkülönbség: 0m."]
["","","","","(2) - A névleges fűtési kapacitás alapja: belső hőmérséklet: 20°C száraz, kültéri hőmérséklet: 7 °C száraz, 6 °C párás, a hűtőközeg egyenértékű csővezetékhossza: 5m, szintkülönbség: 0m."]
["","","","","(3) - Az elektromos adatokat lásd külön rajzokon"]
["","","","","(4) - Az üzemi tartomány tekintetében ld. az önálló ábrát"]