{"text_format":"2","workbook":"xls","n_sheets":1,"sheets":["Products"],"not_rendered":{"charts":0,"images":0,"macros":0,"external_links":1,"defined_names":0,"comments":0,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"run_cost":"one","rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900","formulas":"cached_only"}

{"sheet":"Products","index":0,"n_rows":50,"n_cols":6,"rows_kept":50,"cut":false,"hidden":false,"merged":[],"flags":["formulas_cached_only"]}
["PRODUCT NAME","FTXTA-CB"]
[]
[]
[]
[]
["","","","","","FTXTA30C2V1BB"]
["Elektromos bemenet","Hűtés","","Névl.","kW","0.023"]
["","Fűtés","","Névl.","kW","0.022"]
["Burkolat","Szín","","","","Fekete"]
["Méretek","Egység","","Magasság","pp","295"]
["","","","Szélesség","pp","798"]
["","","","Mélység","pp","189"]
["Tömeg","Egység","","","kg","12"]
["Ventilátor","Légáramlási arány","Hűtés","Magas","m³/perc","13.1"]
["","Légszállítási sebesség","Hűtés","Közepes","m³/perc","9"]
["","","","Alacsony","m³/perc","6"]
["","","","Csendes működés","m³/perc","4.9"]
["","","Fűtés","Magas","m³/perc","12.3"]
["","Légszállítási sebesség","Fűtés","Közepes","m³/perc","8.2"]
["","","Fűtés","Alacsony","m³/perc","5.8"]
["","","","Csendes működés","m³/perc","5"]
["Hangteljesítményszint","Hűtés","","","dBA","60"]
["","Fűtés","","","dBA","60"]
["Hangnyomás szint","Hűtés","","Magas","dBA","43"]
["Hangnyomásszint","Hűtés","","Közepes","dBA","32"]
["Hangnyomás szint","Hűtés","","Alacsony","dBA","25"]
["","","","Csendes működés","dBA","20"]
["","Fűtés","","Magas","dBA","41"]
["Hangnyomásszint","Fűtés","","Közepes","dBA","31"]
["Hangnyomás szint","Fűtés","","Alacsony","dBA","24"]
["","","","Csendes működés","dBA","19"]
["Hűtőközeg","GWP","","","","675"]
["Csőcsatlakozások","Folyadék","","Külső átm.","pp","6.35"]
["","Gáz","","Külső átm.","pp","9.5"]
["","Ürítés","","","","18"]
["Vezérlőrendszerek","Infrared remote control","","","","ARC466A84"]
["Vezérlőrendszerek","Vezetékes távszabályzó","","","","BRC073A4"]
["Standard Accessories","Installation manual","","","","1"]
["","Wireless remote control","","","","1"]
["","Screw cover","","","","2"]
["","AAA dry-cell batteries","","","","2"]
["","General safety precautions","","","","1"]
["","Operation manual","","","","1"]
["","Titanium apatite deodorizing filter","","","","1"]
["","Silver particle filter","","","","1"]
["","Remote control holder","","","","1"]
["","Screw bag","","","","1"]
["Áramellátás","fázis","","","","1~"]
["","Frekvencia","","","Hz","50"]
["","Feszültség","","","V","220-240"]