{"text_format":"2","workbook":"xls","n_sheets":1,"sheets":["Products"],"not_rendered":{"charts":0,"images":0,"macros":0,"external_links":1,"defined_names":0,"comments":0,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"run_cost":"one","rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900","formulas":"cached_only"}

{"sheet":"Products","index":0,"n_rows":40,"n_cols":7,"rows_kept":40,"cut":false,"hidden":false,"merged":[],"flags":["formulas_cached_only"]}
["PRODUCT NAME","FTXTM-M"]
[]
[]
[]
[]
["","","","","","FTXTM30M2V1B","FTXTM40M2V1B"]
["Elektromos bemenet","Hűtés","","Névl.","kW","0.032","0.037"]
["","Fűtés","","Névl.","kW","0.037","0.04"]
["Burkolat","Szín","","","","Fehér","Fehér"]
["Méretek","Egység","","Magasság","mm","294","300"]
["","","","Szélesség","mm","811","1040"]
["","","","Mélység","mm","272","295"]
["Tömeg","Egység","","","kg","10","14.5"]
["Ventilátor","Légáramlási arány","Hűtés","Magas","m³/perc","11.7","15.5"]
["","Légszállítási sebesség","Hűtés","Közepes","m³/perc","8","9.2"]
["","","","Alacsony","m³/perc","6.3","5.7"]
["","","","Csendes működés","m³/perc","5.2","4.6"]
["","","Fűtés","Magas","m³/perc","12.2","17.7"]
["","Légszállítási sebesség","Fűtés","Közepes","m³/perc","7.5","11"]
["","","Fűtés","Alacsony","m³/perc","5.1","7.5"]
["","","","Csendes működés","m³/perc","4.1","6.3"]
["Hangteljesítményszint","Hűtés","","","dB(A)","60","60"]
["","Fűtés","","","dB(A)","61","61"]
["Hangnyomás szint","Hűtés","","Magas","dB(A)","45","46"]
["Hangnyomásszint","Hűtés","","Közepes","dB(A)","33","32"]
["Hangnyomás szint","Hűtés","","Alacsony","dB(A)","25","24"]
["","","","Csendes működés","dB(A)","21","20"]
["","Fűtés","","Magas","dB(A)","45","46"]
["Hangnyomásszint","Fűtés","","Közepes","dB(A)","31","31"]
["Hangnyomás szint","Fűtés","","Alacsony","dB(A)","22","22"]
["","","","Csendes működés","dB(A)","19","19"]
["Csőcsatlakozások","Folyadék","","Külső átm.","mm","6.35","6.35"]
["","Gáz","","Külső átm.","mm","9.5","9.5"]
["","Ürítés","","","","16 (a csatlakozótömlő belső átmérője)","16 (a csatlakozótömlő belső átmérője)"]
["Vezérlőrendszerek","Infravörös távszabályzó","","","","ARC466A55","ARC466A55"]
["","Vezetékes távszabályzó","","","","BRC944B2, BRC073A1","BRC944B2, BRC073A1"]
["Áramellátás","Megnevezés","","","","V1","V1"]
["","fázis","","","","1~","1~"]
["","Frekvencia","","","Hz","50","50"]
["","Feszültség","","","V","220-240","220-240"]