{"text_format":"2","workbook":"xls","n_sheets":1,"sheets":["Products"],"not_rendered":{"charts":0,"images":0,"macros":0,"external_links":1,"defined_names":0,"comments":0,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"run_cost":"one","rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900","formulas":"cached_only"}

{"sheet":"Products","index":0,"n_rows":94,"n_cols":7,"rows_kept":94,"cut":false,"hidden":false,"merged":[],"flags":["formulas_cached_only"]}
["PRODUCT NAME","FTXTM-R"]
[]
[]
[]
[]
["","","","","","FTXTM30R2V1B","FTXTM40R2V1B"]
["Hangnyomás szint","Fűtés","","Magas","dB(A)","45.0"]
["","","","Közepes","dB(A)","31.0"]
["","","","Csendes működés","dB(A)","19.0"]
["","","","Alacsony","dB(A)","22.0"]
["","Hűtés","","Medium","dB(A)","33.0"]
["","","","Csendes működés","dB(A)","21.0"]
["","","","Alacsony","dB(A)","25.0"]
["","","","Magas","dB(A)","45.0"]
["Standard Accessories","Telepítési utasítás","","","","1"]
["","Használati utasítás","","","","1"]
["","Vezeték nélküli távirányító","","","","1"]
["","AAA szárazelemek","","","","2"]
["","Távirányító tartó","","","","1"]
["","Szerelőlemez","","","","1"]
["","Beltéri egység rögzítő csavarja","","","","2"]
["","Ezüst részecskeszűrő","","","","1"]
["Control systems","Wired remote control","","","","BRC073A1"]
["","Infrared remote control","","","","ARC466A75"]
["Csőcsatlakozások","Folyadék","","Külső átm.","pp","6.35"]
["","Gáz","","Külső átm.","pp","9.50"]
["","Ürítés","","","","18"]
["Elektromos bemenet","Hűtés","","Névl.","kW","0.035"]
["","Fűtés","","Névl.","kW","0.039"]
["Sound power level","Hűtés","","","dB(A)","60.0"]
["","Fűtés","","","dB(A)","61.0"]
["Méretek","Egység","","Szélesség","pp","778"]
["","","","Mélység","pp","272"]
["","","","Magasság","pp","295"]
["Burkolat","Szín","","","","Fehér"]
["Tömeg","Egység","","","kg","10.0"]
["Ventilátor","Légszállítási sebesség","Fűtés","Magas","m³/perc","12.5"]
["","","","Alacsony","m³/perc","4.9"]
["","","","Medium","m³/perc","7.5"]
["","","","Csendes működés","m³/perc","4.0"]
["","","Hűtés","Alacsony","m³/perc","5.3"]
["","","","Medium","m³/perc","7.8"]
["","","","Magas","m³/perc","12.2"]
["","","","Csendes működés","m³/perc","4.1"]
["Power supply","fázis","","","","1~"]
["","Frekvencia","","","Hz","50"]
["","Megnevezés","","","","V1"]
["","Feszültség","","","V","220-240"]
["Notes","","","","","(1) - Hűtés: belső hőm. 27°CDB, 19,0°CWB; kültéri hőm. 35°C száraz hőm., 24°C nedves hőm.; egyenlő csőhossz: 5m"]
["","","","","","(2) - Fűtés: belső hőm. 20°C száraz hőm.; külső hőm. 7 °C száraz hőm., 6 °C nedves hőm.; a hűtőközeg egyenértékű csővezetékhossza: 5m"]
["","","","","","(3) - Az elektromos adatokat lásd külön rajzokon"]
["Elektromos bemenet","Hűtés","","Névl.","kW","","0.053"]
["","Fűtés","","Névl.","kW","","0.06"]
["Burkolat","Szín","","","","","Fehér"]
["Méretek","Egység","","Magasság","pp","","299"]
["","","","Szélesség","pp","","998"]
["","","","Mélység","pp","","292"]
["Tömeg","Egység","","","kg","","14.5"]
["Ventilátor","Légáramlási arány","Hűtés","Magas","m³/perc","","15.4"]
["","Légszállítási sebesség","Hűtés","Közepes","m³/perc","","9.5"]
["","","","Alacsony","m³/perc","","5.8"]
["","","","Csendes működés","m³/perc","","4.6"]
["","","Fűtés","Magas","m³/perc","","17.5"]
["","Légszállítási sebesség","Fűtés","Közepes","m³/perc","","10.5"]
["","","Fűtés","Alacsony","m³/perc","","7.1"]
["","","","Csendes működés","m³/perc","","5.9"]
["Hangteljesítményszint","Hűtés","","","dB(A)","","60"]
["","Fűtés","","","dB(A)","","61"]
["Hangnyomás szint","Hűtés","","Magas","dB(A)","","46"]
["Hangnyomásszint","Hűtés","","Közepes","dB(A)","","32"]
["Hangnyomás szint","Hűtés","","Alacsony","dB(A)","","24"]
["","","","Csendes működés","dB(A)","","20"]
["","Fűtés","","Magas","dB(A)","","46"]
["Hangnyomásszint","Fűtés","","Közepes","dB(A)","","31"]
["Hangnyomás szint","Fűtés","","Alacsony","dB(A)","","22"]
["","","","Csendes működés","dB(A)","","19"]
["Csőcsatlakozások","Folyadék","","Külső átm.","pp","","6.35"]
["","Gáz","","Külső átm.","pp","","9.5"]
["","Ürítés","","","","","18"]
["Control systems","Infrared remote control","","","","","ARC466A75"]
["Vezérlőrendszerek","Vezetékes távszabályzó","","","","","BRC073A1"]
["Standard Accessories","Installation manual","","","","","1"]
["","Wireless remote control","","","","","1"]
["","AAA dry-cell batteries","","","","","2"]
["","Operation manual","","","","","1"]
["","Titanium apatite deodorizing filter","","","","","1"]
["","Silver particle filter","","","","","1"]
["","Indoor unit fixing screws","","","","","2"]
["","Mounting plate","","","","","1"]
["","Remote control holder","","","","","1"]
["Áramellátás","Megnevezés","","","","","V1"]
["","fázis","","","","","1~"]
["","Frekvencia","","","Hz","","50"]
["","Feszültség","","","V","","220-240"]