{"text_format":"2","workbook":"xls","n_sheets":1,"sheets":["Products"],"not_rendered":{"charts":0,"images":0,"macros":0,"external_links":1,"defined_names":0,"comments":0,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"run_cost":"one","rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900","formulas":"cached_only"}

{"sheet":"Products","index":0,"n_rows":47,"n_cols":7,"rows_kept":47,"cut":false,"hidden":false,"merged":[],"flags":["formulas_cached_only"]}
["PRODUCT NAME","FTXTM-S"]
[]
[]
[]
[]
["","","","","","FTXTM30S2V1B","FTXTM40S2V1B"]
["Elektromos bemenet","Hűtés","","Névl.","kW","0.035","0.053"]
["","Fűtés","","Névl.","kW","0.039","0.06"]
["Burkolat","Szín","","","","Fehér","Fehér"]
["Méretek","Egység","","Magasság","pp","295","299"]
["","","","Szélesség","pp","778","998"]
["","","","Mélység","pp","272","292"]
["Tömeg","Egység","","","kg","10","15"]
["Ventilátor","Légáramlási arány","Hűtés","Magas","m³/perc","11.5","15.1"]
["","Légszállítási sebesség","Hűtés","Közepes","m³/perc","7.5","9.2"]
["","","","Alacsony","m³/perc","5.2","5.6"]
["","","","Csendes működés","m³/perc","4.2","4.8"]
["","","Fűtés","Magas","m³/perc","11.6","17"]
["","Légszállítási sebesség","Fűtés","Közepes","m³/perc","7.3","10"]
["","","Fűtés","Alacsony","m³/perc","4.7","6"]
["","","","Csendes működés","m³/perc","4","5.1"]
["Hangteljesítményszint","Hűtés","","","dB(A)","60","60"]
["","Fűtés","","","dB(A)","60","60"]
["Hangnyomás szint","Hűtés","","Magas","dB(A)","45","46"]
["Hangnyomásszint","Hűtés","","Közepes","dB(A)","33","32"]
["Hangnyomás szint","Hűtés","","Alacsony","dB(A)","25","24"]
["","","","Csendes működés","dB(A)","21","20"]
["","Fűtés","","Magas","dB(A)","45","46"]
["Hangnyomásszint","Fűtés","","Közepes","dB(A)","31","31"]
["Hangnyomás szint","Fűtés","","Alacsony","dB(A)","22","22"]
["","","","Csendes működés","dB(A)","19","19"]
["Hűtőközeg","GWP","","","","675","675"]
["Csőcsatlakozások","Folyadék","","Külső átm.","pp","6.35","6.35"]
["","Gáz","","Külső átm.","pp","9.5","9.5"]
["","Ürítés","","","","18","18"]
["Vezérlőrendszerek","Infravörös távszabályzó","","","","ARC466A83","ARC466A83"]
["","Vezetékes távszabályzó","","","","BRC073A1","BRC073A1"]
["Standard Accessories","Installation manual","","","","1","1"]
["","Wireless remote control","","","","1","1"]
["","AAA dry-cell batteries","","","","2","2"]
["","General safety precautions","","","","1","1"]
["","Silver particle filter","","","","1","1"]
["","Remote control holder","","","","1","1"]
["","Screw bag","","","","1","1"]
["Áramellátás","fázis","","","","1~","1~"]
["","Frekvencia","","","Hz","50","50"]
["","Feszültség","","","V","220-240","220-240"]