{"text_format":"2","workbook":"xls","n_sheets":1,"sheets":["Products"],"not_rendered":{"charts":0,"images":0,"macros":0,"external_links":1,"defined_names":0,"comments":0,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"run_cost":"one","rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900","formulas":"cached_only"}

{"sheet":"Products","index":0,"n_rows":55,"n_cols":7,"rows_kept":55,"cut":false,"hidden":false,"merged":[],"flags":["formulas_cached_only"]}
["PRODUCT NAME","FTXTP-A"]
[]
[]
[]
[]
["","","","","","FTXTP25A5V1B","FTXTP35A5V1B"]
["Elektromos bemenet","Hűtés","","Névl.","kW","0.032","0.032"]
["","Fűtés","","Névl.","kW","0.032","0.032"]
["Burkolat","Szín","","","","Fehér","Fehér"]
["Méretek","Egység","","Magasság","mm","286","286"]
["","","","Szélesség","mm","770","770"]
["","","","Mélység","mm","225","225"]
["Tömeg","Egység","","","kg","9","9"]
["Ventilátor","Légáramlási arány","Hűtés","Magas","m³/perc","11","11"]
["","Légszállítási sebesség","Hűtés","Közepes","m³/perc","7.9","7.9"]
["","","","Alacsony","m³/perc","5","5"]
["","","","Csendes működés","m³/perc","3.7","3.7"]
["","","Fűtés","Magas","m³/perc","10.5","10.5"]
["","Légszállítási sebesség","Fűtés","Közepes","m³/perc","9","9"]
["","","Fűtés","Alacsony","m³/perc","5.5","5.5"]
["","","","Csendes működés","m³/perc","4.4","4.4"]
["Hangteljesítményszint","Hűtés","","","dB(A)","58","58"]
["","Fűtés","","","dB(A)","58","58"]
["Hangnyomás szint","Hűtés","","Magas","dB(A)","43","43"]
["Hangnyomásszint","Hűtés","","Közepes","dB(A)","35","35"]
["Hangnyomás szint","Hűtés","","Alacsony","dB(A)","26","26"]
["","","","Csendes működés","dB(A)","21","21"]
["","Fűtés","","Magas","dB(A)","43","43"]
["Hangnyomásszint","Fűtés","","Közepes","dB(A)","35","35"]
["Hangnyomás szint","Fűtés","","Alacsony","dB(A)","26","26"]
["","","","Csendes működés","dB(A)","21","21"]
["Hűtőközeg","GWP","","","","675","675"]
["Csőcsatlakozások","Folyadék","","Külső átm.","mm","6.35","6.35"]
["","Gáz","","Külső átm.","mm","9.5","9.5"]
["","Ürítés","","","","18","18"]
["Control systems","Infrared remote control","","","","ARC480A78","ARC480A78"]
["Standard Accessories","FTXTP25A5V1B","","","","1"]
["","Installation manual","","","","1","1"]
["","Wireless remote control","","","","1","1"]
["","Screw cover","","","","2","2"]
["","AAA dry-cell batteries","","","","2","2"]
["","General safety precautions","","","","1","1"]
["","Operation manual","","","","1","1"]
["","Titanium apatite deodorizing filter","","","","1","1"]
["","Silver particle filter","","","","1","1"]
["","Remote control holder","","","","1","1"]
["","Screw bag","","","","1","1"]
["Áramellátás","Megnevezés","","","","V1","V1"]
["","fázis","","","","1~","1~"]
["","Frekvencia","","","Hz","50","50"]
["","Feszültség","","","V","220-240","220-240"]
["Notes","","","","","(1) - Hűtés: belső hőm. 27 °C száraz, 19 °C nedves hőm.; kültéri hőm. 35°C száraz hőm., 24°C nedves hőm.; egyenlő csőhossz: 5m","(1) - Hűtés: belső hőm. 27 °C száraz, 19 °C nedves hőm.; kültéri hőm. 35°C száraz hőm., 24°C nedves hőm.; egyenlő csőhossz: 5m"]
["","","","","","(2) - Fűtés: belső hőm. 20°C száraz hőm.; külső hőm. 7 °C száraz hőm., 6 °C nedves hőm.; a hűtőközeg egyenértékű csővezetékhossza: 5m","(2) - Fűtés: belső hőm. 20°C száraz hőm.; külső hőm. 7 °C száraz hőm., 6 °C nedves hőm.; a hűtőközeg egyenértékű csővezetékhossza: 5m"]
["","","","","","(3) - Az elektromos adatokat lásd külön rajzokon","(3) - Az elektromos adatokat lásd külön rajzokon"]
["Standard Accessories","FTXTP35A5V1B","","","","","1"]