{"text_format":"2","workbook":"xls","n_sheets":1,"sheets":["Products"],"not_rendered":{"charts":0,"images":0,"macros":0,"external_links":1,"defined_names":0,"comments":0,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"run_cost":"one","rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900","formulas":"cached_only"}

{"sheet":"Products","index":0,"n_rows":83,"n_cols":7,"rows_kept":83,"cut":false,"hidden":false,"merged":[],"flags":["formulas_cached_only"]}
["PRODUCT NAME","FTXTP-K"]
[]
[]
[]
[]
["","","","","","FTXTP25K3V1B","FTXTP35K3V1B"]
["Hangnyomás szint","Fűtés","","Magas","dB(A)","43"]
["","","","Közepes","dB(A)","35"]
["","","","Csendes működés","dB(A)","21"]
["","","","Alacsony","dB(A)","26"]
["","Hűtés","","Közepes","dB(A)","35"]
["","","","Csendes működés","dB(A)","21"]
["","","","Alacsony","dB(A)","26"]
["","","","Magas","dB(A)","43"]
["Standard Accessories","Telepítési utasítás","","","","1"]
["","Használati utasítás","","","","1"]
["","Vezeték nélküli távirányító","","","","1"]
["","AAA szárazelemek","","","","2"]
["","Távirányító tartó","","","","1"]
["","Szerelőlemez","","","","1"]
["","Titán apatit szagtalanító szűrő","","","","2"]
["","Beltéri egység rögzítő csavarja","","","","2"]
["Control systems","Wired remote control","","","","BRC944B2, BRC073A1"]
["","Infrared remote control","","","","ARC480A11"]
["Csőcsatlakozások","Folyadék","","Külső átm.","mm","6.35"]
["","Gáz","","Külső átm.","mm","9.50"]
["","Ürítés","","","","16 (a csatlakozótömlő belső átmérője)"]
["Elektromos bemenet","Hűtés","","Névl.","kW","0.030"]
["","Fűtés","","Névl.","kW","0.035"]
["Sound power level","Hűtés","","","dB(A)","58"]
["","Fűtés","","","dB(A)","58"]
["Méretek","Egység","","Szélesség","mm","770"]
["","","","Mélység","mm","225"]
["","","","Magasság","mm","285"]
["Burkolat","Szín","","","","Fehér"]
["Tömeg","Egység","","","kg","9.0"]
["Power supply","fázis","","","","1~"]
["","Frekvencia","","","Hz","50"]
["","Megnevezés","","","","V1"]
["","Feszültség","","","V","220-240"]
["Notes","","","","","(1) - Az elektromos adatokat lásd külön rajzokon"]
["Elektromos bemenet","Hűtés","","Névl.","kW","","0.03"]
["","Fűtés","","Névl.","kW","","0.035"]
["Burkolat","Szín","","","","","Fehér"]
["Méretek","Egység","","Magasság","mm","","285"]
["","","","Szélesség","mm","","770"]
["","","","Mélység","mm","","225"]
["Tömeg","Egység","","","kg","","9"]
["Ventilátor","Légáramlási arány","Hűtés","Magas","m³/perc","","11.4"]
["","Légszállítási sebesség","Hűtés","Közepes","m³/perc","","8.2"]
["","","","Alacsony","m³/perc","","5.4"]
["","","","Csendes működés","m³/perc","","4.3"]
["","","Fűtés","Magas","m³/perc","","10.8"]
["","Légszállítási sebesség","Fűtés","Közepes","m³/perc","","7.8"]
["","","Fűtés","Alacsony","m³/perc","","5.8"]
["","","","Csendes működés","m³/perc","","4.9"]
["Hangteljesítményszint","Hűtés","","","dB(A)","","58"]
["","Fűtés","","","dB(A)","","58"]
["Hangnyomás szint","Hűtés","","Magas","dB(A)","","43"]
["Hangnyomásszint","Hűtés","","Közepes","dB(A)","","35"]
["Hangnyomás szint","Hűtés","","Alacsony","dB(A)","","26"]
["","","","Csendes működés","dB(A)","","21"]
["","Fűtés","","Magas","dB(A)","","43"]
["Hangnyomásszint","Fűtés","","Közepes","dB(A)","","35"]
["Hangnyomás szint","Fűtés","","Alacsony","dB(A)","","26"]
["","","","Csendes működés","dB(A)","","21"]
["Csőcsatlakozások","Folyadék","","Külső átm.","mm","","6.35"]
["","Gáz","","Külső átm.","mm","","9.5"]
["","Ürítés","","","","","16 (a csatlakozótömlő belső átmérője)"]
["Control systems","Infrared remote control","","","","","ARC480A11"]
["Vezérlőrendszerek","Vezetékes távszabályzó","","","","","BRC944B2, BRC073A1"]
["Standard Accessories","Installation manual","","","","","1"]
["","Wireless remote control","","","","","1"]
["","AAA dry-cell batteries","","","","","2"]
["","Operation manual","","","","","1"]
["","Titanium apatite deodorizing filter","","","","","2"]
["","Indoor unit fixing screws","","","","","2"]
["","Mounting plate","","","","","1"]
["","Remote control holder","","","","","1"]
["Áramellátás","Megnevezés","","","","","V1"]
["","fázis","","","","","1~"]
["","Frekvencia","","","Hz","","50"]
["","Feszültség","","","V","","220-240"]