{"text_format":"2","workbook":"xls","n_sheets":1,"sheets":["Products"],"not_rendered":{"charts":0,"images":0,"macros":0,"external_links":1,"defined_names":0,"comments":0,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"run_cost":"one","rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900","formulas":"cached_only"}

{"sheet":"Products","index":0,"n_rows":23,"n_cols":10,"rows_kept":23,"cut":false,"hidden":false,"merged":[],"flags":["formulas_cached_only"]}
["PRODUCT NAME","FTXZ-N / RXZ-N"]
[]
[]
[]
[]
["","","","","FTXZ25NV1B / RXZ25NV1B","FTXZ25NV1B / RXZ25NV1B9","FTXZ35NV1B / RXZ35NV1B","FTXZ35NV1B / RXZ35NV1B9","FTXZ50NV1B / RXZ50NV1B","FTXZ50NV1B / RXZ50NV1B9"]
["Hűtési teljesítmény","Min.","","kW","0.6","0.6","0.6","0.6","0.6","0.6"]
["","Max.","","kW","3.9","3.9","5.3","5.3","5.8","5.8"]
["","Névl.","","kW","2.5","2.5","3.5","3.5","5.0","5.0"]
["Csőcsatlakozások","Folyadék","Külső átm.","mm","6.35","6.35","6.35","6.35","6.35","6.35"]
["","Gáz","külső átm.","mm","9.5","9.5","9.5","9.5","9.5","9.5"]
["Normál hatékonyság","Éves energiafogyasztás","","kWh","205","205","330","330","550","550"]
["","EER","","","6.10","6.10","5.30","5.30","4.55","4.55"]
["","COP","","","5.80","5.80","5.00","5.00","4.47","4.47"]
["","Energiacímkézés irányelve","Hűtés","","A","A","A","A","A","A"]
["","","Fűtés","","A","A","A","A","A","A"]
["Fűtőkapacitás","Névl.","","kW","3.6","3.6","5.0","5.0","6.3","6.3"]
["","Min.","","kW","0.6","0.6","0.6","0.6","0.6","0.6"]
["","Max.","","kW","7.5","7.5","9.0","9.0","9.4","9.4"]
["Notes","","","","(1) - Névleges hatékonyság: hűtés 35°/27° névleges terhelésen, fűtés 7°/20° névleges terhelésen","(1) - Névleges hatékonyság: hűtés 35°/27° névleges terhelésen, fűtés 7°/20° névleges terhelésen","(1) - Névleges hatékonyság: hűtés 35°/27° névleges terhelésen, fűtés 7°/20° névleges terhelésen","(1) - Névleges hatékonyság: hűtés 35°/27° névleges terhelésen, fűtés 7°/20° névleges terhelésen","(1) - Névleges hatékonyság: hűtés 35°/27° névleges terhelésen, fűtés 7°/20° névleges terhelésen","(1) - Névleges hatékonyság: hűtés 35°/27° névleges terhelésen, fűtés 7°/20° névleges terhelésen"]
["","","","","(2) - 220V","(2) - 220V","(2) - 220V","(2) - 220V","(2) - 220V","(2) - 220V"]
["","","","","(3) - 230V","(3) - 230V","(3) - 230V","(3) - 230V","(3) - 230V","(3) - 230V"]
["","","","","(4) - 240V","(4) - 240V","(4) - 240V","(4) - 240V","(4) - 240V","(4) - 240V"]