{"text_format":"2","workbook":"xls","n_sheets":1,"sheets":["Products"],"not_rendered":{"charts":0,"images":0,"macros":0,"external_links":1,"defined_names":0,"comments":0,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"run_cost":"one","rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900","formulas":"cached_only"}

{"sheet":"Products","index":0,"n_rows":49,"n_cols":8,"rows_kept":49,"cut":false,"hidden":false,"merged":[],"flags":["formulas_cached_only"]}
["PRODUCT NAME","FTXZ-N"]
[]
[]
[]
[]
["","","","","","FTXZ25NV1B","FTXZ35NV1B","FTXZ50NV1B"]
["Hangnyomás szint","Fűtés","","Magas","dB(A)","39","42","44"]
["","","","Csendes működés","dB(A)","19","19","24"]
["","","","Alacsony","dB(A)","28","29","31"]
["","Hűtés","","Csendes működés","dB(A)","19","19","23"]
["","","","Alacsony","dB(A)","26","27","30"]
["","","","Magas","dB(A)","38","42","47"]
["","","","Névl.","dB(A)","35","36","38"]
["","Hűtés","","Névl.","dB(A)","33","35","38"]
["Standard Accessories","Fotokatalitikus légtisztító és szagtalanító szűrő","","","","1","1","1"]
["","Vezeték nélküli távirányító","","","","1","1","1"]
["","Szárazelemek","","","","2","2","2"]
["","Távirányító tartó","","","","1","1","1"]
["","Beltéri egység rögzítő csavarja","","","","3","3","3"]
["","Szerelőlemez","","","","1","1","1"]
["Control systems","Infrared remote control","","","","ARC477A1","ARC477A1","ARC477A1"]
["Csőcsatlakozások","Folyadék","","Külső átm.","mm","6.35","6.35","6.35"]
["","Gáz","","Külső átm.","mm","9.5","9.5","9.5"]
["Elektromos bemenet","Hűtés","","Névl.","kW","0.030","0.030","0.030"]
["","Fűtés","","Névl.","kW","0.030","0.030","0.030"]
["Sound power level","Hűtés","","","dB(A)","54","57","60"]
["","Fűtés","","","dB(A)","56","57","59"]
["Méretek","Egység","","Szélesség","mm","798","798","798"]
["","","","Mélység","mm","372","372","372"]
["","","","Magasság","mm","295","295","295"]
["Burkolat","Colour","","","","Fehér","Fehér","Fehér"]
["Tömeg","Egység","","","kg","15","15","15"]
["Ventilátor","Légáramlási arány","Fűtés","Magas","m³/perc","11.7","13.3","14.4"]
["","","","Alacsony","m³/perc","6.7","6.9","7.7"]
["","","","Csendes működés","m³/perc","4.8","4.8","5.9"]
["","","Hűtés","Alacsony","m³/perc","5.3","5.6","6.6"]
["","","","Magas","m³/perc","10.7","12.1","15.0"]
["","","","Csendes működés","m³/perc","4.0","4.0","4.6"]
["","","","Névl.","m³/perc","8.6","9.2","10.7"]
["","","Hűtés","Névl.","m³/perc","7.5","8.4","9.2"]
["Power supply","fázis","","","","1~","1~","1~"]
["","Megnevezés","","","","V1","V1","V1"]
["","Frekvencia","","","Hz","50","50","50"]
["","Feszültség","","","V","220-240","220-240","220-240"]
["Notes","","","","","(1) - 220V","(1) - 220V","(1) - 220V"]
["","","","","","(2) - 230V","(2) - 230V","(2) - 230V"]
["","","","","","(3) - 240V","(3) - 240V","(3) - 240V"]
["","","","","","(4) - A hőcserélő eleje","(4) - A hőcserélő eleje","(4) - A hőcserélő eleje"]
["","","","","","(5) - A hőcserélő hátulja","(5) - A hőcserélő hátulja","(5) - A hőcserélő hátulja"]