{"text_format":"2","workbook":"xls","n_sheets":1,"sheets":["Products"],"not_rendered":{"charts":0,"images":0,"macros":0,"external_links":1,"defined_names":0,"comments":0,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"run_cost":"one","rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900","formulas":"cached_only"}

{"sheet":"Products","index":0,"n_rows":26,"n_cols":16,"rows_kept":26,"cut":false,"hidden":false,"merged":[],"flags":["formulas_cached_only"]}
["PRODUCT NAME","FUA-A / RZQG-L(8)Y1"]
[]
[]
[]
[]
["","","","","FUA100AVEB / RZQG100L8Y1B","FUA100AVEB9 / RZQG100L8Y1B","FUA125AVEB / RZQG125L8Y1B","FUA125AVEB9 / RZQG125L8Y1B","FUA71AVEB / FUA71AVEB / RZQG100L8Y1B","FUA71AVEB / FUA71AVEB / RZQG125L8Y1B","FUA71AVEB9 / FUA71AVEB9 / RZQG100L8Y1B","FUA71AVEB9 / FUA71AVEB9 / RZQG125L8Y1B","FUA100AVEB / RZQG71L8Y1B","FUA100AVEB9 / RZQG71L8Y1B","FUA71AVEB / RZQG71L8Y1B","FUA71AVEB9 / RZQG71L8Y1B"]
["Energiatakarékossági besorolás","","","","A+++ ~ D","A+++ ~ D","A+++ ~ D","A+++ ~ D","A+++ ~ D","A+++ ~ D","A+++ ~ D","A+++ ~ D"]
["Hűtési teljesítmény","Névl.","","kW","","","","","","","","","6.80","6.80","6.80","6.80"]
["Felülethűtés","SEER","","","","","","","","","","","6.42","6.42","6.42","6.42"]
["","Éves energiafogyasztás","","kWh/a","","","","","","","","","371","371","371","371"]
["","Kapacitás","Pdesign","kW","","","","","","","","","6.80","6.80","6.80","6.80"]
["","Energiatakarékossági osztály","","","","","","","","","","","A++","A++","A++","A++"]
["Felületfűtés (Mérsékelt éghajlat)","Kapacitás","Pdesign","kW","","","","","","","","","7.60","7.60","7.60","7.60"]
["","SCOP/A","","","","","","","","","","","4.20","4.20","4.20","4.20"]
["","Energiatakarékossági osztály","","","","","","","","","","","A+","A+","A+","A+"]
["","Éves energiafogyasztás","","kWh/a","","","","","","","","","2,534","2,534","2,534","2,534"]
["Normál hatékonyság","EER","","","","","","","","","","","4.07","4.07","4.07","4.07"]
["Notes","","","","","","","","","","","","(1) - Az üzemi tartomány tekintetében ld. az önálló ábrát","(1) - Az üzemi tartomány tekintetében ld. az önálló ábrát","(1) - A névleges hűtési teljesítmények a következő feltételekre vonatkoznak: belső hőmérséklet: 27 °C száraz hőm., 19 °C nedves hőm., kültéri hőmérséklet: 35°C száraz, a hűtőközeg egyenértékű csővezetékhossza: 5m, szintkülönbség: 0m.","(1) - A névleges hűtési teljesítmények a következő feltételekre vonatkoznak: belső hőmérséklet: 27 °C száraz hőm., 19 °C nedves hőm., kültéri hőmérséklet: 35°C száraz, a hűtőközeg egyenértékű csővezetékhossza: 5m, szintkülönbség: 0m."]
["","","","","","","","","","","","","(2) - Az elektromos adatokat lásd külön rajzokon","(2) - Az elektromos adatokat lásd külön rajzokon","(2) - A névleges fűtési kapacitás alapja: belső hőmérséklet: 20°C száraz, kültéri hőmérséklet: 7 °C száraz, 6 °C párás, a hűtőközeg egyenértékű csővezetékhossza: 5m, szintkülönbség: 0m.","(2) - A névleges fűtési kapacitás alapja: belső hőmérséklet: 20°C száraz, kültéri hőmérséklet: 7 °C száraz, 6 °C párás, a hűtőközeg egyenértékű csővezetékhossza: 5m, szintkülönbség: 0m."]
["Normál hatékonyság","Éves energiafogyasztás","","kWh","","","","","","","","","","","835","835"]
["","COP","","","","","","","","","","","","","4.08","4.08"]
["","Energiacímkézés irányelve","Hűtés","","","","","","","","","","","","A","A"]
["","","Fűtés","","","","","","","","","","","","A","A"]
["Fűtőkapacitás","Névl.","","kW","","","","","","","","","","","7.50","7.50"]
["Notes","","","","","","","","","","","","","","(3) - Az üzemi tartomány tekintetében ld. az önálló ábrát","(3) - Az üzemi tartomány tekintetében ld. az önálló ábrát"]
["","","","","","","","","","","","","","","(4) - Az elektromos adatokat lásd külön rajzokon","(4) - Az elektromos adatokat lásd külön rajzokon"]