{"text_format":"2","workbook":"xls","n_sheets":1,"sheets":["Products"],"not_rendered":{"charts":0,"images":0,"macros":0,"external_links":1,"defined_names":0,"comments":0,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"run_cost":"one","rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900","formulas":"cached_only"}

{"sheet":"Products","index":0,"n_rows":82,"n_cols":11,"rows_kept":82,"cut":false,"hidden":false,"merged":[],"flags":["formulas_cached_only"]}
["PRODUCT NAME","FUA-A"]
[]
[]
[]
[]
["","","","","","FUA71AVEB9","FUA100AVEB9","FUA125AVEB9","FUA71AVEB (Archived)","FUA100AVEB (Archived)","FUA125AVEB (Archived)"]
["Hangnyomás szint","Fűtés","","Magas","dB(A)","","","","41","46","47"]
["","","","Közepes","dB(A)","","","","38","42","43"]
["","","","Alacsony","dB(A)","","","","35","39","40"]
["","Hűtés","","Közepes","dB(A)","","","","38","42","43"]
["","","","Alacsony","dB(A)","","","","35","39","40"]
["","","","Magas","dB(A)","","","","41","46","47"]
["Standard Accessories","Használati utasítás","","","","","","","1","1","1"]
["","Telepítési utasítás","","","","","","","1","1","1"]
["","Leeresztő tömlő","","","","","","","1","1","1"]
["","Hőszigetelő cső","","","","","","","3","3","3"]
["","Szalagkötések","","","","","","","10","10","10"]
["","Tömlősáv","","","","","","","1","1","1"]
["","Tömítő anyag","","","","","","","4","4","4"]
["","Alátétrögzítő lemez","","","","","","","1","1","1"]
["","Leeresztő illesztés","","","","","","","1","1","1"]
["","Nem szőtt anyag","","","","","","","1","1","1"]
["","Alátét","","","","","","","8","8","8"]
["","A leeresztő tömlő rögzítő csavarja","","","","","","","5","5","5"]
["Vezérlőrendszerek","Vezetékes távszabályzó","","","","","","","BRC1H52W/S/K, BRC1E53A, BRC1E53B, BRC1E53C, BRC1D52","BRC1H52W/S/K, BRC1E53A, BRC1E53B, BRC1E53C, BRC1D52","BRC1H52W/S/K, BRC1E53A, BRC1E53B, BRC1E53C, BRC1D52"]
["Hűtési teljesítmény","Összes teljesítmény","","Névl.","kW","","","","","","12.1"]
["Csőcsatlakozások","Folyadék","","Külső átm.","mm","","","","9.52","9.52","9.52"]
["","Gáz","","Külső átm.","mm","","","","15.9","15.9","15.9"]
["","Ürítés","","","","","","","VP25 (OD Ø32.0)","VP25 (OD Ø32.0)","VP25 (OD Ø32.0)"]
["Sound power level","Hűtés","","","dB(A)","","","","59","64","65"]
["","Fűtés","","","dB(A)","","","","59","64"]
["Méretek","Egység","","Szélesség","mm","","","","950","950","950"]
["","","","Mélység","mm","","","","950","950","950"]
["","","","Magasság","mm","","","","198","198","198"]
["Burkolat","Anyag","","","","","","","Műgyanta","Műgyanta","Műgyanta"]
["","Szín","","","","","","","Friss fehér","Friss fehér","Friss fehér"]
["Tömeg","Egység","","","kg","","","","25.0","26.0","26"]
["Ventilátor","Légáramlási arány","Fűtés","Magas","m³/perc","","","","23.0","31.0","32.5"]
["","","","Medium","m³/perc","","","","19.5","25.5","26.5"]
["","","","Alacsony","m³/perc","","","","16.0","20.0","20.5"]
["","","Hűtés","Alacsony","m³/perc","","","","16.0","20.0","20.5"]
["","","","Medium","m³/perc","","","","19.5","25.5","26.5"]
["","","","Magas","m³/perc","","","","23.0","31.0","32.5"]
["Leeresztési emelési magasság","mm","","","","","","","600","600","600"]
["Fűtőkapacitás","Összes teljesítmény","","Névl.","kW","","","","","","13.5"]
["Burkolat","Szín","","","","Friss fehér","Friss fehér","Friss fehér"]
["","Anyag","","","","Műgyanta","Műgyanta","Műgyanta"]
["Méretek","Egység","","Magasság","mm","198","198","198"]
["","","","Szélesség","mm","950","950","950"]
["","","","Mélység","mm","950","950","950"]
["Tömeg","Egység","","","kg","25.0","26.0","26.0"]
["Ventilátor","Légáramlási arány","Hűtés","Magas","m³/perc","23.0","31.0","32.5"]
["","Légszállítási sebesség","Hűtés","Közepes","m³/perc","19.5","25.5","26.5"]
["","","","Alacsony","m³/perc","16.0","20.0","20.5"]
["","","Fűtés","Magas","m³/perc","23.0","31.0","32.5"]
["","Légszállítási sebesség","Fűtés","Közepes","m³/perc","19.5","25.5","26.5"]
["","","Fűtés","Alacsony","m³/perc","16.0","20.0","20.5"]
["Hangteljesítményszint","Hűtés","","","dB(A)","59","64","65"]
["Hangnyomás szint","Hűtés","","Magas","dB(A)","41","46","47"]
["Hangnyomásszint","Hűtés","","Közepes","dB(A)","38","42","43"]
["Hangnyomás szint","Hűtés","","Alacsony","dB(A)","35","39","40"]
["","Fűtés","","Magas","dB(A)","41","46","47"]
["Hangnyomásszint","Fűtés","","Közepes","dB(A)","38","42","43"]
["Hangnyomás szint","Fűtés","","Alacsony","dB(A)","35","39","40"]
["Csőcsatlakozások","Folyadék","","Külső átm.","mm","9.52","9.52","9.52"]
["","Gáz","","Külső átm.","mm","15.9","15.9","15.9"]
["","Ürítés","","","","VP25 (OD Ø32.0)","VP25 (OD Ø32.0)","VP25 (OD Ø32.0)"]
["Leeresztési emelési magasság","mm","","","","600","600","600"]
["Standard Accessories","Installation manual","","","","1","1","1"]
["","Thermal insulation tube","","","","3","3","3"]
["","Non woven fabric","","","","1","1","1"]
["","Drain joint","","","","1","1","1"]
["","Hose band","","","","1","1","1"]
["","Operation manual","","","","1","1","1"]
["","Drain hose","","","","1","1","1"]
["","Fixing screw for drain hose","","","","5","5","5"]
["","Sealing material","","","","4","4","4"]
["","Tie-wraps","","","","10","10","10"]
["","Washer","","","","8","8","8"]
["","Washer fixing plate","","","","1","1","1"]
["Hűtési teljesítmény","Hűtési összteljesítmény","","Névl.","kW","","","12.10"]
["Fűtési teljesítmény","Összes teljesítmény","","Névl.","kW","","","13.5"]