{"text_format":"2","workbook":"xls","n_sheets":1,"sheets":["Products"],"not_rendered":{"charts":0,"images":0,"macros":0,"external_links":1,"defined_names":0,"comments":0,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"run_cost":"one","rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900","formulas":"cached_only"}

{"sheet":"Products","index":0,"n_rows":46,"n_cols":9,"rows_kept":46,"cut":false,"hidden":false,"merged":[],"flags":["formulas_cached_only"]}
["PRODUCT NAME","FVA-A"]
[]
[]
[]
[]
["","","","","","FVA71AMVEB","FVA100AMVEB","FVA125AMVEB","FVA140AMVEB"]
["Hűtési teljesítmény","Hűtési összteljesítmény","","Névl.","kW","","","12.10","13.40"]
["Fűtési teljesítmény","Összes teljesítmény","","Névl.","kW","","","13.5","15.5"]
["Burkolat","Szín","","","","Friss fehér","Friss fehér","Friss fehér","Friss fehér"]
["Méretek","Egység","","Magasság","mm","1850","1850","1850","1850"]
["","","","Szélesség","mm","600","600","600","600"]
["","","","Mélység","mm","270","350","350","350"]
["Tömeg","Egység","","","kg","42","50","50","50"]
["Ventilátor","Légáramlási arány","Hűtés","Magas","m³/perc","18","28","28","30"]
["","Légszállítási sebesség","Hűtés","Közepes","m³/perc","16","25","26","28"]
["","","","Alacsony","m³/perc","14","22","24","26"]
["","","Fűtés","Magas","m³/perc","18","28","28","30"]
["","Légszállítási sebesség","Fűtés","Közepes","m³/perc","16","25","26","28"]
["","","Fűtés","Alacsony","m³/perc","14","22","24","26"]
["Hangteljesítményszint","Hűtés","","","dB(A)","55","62","63","65"]
["Hangnyomás szint","Hűtés","","Magas","dB(A)","43","50","51","53"]
["Hangnyomásszint","Hűtés","","Közepes","dB(A)","41","47","48","51"]
["Hangnyomás szint","Hűtés","","Alacsony","dB(A)","38","44","46","48"]
["","Fűtés","","Magas","dB(A)","43","50","51","53"]
["Hangnyomásszint","Fűtés","","Közepes","dB(A)","38","44","46","48"]
["Hangnyomás szint","Fűtés","","Névl.","dB(A)","41","47","48","51"]
["Csőcsatlakozások","Folyadék","","Külső átm.","mm","9.52","9.52","9.52","9.52"]
["","Gáz","","Külső átm.","mm","15.9","15.9","15.9","15.9"]
["","Ürítés","","","","I.D. 20/O.D. 26","I.D. 20/O.D. 26","I.D. 20/O.D. 26","I.D. 20/O.D. 26"]
["Vezérlőrendszerek","Vezetékes távszabályzó","","","","BRC1H52W/S/K, BRC1E53A, BRC1E53B, BRC1E53C, BRC1D52","BRC1H52W/S/K, BRC1E53A, BRC1E53B, BRC1E53C, BRC1D52","BRC1H52W/S/K, BRC1E53A, BRC1E53B, BRC1E53C, BRC1D52","BRC1H52W/S/K, BRC1E53A, BRC1E53B, BRC1E53C, BRC1D52"]
["Standard Accessories","Installation manual","","","","1","1","1","1"]
["","Hole protection rubber","","","","2","2","2","2"]
["","Cover","","","","1","1","1","1"]
["","Dew proof material","","","","1","1","1","1"]
["","Remote control wiring","","","","1","1","1","1"]
["","Bracket for installation","","","","1","1","1","1"]
["","Operation manual","","","","1","1","1","1"]
["","Bush","","","","1","1","1","1"]
["","Installation pattern","","","","1","1","1","1"]
["","Insulation for fitting for gas pipe","","","","1","1","1","1"]
["","Insulation for fitting for liquid pipe","","","","1","1","1","1"]
["","Screws","","","","5","5","5","5"]
["","Tie-wraps","","","","5","5","5","5"]
["Áramellátás","fázis","","","","1~","1~","1~","1~"]
["","Frekvencia","","","Hz","50/60","50/60","50/60","50/60"]
["","Feszültség","","","V","220-240/220","220-240/220","220-240/220","220-240/220"]