{"text_format":"2","workbook":"xls","n_sheets":1,"sheets":["Products"],"not_rendered":{"charts":0,"images":0,"macros":0,"external_links":1,"defined_names":0,"comments":0,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"run_cost":"one","rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900","formulas":"cached_only"}

{"sheet":"Products","index":0,"n_rows":29,"n_cols":7,"rows_kept":29,"cut":false,"hidden":false,"merged":[],"flags":["formulas_cached_only"]}
["PRODUCT NAME","FVXG-K / RXG-L"]
[]
[]
[]
[]
["","","","","FVXG25K2V1B / RXG25L2V1B","FVXG35K2V1B / RXG35L2V1B","FVXG50K2V1B / RXG50L2V1B"]
["Hűtési teljesítmény","Min.","","kW","1.3","1.4","1.7"]
["","Névl.","","kW","2.5","3.5","5.0"]
["","Max.","","kW","3.0","3.8","5.6"]
["Fűtőkapacitás","Min.","","kW","1.3","1.4","1.7"]
["","Névl.","","kW","3.4","4.5","5.8"]
["","Max.","","kW","4.5","5.0","8.1"]
["Névleges hatékonyság","EER","","","4.63","3.72","3.31"]
["","COP","","","4.42","3.75","3.69"]
["","Éves energiafogyasztás","","kWh","270","470","755"]
["Normál hatékonyság","Energiacímkézés irányelve","Hűtés","","A","A","A"]
["","","Fűtés","","A","A","A"]
["Csőcsatlakozások","Gáz","Külső átm.","mm","9.5","9.5","12.7"]
["","Folyadék","Külső átm.","mm","6.35","6.35","6.35"]
["Felülethűtés","Energiatakarékossági osztály","","","A++","A++","A"]
["","Kapacitás","Pdesign","kW","2.50","3.50","5.00"]
["","SEER","","","6.53","6.48","5.41"]
["","Éves energiafogyasztás","","kWh/a","134","189","324"]
["Felülethűtés (Mérsékelt éghajlat)","Energiatakarékossági osztály","","","A++","A+","A+"]
["","Kapacitás","Pdesign","kW","2.80","3.10","4.60"]
["","SCOP/A","","","4.65","4.00","4.18"]
["","Éves energiafogyasztás","","kWh/a","842","1087","1543"]
["Notes","","","","(1) - Hűtés: belső hőm. 27 °C száraz, 19 °C nedves hőmérséklet; külső hőm. 35 °C száraz, 24 °C párás hőmérséklet","(1) - Hűtés: belső hőm. 27 °C száraz, 19 °C nedves hőmérséklet; külső hőm. 35 °C száraz, 24 °C párás hőmérséklet","(1) - Hűtés: belső hőm. 27 °C száraz, 19 °C nedves hőmérséklet; külső hőm. 35 °C száraz, 24 °C párás hőmérséklet"]
["","","","","(2) - Fűtés: belső hőm. 20°C száraz hőm.; külső hőm. 7 °C száraz / 6 °C párás hőmérséklet","(2) - Fűtés: belső hőm. 20°C száraz hőm.; külső hőm. 7 °C száraz / 6 °C párás hőmérséklet","(2) - Fűtés: belső hőm. 20°C száraz hőm.; külső hőm. 7 °C száraz / 6 °C párás hőmérséklet"]