{"text_format":"2","workbook":"xls","n_sheets":1,"sheets":["Products"],"not_rendered":{"charts":0,"images":0,"macros":0,"external_links":1,"defined_names":0,"comments":0,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"run_cost":"one","rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900","formulas":"cached_only"}

{"sheet":"Products","index":0,"n_rows":51,"n_cols":8,"rows_kept":51,"cut":false,"hidden":false,"merged":[],"flags":["formulas_cached_only"]}
["PRODUCT NAME","FVXG-K"]
[]
[]
[]
[]
["","","","","","FVXG25K2V1B","FVXG35K2V1B","FVXG50K2V1B"]
["Elektromos bemenet","Hűtés","","Névl.","kW","0.019, 0.019, 0.019","0.021 (1) (2) (3), 0.021 (1) (2) (3), 0.021 (1) (2) (3)","0.032, 0.032, 0.032"]
["","Fűtés","","Névl.","kW","0.022, 0.022, 0.022","0.024 (2) (1) (3), 0.024 (2) (1) (3), 0.024 (2) (1) (3)","0.035, 0.035, 0.035"]
["Burkolat","Szín","","","","Friss fehér (6.5Y 9.5/0.5)","Friss fehér (6.5Y 9.5/0.5)","Friss fehér (6.5Y 9.5/0.5)"]
["Méretek","Egység","","Magasság","pp","600","600","600"]
["","","","Szélesség","pp","950","950","950"]
["","","","Mélység","pp","215","215","215"]
["Tömeg","Egység","","","kg","22.0","22.0","22.0"]
["Ventilátor","Légáramlási arány","Hűtés","Magas","m³/perc","8.9","9.1","10.6"]
["","Légszállítási sebesség","Hűtés","Közepes","m³/perc","7.0","7.2","8.9"]
["","","","Alacsony","m³/perc","5.3","5.3","7.3"]
["","","","Csendes működés","m³/perc","4.5","4.5","6.0"]
["","","Fűtés","Magas","m³/perc","9.9","10.2","12.2"]
["","Légszállítási sebesség","Fűtés","Közepes","m³/perc","7.8","8.0","10.0"]
["","","Fűtés","Alacsony","m³/perc","5.7","5.8","7.8"]
["","","","Csendes működés","m³/perc","4.7","5.0","6.8"]
["Hangteljesítményszint","Hűtés","","","dB(A)","54","55","56"]
["","Fűtés","","","dB(A)","55","56","58"]
["Hangnyomás szint","Hűtés","","Magas","dB(A)","38","39","44"]
["Hangnyomásszint","Hűtés","","Közepes","dB(A)","32","33","40"]
["Hangnyomás szint","Hűtés","","Alacsony","dB(A)","26","27","36"]
["","","","Csendes működés","dB(A)","23","24","32"]
["","Fűtés","","Magas","dB(A)","39","40","46"]
["Hangnyomásszint","Fűtés","","Közepes","dB(A)","32","33","40"]
["Hangnyomás szint","Fűtés","","Alacsony","dB(A)","26","27","34"]
["","","","Csendes működés","dB(A)","22","23","30"]
["Csőcsatlakozások","Folyadék","","Külső átm.","pp","6.35","6.35","6.35"]
["","Gáz","","Külső átm.","pp","9.50","9.50","12.7"]
["","Ürítés","","","","18","18","18"]
["Vezérlőrendszerek","Infravörös távszabályzó","","","","ARC466A2","ARC466A2","ARC466A2"]
["Standard Accessories","Installation manual","","","","1","1","1"]
["","Wireless remote control","","","","1","1","1"]
["","Installation plate","","","","1","1","1"]
["","Thermal insulation (thermal insulation tube)","","","","1","1","1"]
["","AAA dry-cell batteries","","","","2","2","2"]
["","Operation manual","","","","1","1","1"]
["","Titanium apatite deodorizing filter","","","","2","2","2"]
["","Drain hose","","","","1","1","1"]
["","Remote control holder","","","","1","1","1"]
["Áramellátás","Megnevezés","","","","V1","V1","V1"]
["","fázis","","","","1~","1~","1~"]
["","Frekvencia","","","Hz","50","50","50"]
["","Feszültség","","","V","220-240","220-240","220-240"]
["Notes","","","","","(1) - 220V","(1) - 220V","(1) - 220V"]
["","","","","","(2) - 230V","(2) - 230V","(2) - 230V"]
["","","","","","(3) - 240V","(3) - 240V","(3) - 240V"]