{"text_format":"2","workbook":"xls","n_sheets":1,"sheets":["Products"],"not_rendered":{"charts":0,"images":0,"macros":0,"external_links":1,"defined_names":0,"comments":0,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"run_cost":"one","rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900","formulas":"cached_only"}

{"sheet":"Products","index":0,"n_rows":48,"n_cols":8,"rows_kept":48,"cut":false,"hidden":false,"merged":[],"flags":["formulas_cached_only"]}
["PRODUCT NAME","FVXM-A9"]
[]
[]
[]
[]
["","","","","","FVXM25A3V1B9","FVXM35A3V1B9","FVXM50A3V1B9"]
["Elektromos bemenet","Hűtés","","Névl.","kW","0.02","0.02","0.03"]
["","Fűtés","","Névl.","kW","0.02","0.03","0.03"]
["Burkolat","Szín","","","","Fehér","Fehér","Fehér"]
["Méretek","Egység","","Magasság","mm","600","600","600"]
["","","","Szélesség","mm","750","750","750"]
["","","","Mélység","mm","238","238","238"]
["Tömeg","Egység","","","kg","17","17","17"]
["Ventilátor","Légáramlási arány","Hűtés","Magas","m³/perc","8.7","9.2","11.6"]
["","Légszállítási sebesség","Hűtés","Közepes","m³/perc","7","7","9"]
["","","","Alacsony","m³/perc","4.9","4.9","6.6"]
["","","","Csendes működés","m³/perc","4.1","4.1","5.4"]
["","","Fűtés","Magas","m³/perc","9.2","9.8","12.8"]
["","Légszállítási sebesség","Fűtés","Közepes","m³/perc","7.2","7.2","10"]
["","","Fűtés","Alacsony","m³/perc","5.6","5.6","8.4"]
["","","","Csendes működés","m³/perc","4.1","4.1","5.9"]
["Hangteljesítményszint","Hűtés","","","dB(A)","52","53","61"]
["","Fűtés","","","dB(A)","52","53","62"]
["Hangnyomás szint","Hűtés","","Magas","dB(A)","38","39","44"]
["Hangnyomásszint","Hűtés","","Közepes","dB(A)","32","32","38"]
["Hangnyomás szint","Hűtés","","Alacsony","dB(A)","25","25","31"]
["","","","Csendes működés","dB(A)","20","20","27"]
["","Fűtés","","Magas","dB(A)","38","39","46"]
["Hangnyomásszint","Fűtés","","Közepes","dB(A)","32","32","40"]
["Hangnyomás szint","Fűtés","","Alacsony","dB(A)","25","25","35"]
["","","","Csendes működés","dB(A)","19","19","29"]
["Hűtőközeg","GWP","","","","675","675","675"]
["Csőcsatlakozások","Folyadék","","Külső átm.","mm","6.4","6.4","6.4"]
["","Gáz","","Külső átm.","mm","9.5","9.5","12.7"]
["","Ürítés","","","","VP20 (I.D. 20/O.D. 26)","VP20 (I.D. 20/O.D. 26)","VP20 (I.D. 20/O.D. 26)"]
["Vezérlőrendszerek","Infravörös távszabályzó","","","","ARC466A66","ARC466A66","ARC466A66"]
["","Vezetékes távszabályzó","","","","BRC073A1","BRC073A1","BRC073A1"]
["Standard Accessories","Installation manual","","","","1","1","1"]
["","Wireless remote control","","","","1","1","1"]
["","AAA dry-cell batteries","","","","2","2","2"]
["","General safety precautions","","","","1","1","1"]
["","Operation manual","","","","1","1","1"]
["","Titanium apatite deodorizing filter","","","","2","2","2"]
["","Remote control holder","","","","1","1","1"]
["","Screw bag","","","","1","1","1"]
["Áramellátás","fázis","","","","1~","1~","1~"]
["","Frekvencia","","","Hz","50","50","50"]
["","Feszültség","","","V","220-240","220-240","220-240"]