{"text_format":"2","workbook":"xls","n_sheets":1,"sheets":["Products"],"not_rendered":{"charts":0,"images":0,"macros":0,"external_links":1,"defined_names":0,"comments":0,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"run_cost":"one","rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900","formulas":"cached_only"}

{"sheet":"Products","index":0,"n_rows":30,"n_cols":5,"rows_kept":30,"cut":false,"hidden":false,"merged":[],"flags":["formulas_cached_only"]}
["PRODUCT NAME","FVXTM-A / RXTM-A"]
[]
[]
[]
[]
["","","","","FVXTM30A3V1B / RXTM30A2V1B"]
["Hűtési teljesítmény","Min.","","kW","1.2"]
["","Névl.","","kW","3"]
["","Max.","","kW","4.4"]
["Fűtőkapacitás","Min.","","kW","1.2"]
["","Névl.","","kW","3.2"]
["","Max.","","kW","6.2"]
["Névleges hatékonyság","EER","","","4.35"]
["","COP","","","4.45"]
["","Éves energiafogyasztás","","kWh","345"]
["Normál hatékonyság","Energiacímkézés irányelve","Hűtés","","A"]
["","","Fűtés","","A"]
["Felülethűtés","Energiatakarékossági osztály","","","A++"]
["","Kapacitás","Pdesign","kW","3"]
["","SEER","","","7.5"]
["","Éves energiafogyasztás","","kWh/a","140"]
["Felülethűtés (Mérsékelt éghajlat)","Energiatakarékossági osztály","","","A++"]
["","Kapacitás","Pdesign","kW","3"]
["","SCOP/A","","","4.75"]
["","Pdh fűtőteljesítmény -10 ° hőmérsékleten","","kW","3"]
["","Éves energiafogyasztás","","kWh/a","884"]
["Notes","","","","(1) - Az elektromos adatokat lásd külön rajzokon"]
["","","","","(2) - Az üzemi tartomány tekintetében ld. az önálló ábrát"]
["","","","","(3) - A névleges hűtési teljesítmények a következő feltételekre vonatkoznak: belső hőmérséklet: 27 °C száraz hőm., 19 °C nedves hőm., kültéri hőm.: 35°C száraz, a hűtőközeg egyenértékű csővezetékhossza: 5m, szintkülönbség: 0m."]
["","","","","(4) - A névleges fűtési kapacitás alapja: belső hőmérséklet: 20°C száraz, kültéri hőmérséklet: 7 °C száraz, 6 °C párás, a hűtőközeg egyenértékű csővezetékhossza: 5m, szintkülönbség: 0m."]