{"text_format":"2","workbook":"xls","n_sheets":1,"sheets":["Products"],"not_rendered":{"charts":0,"images":0,"macros":0,"external_links":1,"defined_names":0,"comments":0,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"run_cost":"one","rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900","formulas":"cached_only"}

{"sheet":"Products","index":0,"n_rows":52,"n_cols":6,"rows_kept":52,"cut":false,"hidden":false,"merged":[],"flags":["formulas_cached_only"]}
["PRODUCT NAME","FVXTM-B"]
[]
[]
[]
[]
["","","","","","FVXTM30B2V1B"]
["Elektromos bemenet","Hűtés","","Névl.","kW","0.02"]
["","Fűtés","","Névl.","kW","0.03"]
["Burkolat","Szín","","","","Fehér"]
["Méretek","Egység","","Magasság","mm","600"]
["","","","Szélesség","mm","750"]
["","","","Mélység","mm","238"]
["Tömeg","Egység","","","kg","17"]
["Ventilátor","Légáramlási arány","Hűtés","Magas","m³/perc","9"]
["","Légszállítási sebesség","Hűtés","Közepes","m³/perc","6.7"]
["","","","Alacsony","m³/perc","4.8"]
["","","","Csendes működés","m³/perc","4"]
["","","Fűtés","Magas","m³/perc","9.4"]
["","Légszállítási sebesség","Fűtés","Közepes","m³/perc","6.8"]
["","","Fűtés","Alacsony","m³/perc","5.3"]
["","","","Csendes működés","m³/perc","4"]
["Hangteljesítményszint","Hűtés","","","dB(A)","53"]
["","Fűtés","","","dB(A)","53"]
["Hangnyomás szint","Hűtés","","Magas","dB(A)","39"]
["Hangnyomásszint","Hűtés","","Közepes","dB(A)","32"]
["Hangnyomás szint","Hűtés","","Alacsony","dB(A)","25"]
["","","","Csendes működés","dB(A)","20"]
["","Fűtés","","Magas","dB(A)","39"]
["Hangnyomásszint","Fűtés","","Közepes","dB(A)","32"]
["Hangnyomás szint","Fűtés","","Alacsony","dB(A)","25"]
["","","","Csendes működés","dB(A)","19"]
["Hűtőközeg","GWP","","","","675"]
["Csőcsatlakozások","Folyadék","","Külső átm.","mm","6.35"]
["","Gáz","","Külső átm.","mm","9.5"]
["","Ürítés","","","","VP20 (I.D. 20/O.D. 26)"]
["Vezérlőrendszerek","Infravörös távszabályzó","","","","ARC466A90"]
["","Vezetékes távszabályzó","","","","BRC073A1"]
["Standard Accessories","Installation manual","","","","1"]
["","Wireless remote control","","","","1"]
["","AAA dry-cell batteries","","","","2"]
["","General safety precautions","","","","1"]
["","Operation manual","","","","1"]
["","Titanium apatite deodorizing filter","","","","2"]
["","Remote control holder","","","","1"]
["","Screw bag","","","","1"]
["Áramellátás","Megnevezés","","","","V1"]
["","fázis","","","","1~"]
["","Frekvencia","","","Hz","50"]
["","Feszültség","","","V","220-240"]
["Notes","","","","","(1) - Hűtés: belső hőm. 27 °C száraz, 19 °C nedves hőm.; kültéri hőm. 35°C száraz hőm., 24°C nedves hőm.; egyenlő csőhossz: 5m"]
["","","","","","(2) - Fűtés: belső hőm. 20°C száraz hőm.; külső hőm. 7 °C száraz hőm., 6 °C nedves hőm.; a hűtőközeg egyenértékű csővezetékhossza: 5m"]
["","","","","","(3) - Az elektromos adatokat lásd külön rajzokon"]