{"text_format":"2","workbook":"xls","n_sheets":1,"sheets":["Products"],"not_rendered":{"charts":0,"images":0,"macros":0,"external_links":1,"defined_names":0,"comments":0,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"run_cost":"one","rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900","formulas":"cached_only"}

{"sheet":"Products","index":0,"n_rows":29,"n_cols":11,"rows_kept":29,"cut":false,"hidden":false,"merged":[],"flags":["formulas_cached_only"]}
["PRODUCT NAME","GM R290"]
[]
[]
[]
[]
["","","","","","BGM0870Y1ACA","MGM1280Y1ACA","MGM2210Y1ACA","MGM2210Y1WAA","BGM0870Y1WAA","MGM1280Y1WAA"]
["Fagyasztási teljesítmény","Alacsony hőmérséklet","R-290","Névl.","kW","0.871","","","","0.871"]
["","Közepes hőmérséklet","R-290","Névl.","kW","","1.281","2.206","2.206","","1.281"]
["Burkolat","Szín","","Kondenzáló egység","","Szürke","Szürke","Szürke","Szürke","Szürke","Szürke"]
["Méretek","Egység","","Magasság","mm","735","735","830","830","735","735"]
["","","","Szélesség","mm","400","400","620","620","400","400"]
["","","","Mélység","mm","790","790","790","790","790","790"]
["Tömeg","Egység","","","kg","64","56","80","80","64","56"]
["Kompresszor","Mennyiség_","","","","1","1","1","1","1","1"]
["","Típus","","","","Hajtott gőzkompresszor","Hajtott gőzkompresszor","Hajtott gőzkompresszor","Hajtott gőzkompresszor","Hajtott gőzkompresszor","Hajtott gőzkompresszor"]
["","Modell","","","","NT2180UV","NEU6217U","NTX6225UV","NT6230U/CSR","NT2210U/CSR","NT6220U/CSR"]
["","Indítási mód_","","","","Közvetlen","Közvetlen","Közvetlen","Közvetlen","Közvetlen","Közvetlen"]
["Kondenzátor","Légáram","","","m³/óra","600","600","1,200","1,200","600","600"]
["Leolvasztás","","","","","Forró gáz","Forró gáz","Forró gáz","Forró gáz","Forró gáz","Forró gáz"]
["Párologtató","Kifúvás","","","m","4","4","4","4","4","4"]
["Üzemi tartomány","Hűtőkamra hőmérséklete","","Min.","°C","-25","-5","-5","-5","-25","-5"]
["","","","Max.","°C","-15","10","10","10","-15","10"]
["","Külső hőmérséklet","","Min.","°C","20","20","20","20","20","20"]
["","","","Max.","°C","45","45","45","45","45","45"]
["Hűtőközeg","Típus","","","","R-290","R-290","R-290","R-290","R-290","R-290"]
["","GWP","","","","3","3","3","3","3","3"]
["Áramellátás","Feszültség","","","V","220-230","220-230","220-230","220-230","220-230","220-230"]
["","fázis","","","","1~","1~","1~","1~","1~","1~"]
["","Frekvencia","","","Hz","60","60","60","50","50","50"]