{"text_format":"2","workbook":"xls","n_sheets":1,"sheets":["Products"],"not_rendered":{"charts":0,"images":0,"macros":0,"external_links":1,"defined_names":0,"comments":0,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"run_cost":"one","rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900","formulas":"cached_only"}

{"sheet":"Products","index":0,"n_rows":35,"n_cols":7,"rows_kept":35,"cut":false,"hidden":false,"merged":[],"flags":["formulas_cached_only"]}
["PRODUCT NAME","JEHCCU-CL3"]
[]
[]
[]
[]
["","","","","","JEHCCU0180CL3","JEHCCU0210CL3"]
["Fagyasztási teljesítmény","Alacsony hőmérséklet","R-449A","Névl.","kW","0.98","1.36"]
["","","R-448A","Névl.","kW","0.98","1.36"]
["Áramfelvétel","Alacsony hőmérséklet","R-449A","Névl.","kW","0.98","1.36"]
["","","R-448A","Névl.","kW","0.98","1.36"]
["COP","Alacsony hőmérséklet","","R-449A","","1.00","1.00"]
["","","","R-448A","","1.00","1.00"]
["Jellemzők teljes terhelés mellett, környezeti hőmérs. 32°C (A pont)","R-448A","Hőm. -10°C","Névl. hűtési teljesítm. (PA)","kW","0.98","1.36"]
["","","","Névl. áramfelvétel (DA)","kW","0.98","1.36"]
["Jellemzők teljes terhelés mellett, környezeti hőmérsékleten 32°C (A pont)","R-448A","Hőm. -10°C","Névleges COP (COPA)","","1.00","1.00"]
["Jellemzők teljes terhelés mellett, környezeti hőmérs. 32°C (A pont)","R-449A","Hőm. -10°C","Névl. hűtési teljesítm. (PA)","kW","0.98","1.36"]
["","","","Névl. áramfelvétel (DA)","kW","0.98","1.36"]
["Jellemzők teljes terhelés mellett, környezeti hőmérsékleten 32°C (A pont)","R-449A","Hőm. -10°C","Névleges COP (COPA)","","1.00","1.00"]
["Jellemzők teljes terhelés mellett, környezeti hőmérsékleten 25°C","R-448A","Hőm. -35°C","Áramfelvétel (D2)","kW","1.00","1.38"]
["","","","Névleges COP (COP2)","","1.15","1.09"]
["","R-449A","Hőm. -35°C","Névleges COP (COP2)","","1.15","1.09"]
["Ventilátor","Típus","","","","Axiális","Axiális"]
["Méretek","Egység","","Magasság","mm","662","662"]
["","","","Szélesség","mm","1101","1101"]
["","","","Mélység","mm","444","444"]
["Tömeg","Egység","","","kg","80","81"]
["Burkolat","Szín","","","","Világosszürke","Világosszürke"]
["Hűtőközeg","5. típus","","","","R-448A","R-448A"]
["","GWP 5-ös típus","","","","1387","1387"]
["Áramellátás","fázis","","","","3~","3~"]
["","Frekvencia","","","Hz","50","50"]
["","Feszültség","","","V","400","400"]
["Notes","","","","","(1) - SRG 20°C, Ta=32°C, Te=-35°C","(1) - SRG 20°C, Ta=32°C, Te=-35°C"]
["","","","","","(2) - A hangnyomás szintjét 10 méterről, nem visszhangzó szobában mértük","(2) - A hangnyomás szintjét 10 méterről, nem visszhangzó szobában mértük"]
["","","","","","(3) - Működéséhez fluor-tartalmú, az ózonréteget károsító gázt használ","(3) - Működéséhez fluor-tartalmú, az ózonréteget károsító gázt használ"]