{"text_format":"2","workbook":"xls","n_sheets":1,"sheets":["Products"],"not_rendered":{"charts":0,"images":0,"macros":0,"external_links":1,"defined_names":0,"comments":0,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"run_cost":"one","rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900","formulas":"cached_only"}

{"sheet":"Products","index":0,"n_rows":42,"n_cols":6,"rows_kept":42,"cut":false,"hidden":false,"merged":[],"flags":["formulas_cached_only"]}
["PRODUCT NAME","LRYEQ-AY"]
[]
[]
[]
[]
["","","","","","LRYEQ16A7Y1"]
["Standard Accessories","Telepítési utasítás","","","","1"]
["","Használati utasítás","","","","1"]
["","Csatlakozó csövek","","","","1"]
["","Hűtőközeg címkéje az F-gáz szabályozáshoz","","","","1"]
["","Hűtőközeg töltési címke","","","","1"]
["","Fluorinált káros gázokra vonatkozó többnyelvű címke","","","","1"]
["Tömeg","Egység","","","kg","370"]
["Refrigerant","Charge","","","TCO2Eq","24.0"]
["","GWP","","","","2,087.5"]
["","Töltet","","","kg","11.5"]
["","Típus","","","","R-410A"]
["Fan motor","Kimenet","","","W","750"]
["","Meghajtás","","","","Közvetlen meghajtás"]
["Hőcserélő","Típus","","","","Keresztbordás tekercs"]
["Méretek","Egység","","Szélesség","pp","1,240"]
["","","","Mélység","pp","765"]
["","","","Magasság","pp","1,680"]
["Burkolat","Colour","","","","Elefántcsontszínű_"]
["Ventilátor","Type","","","","Propeller ventilátor"]
["","Légáramlási arány","Hűtés","Névl.","m³/perc","230"]
["","Mennyiség","","","","2"]
["Power supply","fázis","","","","3~"]
["","Frekvencia","","","Hz","50"]
["","Feszültség","","","V","380-415"]
["Notes","","","","","(1) - Hűtési prioritás mód: belső hőm. 27 °C száraz, 19 °C nedves hőmérséklet; külső hőm. 35°C száraz hőm.; csőhossz; 7,5m; szintkülönbség: 0 m"]
["","","","","","(2) - Hűtési prioritás mód: párologtatási hőm. -10℃; külső hőm. 35°C száraz hőm.; Beszívás SH: 10°C"]
["","","","","","(3) - Hővisszanyerés 100% mód: belső hőm. 20°C száraz hőm.; külső hőm. 7 °C száraz / 6 °C párás hőmérséklet; hűtési terhelés 18kW; csőhossz; 7,5m; szintkülönbség: 0m"]
["","","","","","(4) - A beszívási nyomásnak megfelelő telítési hőmérséklet (hűtési oldal): -10°C (hűtött állapotban); a beltéri légkondicionáló csatlakoztatási kapacitása: 10HP, ha a hővisszanyerés 100%"]
["","","","","","(5) - Kompresszor 1"]
["","","","","","(6) - Kompresszor 2"]
["","","","","","(7) - Kompresszor 3"]
["","","","","","(8) - Az egység gyári töltési mennyisége"]
["","","","","","(9) - Az olajcsapdát a kültéri egységtől 5m-re telepítse"]
["","","","","","(10) - További részleteket lásd az üzemi tartomány ábrán"]
["","","","","","(11) - A standard kiegészítőkre vonatkozó további részletekért lásd a Beszerelési/működtetési útmutatót"]
["","","","","","(12) - Fluor-tartalmú, az ózonréteget károsító gázt tartalmaz"]