{"text_format":"2","workbook":"xls","n_sheets":1,"sheets":["Products"],"not_rendered":{"charts":0,"images":0,"macros":0,"external_links":1,"defined_names":0,"comments":0,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"run_cost":"one","rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900","formulas":"cached_only"}

{"sheet":"Products","index":0,"n_rows":42,"n_cols":6,"rows_kept":42,"cut":false,"hidden":false,"merged":[],"flags":["formulas_cached_only"]}
["PRODUCT NAME","MC30YV"]
[]
[]
[]
[]
["","","","","","MC30YVM"]
["Típus","","","","","Légtisztító"]
["Alkalmazás","","","","","Padlón álló típus"]
["Burkolat","Szín","","","","Fehér"]
["Méretek","Egység","","Magasság","mm","450"]
["","","","Szélesség","mm","270"]
["","","","Mélység","mm","270"]
["Tömeg","Egység","","","kg","5.8"]
["Személyre szabható szobaterület","m²","","","","23 (1), 46 (2)"]
["CADR","m³/ó","","","","180"]
["Légtisztító működés","Elektromos bemenet","","Turbó","kW","0.025"]
["","","","M","kW","0.015"]
["","","","Csendes","kW","0.008"]
["Hangnyomás szint","Légtisztító működés","","Turbó","dB(A)","37"]
["","","","Közepes","dB(A)","27"]
["","","","Csendes","dB(A)","19"]
["Ventilátor","Légáramlási arány","Légtisztító működés","Turbó","m³/ó","180"]
["","","","Közepes","m³/ó","120"]
["","","","Csendes","m³/ó","60"]
["Porgyűjtési eljárás","","","","","Elektrosztatikus HEPA szűrő"]
["Deodorizing method","","","","","Flash streamer + Szagtalanító katalizátor"]
["Standard Accessories","Elektrosztatikus HEPA szűrő","","","","1"]
["","Szagtalanító szűrő","","","","1"]
["","Használati utasítás","","","","1"]
["Hálózati csatlakozózsinór","m","","","","1.8"]
["Power supply","fázis","","","","1~"]
["","Frekvencia","","","Hz","50/60"]
["","Feszültség","","","V","220-240/220-230"]
["Működési áram","Légtisztító működés","","Turbó","A","0.13"]
["","","","Közepes","A","0.09"]
["","","","Csendes","A","0.08"]
["Notes","","","","","(1) - Az alkalmazható helyiségterület megfelelő az egység maximális ventilátorsebességen történő működtetéséhez (HH). Az alkalmazható helyiségterület azt a teret jelöli, ahonnan egy bizonyos mennyiségű porrészecskét 30 perc alatt el lehet távolítani. (JEM 1467)"]
["","","","","","(2) - Az alkalmazható helyiségterület megfelelő az egység maximális ventilátorsebességen történő működtetéséhez (HH). Az alkalmazható helyiségterület számítása az NRCC-54013 szabvány alapján, cigarettafüst CADR használatával történt, amelyet a JEM1467 szerint teszteltek."]
["","","","","","(3) - Átalakítva CADR szabványokká mérési értékekből a JEM1467-nek megfelelően."]
["","","","","","(4) - Az üzemi hangszintek a készülék előtt, felett, jobbra és balra 1 méterre mért értékek átlaga. (Megegyeznek a visszhangmentes szobában mért értékkel.)"]
["","","","","","(5) - Az elektrosztatikus HEPA szűrő az egységhez mellékelve."]
["","","","","","(6) - Egyéb funkció: Automatikus újraindítási funkció."]