{"text_format":"2","workbook":"xls","n_sheets":1,"sheets":["Products"],"not_rendered":{"charts":0,"images":0,"macros":0,"external_links":1,"defined_names":0,"comments":0,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"run_cost":"one","rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900","formulas":"cached_only"}

{"sheet":"Products","index":0,"n_rows":63,"n_cols":6,"rows_kept":63,"cut":false,"hidden":false,"merged":[],"flags":["formulas_cached_only"]}
["PRODUCT NAME","MCK55W"]
[]
[]
[]
[]
["","","","","","MCK55WVM"]
["Type","","","","","Párásító légtisztító"]
["Személyre szabható","","","","","Padlón álló típus"]
["Burkolat","Szín","","","","Fehér"]
["Méretek","Egység","","Magasság","mm","700"]
["","","","Szélesség","mm","270"]
["","","","Mélység","mm","270"]
["Tömeg","Egység","","","kg","9.5"]
["Személyre szabható szobaterület","m²","","","","41 (1), 82 (2)"]
["CADR","m³/ó","","","","320"]
["Légtisztító működés","Elektromos bemenet","","Turbó","kW","0.056"]
["","","","M","kW","0.017"]
["","","","L","kW","0.010"]
["","","","Csendes","kW","0.007"]
["Párásító működés","Elektromos bemenet","","Turbó","kW","0.058"]
["","","","M","kW","0.019"]
["","","","L","kW","0.014"]
["","","","Csendes","kW","0.011"]
["","Víztartály kapacitása","","","l","2.7"]
["Hangnyomás szint","Légtisztító működés","","Turbó","dB(A)","53.0"]
["","","","Közepes","dB(A)","39.0"]
["","","","Alacsony","dB(A)","29.0"]
["","","","Csendes","dB(A)","19.0"]
["","Párásító működés","","Turbó","dB(A)","53.0"]
["","","","Közepes","dB(A)","39.0"]
["","","","Alacsony","dB(A)","33.0"]
["","","","Csendes","dB(A)","25.0"]
["Ventilátor","Légáramlási arány","Légtisztító működés","Turbó","m³/ó","330"]
["","","","Közepes","m³/ó","192"]
["","","","Alacsony","m³/ó","120"]
["","","","Csendes","m³/ó","54"]
["","","Párásító működés","Turbó","m³/ó","330"]
["","","","Közepes","m³/ó","192"]
["","","","Alacsony","m³/ó","144"]
["","","","Csendes","m³/ó","102"]
["Porgyűjtési eljárás","","","","","Elektrosztatikus HEPA szűrő"]
["Szagtalanítási eljárás","","","","","Flash streamer + Szagtalanító katalizátor"]
["Standard Accessories","Operation manual","","","","1"]
["","Electrostatic HEPA filter","","","","1"]
["","Deodorising filter","","","","1"]
["","Caster","","","","4"]
["","Humidifying filter","","","","2"]
["","Remote control holder","","","","1"]
["","Remote control lid","","","","1"]
["Hálózati csatlakozózsinór","Hálózati csatlakozózsinór","","","","1.8"]
["Áramellátás","fázis","","","","1~"]
["","Áramellátás-=-Frekvencia","","Frekvencia","","50/60"]
["","Áramellátás-=-Feszültség","","Feszültség","","220-240/220-230"]
["Működési áram","Légtisztító működés","Működési áram-=-Légtisztító működés-=-Turbó","Turbó","","0.50"]
["","","Működési áram-=-Légtisztító működés-=-Közepes","Közepes","","0.19"]
["","","Működési áram-=-Légtisztító működés-=-Alacsony","Alacsony","","0.12"]
["","","Működési áram-=-Légtisztító működés-=-Csendes","Csendes","","0.09"]
["","Párásító működés","Működési áram-=-Párásító működés-=-Turbó","Turbó","","0.50"]
["","","Működési áram-=-Párásító működés-=-Közepes","Közepes","","0.20"]
["","","Működési áram-=-Párásító működés-=-Alacsony","Alacsony","","0.15"]
["","","Működési áram-=-Párásító működés-=-Csendes","Csendes","","0.13"]
["Notes","","","","","(1) - Az alkalmazható helyiségterület megfelelő az egység maximális ventilátorsebességen történő működtetéséhez (HH). Az alkalmazható helyiségterület azt a teret jelöli, ahonnan egy bizonyos mennyiségű porrészecskét 30 perc alatt el lehet távolítani. (JEM 1467)"]
["","","","","","(2) - Átalakítva NRCC szabványokká mérési értékekből a JEM1467-nek megfelelően."]