{"text_format":"2","workbook":"xls","n_sheets":1,"sheets":["Products"],"not_rendered":{"charts":0,"images":0,"macros":0,"external_links":1,"defined_names":0,"comments":0,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"run_cost":"one","rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900","formulas":"cached_only"}

{"sheet":"Products","index":0,"n_rows":54,"n_cols":6,"rows_kept":54,"cut":false,"hidden":false,"merged":[],"flags":["formulas_cached_only"]}
["PRODUCT NAME","MCK70YV"]
[]
[]
[]
[]
["","","","","","MCK70YVM"]
["Típus","","","","","Párásító légtisztító"]
["Személyre szabható","","","","","Padlón álló típus"]
["Burkolat","Szín","","","","Fehér (N9. 0)"]
["Méretek","Egység","","Magasság","mm","600 (5)"]
["","","","Szélesség","mm","395"]
["","","","Mélység","mm","287"]
["Tömeg","Egység","","","kg","12.5"]
["Személyre szabható szobaterület","m²","","","","48 (1), 96 (2)"]
["CADR","m³/ó","","","","375"]
["Légtisztító működés","Elektromos bemenet","","Turbó","kW","0.066"]
["","","","M","kW","0.016"]
["","","","L","kW","0.01"]
["","","","Csendes","kW","0.008"]
["Párásító működés","Elektromos bemenet","","Turbó","kW","0.068"]
["","","","M","kW","0.018"]
["","","","L","kW","0.012"]
["","","","Csendes","kW","0.011"]
["","Víztartály kapacitása","","","l","3.6"]
["Hangnyomás szint","Légtisztító működés","","Turbó","dB(A)","54"]
["","","","Közepes","dB(A)","37"]
["","","","Alacsony","dB(A)","27"]
["","","","Csendes","dB(A)","18"]
["","Párásító működés","","Turbó","dB(A)","54"]
["","","","Közepes","dB(A)","37"]
["","","","Alacsony","dB(A)","27"]
["","","","Csendes","dB(A)","23"]
["Ventilátor","Légáramlási arány","Légtisztító működés","Turbó","m³/ó","420"]
["","","","Közepes","m³/ó","210"]
["","","","Alacsony","m³/ó","132"]
["","","","Csendes","m³/ó","60"]
["","","Párásító működés","Turbó","m³/ó","420"]
["","","","Közepes","m³/ó","210"]
["","","","Alacsony","m³/ó","132"]
["","","","Csendes","m³/ó","102"]
["Porgyűjtési eljárás","","","","","Elektrosztatikus HEPA szűrő"]
["Szagtalanítási eljárás","","","","","Flash streamer + Szagtalanító katalizátor"]
["Standard Accessories","Operation manual","","","","1"]
["","Electrostatic HEPA filter","","","","1"]
["","Deodorising filter","","","","1"]
["","Caster","","","","4"]
["","Humidifying filter","","","","1"]
["Hálózati csatlakozózsinór","m","","","","2"]
["Áramellátás","fázis","","","","1~"]
["","Frekvencia","","","Hz","50/60"]
["","Feszültség","","","V","220-240/220-230"]
["Notes","","","","","(1) - A lefedett terület megfelelő az egység maximális ventilátorsebességen történő működtetéséhez (HH). A lefedett terület azt a teret jelöli, ahonnan egy bizonyos mennyiségű porrészecskét 30 perc alatt el lehet távolítani."]
["","","","","","(2) - Átalakítva NRCC szabványokká mérési értékekből a JEM1467-nek megfelelően."]
["","","","","","(3) - Az üzemi hangszintek a készülék előtt, felett, jobbra és balra 1 méterre mért értékek átlaga. (Megegyeznek a visszhangmentes szobában mért értékkel.)"]