{"text_format":"2","workbook":"xls","n_sheets":1,"sheets":["Products"],"not_rendered":{"charts":0,"images":0,"macros":0,"external_links":1,"defined_names":0,"comments":0,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"run_cost":"one","rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900","formulas":"cached_only"}

{"sheet":"Products","index":0,"n_rows":36,"n_cols":8,"rows_kept":36,"cut":false,"hidden":false,"merged":[],"flags":["formulas_cached_only"]}
["PRODUCT NAME","RXA-A8"]
[]
[]
[]
[]
["","","","","","RXA20A5V1B8","RXA25A5V1B8","RXA35A5V1B8"]
["Méretek","Egység","","Magasság","mm","550","550","550"]
["","","","Szélesség","mm","840","840","840"]
["","","","Mélység","mm","350","350","350"]
["Tömeg","Egység","","","kg","32","32","32"]
["Kompresszor","Típus","","","","Hermetikusan zárt lengő kompresszor","Hermetikusan zárt lengő kompresszor","Hermetikusan zárt lengő kompresszor"]
["Üzemi tartomány","Hűtés","Környezeti","Min.","°C száraz hőm.","-10","-10","-10"]
["","","","Max.","°C száraz hőm.","46","46","46"]
["","Fűtés","Környezeti","Min.","°C párás hőm.","-15","-15","-15"]
["","","","Max.","°C párás hőm.","18","18","18"]
["Hangnyomás szint","Hűtés","","Névl.","dB(A)","46.0","46.0","49.0"]
["","Fűtés","","Névl.","dB(A)","47.0","47.0","49.0"]
["Hűtőközeg","Típus","","","","R-32","R-32","R-32"]
["","Töltet","","","kg","0.76","0.76","0.76"]
["","Töltet","","","tCO2Eq","0.52","0.52","0.52"]
["","GWP","","","","675.0","675.0","675.0"]
["Csőcsatlakozások","Csőhossz","Max.","OU - IU","m","20","20","20"]
["","További hűtőközeg utántöltés","","","kg/m","0,02 (10m-t meghaladó csőhosszhoz)","0,02 (10m-t meghaladó csőhosszhoz)","0,02 (10m-t meghaladó csőhosszhoz)"]
["","Szintkülönbség","IU - OU","Max.","m","15.0","15.0","15.0"]
["Standard Accessories","Installation manual","","","","1","1","1"]
["","Refrigerant charge label","","","","1","1","1"]
["","Multilingual fluorinated greenhouse gases labels","","","","1","1","1"]
["","General safety precautions","","","","1","1","1"]
["","Drain plug","","","","1","1","1"]
["Energiatakarékossági besorolás","","","","","A+++ ~ D","A+++ ~ D","A+++ ~ D"]
["Áramellátás","fázis","","","","1~","1~","1~"]
["","Frekvencia","","","Hz","50","50","50"]
["","Feszültség","","","V","220-240","220-240","220-240"]
["Notes","","","","","(1) - Fluor-tartalmú, az ózonréteget károsító gázt tartalmaz","(1) - Fluor-tartalmú, az ózonréteget károsító gázt tartalmaz","(1) - Fluor-tartalmú, az ózonréteget károsító gázt tartalmaz"]
["","","","","","(2) - Az üzemi tartomány tekintetében ld. az önálló ábrát","(2) - Az üzemi tartomány tekintetében ld. az önálló ábrát","(2) - Az üzemi tartomány tekintetében ld. az önálló ábrát"]
["","","","","","(3) - Az elektromos adatokat lásd külön rajzokon","(3) - Az elektromos adatokat lásd külön rajzokon","(3) - Az elektromos adatokat lásd külön rajzokon"]