{"text_format":"2","workbook":"xls","n_sheets":1,"sheets":["Products"],"not_rendered":{"charts":0,"images":0,"macros":0,"external_links":1,"defined_names":0,"comments":0,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"run_cost":"one","rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900","formulas":"cached_only"}

{"sheet":"Products","index":0,"n_rows":31,"n_cols":16,"rows_kept":31,"cut":false,"hidden":false,"merged":[],"flags":["formulas_cached_only"]}
["PRODUCT NAME","RXB-C"]
[]
[]
[]
[]
["","","","","","RXB20C2V1B","RXB20C5V1B","RXB20C5V1B9","RXB25C2V1B","RXB25C5V1B","RXB25C5V1B9","RXB35C2V1B","RXB35C5V1B","RXB35C5V1B9","RXB50CV1B","RXB60CV1B"]
["Méretek","Egység","","Magasság","mm","550","550","550","550","550","550","550","550","550","753","753"]
["","","","Szélesség","mm","658","658","658","658","658","658","658","658","658","855","855"]
["","","","Mélység","mm","275","275","275","275","275","275","275","275","275","328","328"]
["Tömeg","Egység","","","kg","28","28","28","28","28","28","30","30","30","44","44"]
["Kompresszor","Típus","","","","Hermetikusan zárt lengő kompresszor","Hermetikusan zárt lengő kompresszor","Hermetikusan zárt lengő kompresszor","Hermetikusan zárt lengő kompresszor","Hermetikusan zárt lengő kompresszor","Hermetikusan zárt lengő kompresszor","Hermetikusan zárt lengő kompresszor","Hermetikusan zárt lengő kompresszor","Hermetikusan zárt lengő kompresszor","Hermetikus légterelő","Hermetikus légterelő"]
["Üzemi tartomány","Hűtés","Környezeti","Min.","°C száraz hőm.","-10","-10","-10","-10","-10","-10","-10","-10","-10","-10","-10"]
["","","","Max.","°C száraz hőm.","46","46","46","46","46","46","46","46","46","46","46"]
["","Fűtés","Környezeti","Min.","°C párás hőm.","-15","-15","-15","-15","-15","-15","-15","-15","-15","-15","-15"]
["","","","Max.","°C párás hőm.","18","18","18","18","18","18","18","18","18","18","18"]
["Hangnyomás szint","Hűtés","","Magas","dB(A)","46","46","46","46","46","46","48","48","48"]
["","","","Névl.","dB(A)","","","","","","","","","","51","51"]
["","Fűtés","","Magas","dB(A)","47","47","47","47","47","47","48","48","48"]
["","","","Névl.","dB(A)","","","","","","","","","","51","51"]
["Hűtőközeg","Típus","","","","R-410A","R-410A","R-410A","R-410A","R-410A","R-410A","R-410A","R-410A","R-410A","R-410A","R-410A"]
["","Töltet","","","kg","0.74","0.74","0.74","0.74","0.74","0.74","1.0","1.0","1.0","1.45","1.45"]
["","Töltet","","","tCO2Eq","1.5","1.5","1.5","1.5","1.5","1.5","2.1","2.1","2.1","3.0","3.0"]
["","GWP","","","","2087.5","2087.5","2087.5","2087.5","2087.5","2087.5","2087.5","2087.5","2087.5","2087.5","2087.5"]
["Csőcsatlakozások","Csőhossz","Max.","OU - IU","m","","","","","","","","","","30","30"]
["Standard Accessories","Installation manual","","","","1","1","1","1","1","1","1","1","1"]
["","Refrigerant charge label","","","","1","1","1","1","1","1","1","1","1"]
["","Multilingual fluorinated greenhouse gases labels","","","","1","1","1","1","1","1","1","1","1"]
["","Drain plug (only heat pump models)","","","","1","1","1","1","1","1","1","1","1"]
["Áramellátás","fázis","","","","1~","1~","1~","1~","1~","1~","1~","1~","1~","1~","1~"]
["","Frekvencia","","","Hz","50","50","50","50","50","50","50","50","50","50","50"]
["","Feszültség","","","V","220-240","220-240","220-240","220-240","220-240","220-240","220-240","220-240","220-240","220-240","220-240"]