{"text_format":"2","workbook":"xls","n_sheets":1,"sheets":["Products"],"not_rendered":{"charts":0,"images":0,"macros":0,"external_links":1,"defined_names":0,"comments":0,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"run_cost":"one","rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900","formulas":"cached_only"}

{"sheet":"Products","index":0,"n_rows":27,"n_cols":11,"rows_kept":27,"cut":false,"hidden":false,"merged":[],"flags":["formulas_cached_only"]}
["PRODUCT NAME","RXC-D"]
[]
[]
[]
[]
["","","","","","RXC20DV1B","RXC25DV1B","RXC35DV1B","RXC50DV1B","RXC60DV1B","RXC71DV1B"]
["Hangteljesítményszint","Hűtés","","","dB(A)","58","58","60","65","66","69"]
["Méretek","Egység","","Magasság","mm","550","550","550","615","615","695"]
["","","","Szélesség","mm","658","658","658","845","845","930"]
["","","","Mélység","mm","273","273","273","300","300","350"]
["Tömeg","Egység","","","kg","24","24","26","39","39","45"]
["Kompresszor","Típus","","","","Hermetikus légterelő","Hermetikus légterelő","Hermetikus légterelő","Hermetikus légterelő","Hermetikus légterelő","Hermetikus légterelő"]
["Üzemi tartomány","Hűtés","Környezeti","Min.","°C száraz hőm.","10","10","10","-10","-10","-10"]
["","","","Max.","°C száraz hőm.","46","46","46","46","46","46"]
["","Fűtés","Környezeti","Min.","°C párás hőm.","-15","-15","-15","-15","-15","-15"]
["","","","Max.","°C párás hőm.","18","18","18","18","18","18"]
["Hangnyomás szint","Hűtés","","Magas","dB(A)","45","45","46","51","54","54"]
["Hűtőközeg","Típus","","","","R-32","R-32","R-32","R-32","R-32","R-32"]
["","Töltet","","","kg","0.55","0.55","0.75","1","1.1","1.15"]
["","Töltet","","","tCO2Eq","0.371","0.371","0.506","0.675","0.743","0.776"]
["","GWP","","","","675.0","675.0","675.0","675.0","675.0","675.0"]
["Csőcsatlakozások","Csőhossz","Max.","OU - IU","m","20","20","20","30","30","30"]
["","További hűtőközeg utántöltés","","","kg/m","0 017 (75m-t meghaladó csőhosszhoz)","0 017 (75m-t meghaladó csőhosszhoz)","0 017 (75m-t meghaladó csőhosszhoz)","0 017 (75m-t meghaladó csőhosszhoz)","0 017 (75m-t meghaladó csőhosszhoz)","0 017 (75m-t meghaladó csőhosszhoz)"]
["","Szintkülönbség","IU - OU","Max.","m","15.0","15.0","15.0","20.0","20.0","20.0"]
["Áramellátás","fázis","","","","1~","1~","1~","1~","1~","1~"]
["","Frekvencia","","","Hz","50","50","50","50","50","50"]
["","Feszültség","","","V","220-240","220-240","220-240","220-240","220-240","220-240"]