{"text_format":"2","workbook":"xls","n_sheets":1,"sheets":["Products"],"not_rendered":{"charts":0,"images":0,"macros":0,"external_links":1,"defined_names":0,"comments":0,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"run_cost":"one","rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900","formulas":"cached_only"}

{"sheet":"Products","index":0,"n_rows":38,"n_cols":10,"rows_kept":38,"cut":false,"hidden":false,"merged":[],"flags":["formulas_cached_only"]}
["PRODUCT NAME","RXL-K"]
[]
[]
[]
[]
["","","","","","RXL20K3V1B","RXL25K3V1B","RXL35K2V1B","RXL42K2V1B","RXL50K2V1B"]
["Ventilátor","Légáramlási arány","Hűtés","Szuper alacsony","m³/perc","","","30.1","30.6","48.9"]
["","","Fűtés","Szuper alacsony","m³/perc","","","25.6","27.2","43.1"]
["","","","Szuper alacsony","cfm","","","1063","1080","1727"]
["","","Fűtés","Szuper alacsony","cfm","","","904","960","1522"]
["Méretek","Egység","","Magasság","pp","550","550","550","550","735"]
["","","","Szélesség","pp","765","765","765","765","825"]
["","","","Mélység","pp","285","285","285","285","300"]
["Tömeg","Egység","","","kg","34","34","34","39","47"]
["Ventilátor motor","Sebesség","Hűtés","Szuper alacsony","1/perc","780","780","780","790","670"]
["","","Fűtés","Szuper alacsony","1/perc","740","740","740","780","670"]
["Kompresszor","Type","","","","Hermetikusan zárt lengő kompresszor","Hermetikusan zárt lengő kompresszor","Hermetikusan zárt lengő kompresszor","Hermetikusan zárt lengő kompresszor","Hermetikusan zárt lengő kompresszor"]
["Üzemi tartomány","Hűtés","Környezeti","Min.","°C száraz hőm.","-10","-10","-10","-10","-10"]
["","","","Max.","°C száraz hőm.","46","46","46","46","46"]
["","Fűtés","Környezeti","Min.","°C párás hőm.","-25","-25","-25","-25","-25"]
["","","","Max.","°C párás hőm.","18","18","18","18","18"]
["Hangnyomás szint","Hűtés","","Magas","dB(A)","46","46","48","48","48"]
["","Fűtés","","Magas","dB(A)","47","47","48","48","48"]
["Hűtőközeg","Típus","","","","R-410A","R-410A","R-410A","R-410A","R-410A"]
["","Töltet","","","kg","1.0","1.05","1.2","1.3","1.7"]
["","Töltet","","","tCO2Eq","2.1","2.2","2.5","2.7","3.5"]
["","GWP","","","","2087.5","2087.5","2087.5","2087.5","2087.5"]
["Csőcsatlakozások","Csőhossz","Max.","OU - IU","m","20","20","20","20","30"]
["","További hűtőközeg utántöltés","","","kg/m","0,02 (10m-t meghaladó csőhosszhoz)","0,02 (10m-t meghaladó csőhosszhoz)","0,02 (10m-t meghaladó csőhosszhoz)","0,02 (10m-t meghaladó csőhosszhoz)","0,02 (10m-t meghaladó csőhosszhoz)"]
["","Szintkülönbség","IU - OU","Max.","m","15","15","15","15","20"]
["Standard Accessories","Installation manual","","","","1","1","1","1","1"]
["","Drain plug","","","","1"]
["Áramellátás","fázis","","","","1~","1~","1~","1~","1~"]
["","Frekvencia","","","Hz","50","50","50","50","50"]
["","Feszültség","","","V","220-240","220-240","220-230-240","220-230-240","220-230-240"]
["Notes","","","","","(1) - 220V","(1) - 220V","(1) - 220V","(1) - 220V","(1) - 220V"]
["","","","","","(2) - 230V","(2) - 230V","(2) - 230V","(2) - 230V","(2) - 230V"]
["","","","","","(3) - 240V","(3) - 240V","(3) - 240V","(3) - 240V","(3) - 240V"]