{"text_format":"2","workbook":"xls","n_sheets":1,"sheets":["Products"],"not_rendered":{"charts":0,"images":0,"macros":0,"external_links":1,"defined_names":0,"comments":0,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"run_cost":"one","rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900","formulas":"cached_only"}

{"sheet":"Products","index":0,"n_rows":36,"n_cols":7,"rows_kept":36,"cut":false,"hidden":false,"merged":[],"flags":["formulas_cached_only"]}
["PRODUCT NAME","RXLG-M"]
[]
[]
[]
[]
["","","","","","RXLG25M2V1B","RXLG35M2V1B"]
["Ventilátor","Légáramlási arány","Hűtés","Szuper alacsony","m³/perc","30.6","30.6"]
["","","Fűtés","Szuper alacsony","m³/perc","27.2","27.2"]
["","","","Szuper alacsony","cfm","1080","1080"]
["","","Fűtés","Szuper alacsony","cfm","960","960"]
["Méretek","Egység","","Magasság","mm","550","550"]
["","","","Szélesség","mm","858","858"]
["","","","Mélység","mm","330","330"]
["Tömeg","Egység","","","kg","40","40"]
["Kompresszor","Type","","","","","Hermetikusan zárt lengő kompresszor"]
["Üzemi tartomány","Hűtés","Környezeti","Min.","°C száraz hőm.","-10","-10"]
["","","","Max.","°C száraz hőm.","46","46"]
["","Fűtés","Környezeti","Min.","°C párás hőm.","-25","-25"]
["","","","Max.","°C párás hőm.","18","18"]
["Hangnyomás szint","Hűtés","","Magas","dB(A)","48","48"]
["","","","Alacsony","dB(A)","44","44"]
["","Fűtés","","Magas","dB(A)","49","49"]
["","","","Alacsony","dB(A)","45","45"]
["Hűtőközeg","Típus","","","","R-410A","R-410A"]
["","Töltet","","","kg","1","1"]
["","Töltet","","","tCO2Eq","2.1","2.1"]
["","GWP","","","","2087.5","2087.5"]
["Csőcsatlakozások","Csőhossz","Max.","OU - IU","m","20","20"]
["","További hűtőközeg utántöltés","","","kg/m","0,02 (10m-t meghaladó csőhosszhoz)","0,02 (10m-t meghaladó csőhosszhoz)"]
["","Szintkülönbség","IU - IU","Max.","m","15","15"]
["Standard Accessories","Installation manual","","","","1","1"]
["","Drain plug","","","","1","1"]
["Áramellátás","fázis","","","","1~","1~"]
["","Frekvencia","","","Hz","50","50"]
["","Feszültség","","","V","220-240","220-240"]
["Kompresszor","Típus","","","","Hermetikusan zárt lengő kompresszor"]