{"text_format":"2","workbook":"xls","n_sheets":1,"sheets":["Products"],"not_rendered":{"charts":0,"images":0,"macros":0,"external_links":1,"defined_names":0,"comments":0,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"run_cost":"one","rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900","formulas":"cached_only"}

{"sheet":"Products","index":0,"n_rows":40,"n_cols":8,"rows_kept":40,"cut":false,"hidden":false,"merged":[],"flags":["formulas_cached_only"]}
["PRODUCT NAME","RXM-A9"]
[]
[]
[]
[]
["","","","","","RXM25A5V1B9","RXM35A5V1B9","RXM50A5V1B9"]
["Méretek","Egység","","Magasság","pp","610","610","734"]
["","","","Szélesség","pp","923","923","954"]
["","","","Mélység","pp","367","367","401"]
["Tömeg","Egység","","","kg","36","36","49"]
["Ventilátor motor","Sebesség","Hűtés","Szuper alacsony","1/perc","600","600","500"]
["Kompresszor","Típus","","","","Hermetikusan zárt lengő kompresszor","Hermetikusan zárt lengő kompresszor","Hermetikusan zárt lengő kompresszor"]
["Üzemi tartomány","Hűtés","Környezeti","Min.","°C száraz hőm.","-10","-10","-10"]
["","","","Max.","°C száraz hőm.","50","50","46 (1)"]
["","Fűtés","Környezeti","Min.","°C párás hőm.","-21","-21","-15 (1)"]
["","","","Max.","°C párás hőm.","18","18","18"]
["Hangnyomás szint","Hűtés","","Névl.","dB(A)","46","47","48"]
["","Fűtés","","Névl.","dB(A)","47","49","49"]
["Hűtőközeg","Típus","","","","R-32","R-32","R-32"]
["","Töltet","","","kg","0.95","0.95","1.10"]
["","Töltet","","","tCO2Eq","0.65","0.65","0.75"]
["","GWP","","","","675","675","675"]
["Csőcsatlakozások","Csőhossz","Max.","OU - IU","m","20","20","30"]
["","További hűtőközeg utántöltés","","","kg/m","0,02 (10m-t meghaladó csőhosszhoz)","0,02 (10m-t meghaladó csőhosszhoz)","0,02 (10m-t meghaladó csőhosszhoz)"]
["","Szintkülönbség","IU - OU","Max.","m","15","15","20"]
["Standard Accessories","RXM25A5V1B9","","","","1"]
["","Installation manual","","","","1","1","1"]
["","Drain joint","","","","1","1","1"]
["","Refrigerant charge label","","","","1","1","1"]
["","Multilingual fluorinated greenhouse gases labels","","","","1","1","1"]
["","General safety precautions","","","","1","1","1"]
["","LOT10 Energy Label","","","","1","1","1"]
["","Drain cap","","","","3","3","1"]
["Áramellátás","fázis","","","","1~","1~","1~"]
["","Frekvencia","","","Hz","50","50","50"]
["","Feszültség","","","V","220-240","220-240","220-240"]
["Notes","","","","","(1) - Az üzemi tartomány tekintetében ld. az önálló ábrát","(1) - Az üzemi tartomány tekintetében ld. az önálló ábrát","(1) - Az üzemi tartomány tekintetében ld. az önálló ábrát"]
["","","","","","(2) - Az elektromos adatokat lásd külön rajzokon","(2) - Az elektromos adatokat lásd külön rajzokon","(2) - Az elektromos adatokat lásd külön rajzokon"]
["","","","","","(3) - Fluor-tartalmú, az ózonréteget károsító gázt tartalmaz","(3) - Fluor-tartalmú, az ózonréteget károsító gázt tartalmaz","(3) - Fluor-tartalmú, az ózonréteget károsító gázt tartalmaz"]
["Standard Accessories","RXM35A5V1B9","","","","","1"]