{"text_format":"2","workbook":"xls","n_sheets":1,"sheets":["Products"],"not_rendered":{"charts":0,"images":0,"macros":0,"external_links":1,"defined_names":0,"comments":0,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"run_cost":"one","rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900","formulas":"cached_only"}

{"sheet":"Products","index":0,"n_rows":33,"n_cols":9,"rows_kept":33,"cut":false,"hidden":false,"merged":[],"flags":["formulas_cached_only"]}
["PRODUCT NAME","RXM-N"]
[]
[]
[]
[]
["","","","","","RXM42N2V1B","RXM50N2V1B","RXM60N2V1B","RXM71N2V1B"]
["Méretek","Egység","","Magasság","pp","734","734","734","734"]
["","","","Szélesség","pp","870","870","870","870"]
["","","","Mélység","pp","373","373","373","320"]
["Tömeg","Egység","","","kg","50","50","50","56"]
["Kompresszor","Type","","","","Hermetikusan zárt lengő kompresszor","","Hermetikusan zárt lengő kompresszor","Hermetikusan zárt lengő kompresszor"]
["Üzemi tartomány","Hűtés","Környezeti","Min.","°C száraz hőm.","-10","-10","-10","-10"]
["","","","Max.","°C száraz hőm.","46","46","46","46"]
["","Fűtés","Környezeti","Min.","°C párás hőm.","-15","-15","-15","-15"]
["","","","Max.","°C párás hőm.","18","18","18","18"]
["Hangnyomás szint","Hűtés","","Névl.","dB(A)","48.0","48.0","48.0","47"]
["","Fűtés","","Névl.","dB(A)","48.0","49.0","49.0","48"]
["Hűtőközeg","Típus","","","","R-32","R-32","R-32","R-32"]
["","Töltet","","","kg","1.10","1.15","1.15","1.15"]
["","Töltet","","","tCO2Eq","0.75","0.78","0.78","0.78"]
["","GWP","","","","675","675","675","675.0"]
["Csőcsatlakozások","Csőhossz","Max.","OU - IU","m","30","30","30","30.0"]
["","További hűtőközeg utántöltés","","","kg/m","0,02 (10m-t meghaladó csőhosszhoz)","0,02 (10m-t meghaladó csőhosszhoz)","0,02 (10m-t meghaladó csőhosszhoz)","0,02 (10m-t meghaladó csőhosszhoz)"]
["","Szintkülönbség","IU - OU","Max.","m","20","20","20","20.0"]
["Standard Accessories","Installation manual","","","","1","1","1","1"]
["","Refrigerant charge label","","","","1","1","1","1"]
["","Multilingual fluorinated greenhouse gases labels","","","","1","1","1","1"]
["","Drain cap","","","","3","3","3","3"]
["","Drain plug","","","","1","1","1","1"]
["Áramellátás","fázis","","","","1~","1~","1~","1~"]
["","Frekvencia","","","Hz","50","50","50","50"]
["","Feszültség","","","V","220-240","220-240","220-240","220-240"]
["Kompresszor","Típus","","","","","Hermetikusan zárt lengő kompresszor"]