{"text_format":"2","workbook":"xls","n_sheets":1,"sheets":["Products"],"not_rendered":{"charts":0,"images":0,"macros":0,"external_links":1,"defined_names":0,"comments":0,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"run_cost":"one","rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900","formulas":"cached_only"}

{"sheet":"Products","index":0,"n_rows":38,"n_cols":9,"rows_kept":38,"cut":false,"hidden":false,"merged":[],"flags":["formulas_cached_only"]}
["PRODUCT NAME","RXN-L"]
[]
[]
[]
[]
["","","","","","RXN25LV1B","RXN35LV1B (Archived)","RXN50LV1B (Archived)","RXN60LV1B (Archived)"]
["Hangnyomás szint","Hűtés","","Magas","dB(A)","","48","51","51"]
["Refrigerant","Charge","","","TCO2Eq","","2.1","3","3.1"]
["","GWP","","","","","2,087.5","2,087.5","2,087.5"]
["","Töltet","","","kg","","1.00","1.45","1.50"]
["","Típus","","","","","R-410A","R-410A","R-410A"]
["Kompresszor","Type","","","","","Hermetikus légterelő","Hermetikus légterelő","Hermetikus légterelő"]
["Méretek","Berendezés","","Szélesség","mm","","658","855","855"]
["","","","Mélység","mm","","289","328","328"]
["","","","Magasság","mm","","550","753","753"]
["Tömeg","Egység","","","kg","","30","49","49"]
["Power supply","Phase","","","","","1~","1~","1~"]
["","Frekvencia","","","Hz","","50","50","50"]
["","Feszültség","","","V","","220-240","220-240","220-240"]
["Notes","","","","","","(1) - A gyártó fenntartja az összes műszaki jellemző előzetes értesítés nélküli megváltoztatásának jogát.","(1) - A gyártó fenntartja az összes műszaki jellemző előzetes értesítés nélküli megváltoztatásának jogát.","(1) - A gyártó fenntartja az összes műszaki jellemző előzetes értesítés nélküli megváltoztatásának jogát."]
["","","","","","","(2) - Fluor-tartalmú, az ózonréteget károsító gázt tartalmaz","(2) - Fluor-tartalmú, az ózonréteget károsító gázt tartalmaz","(2) - Fluor-tartalmú, az ózonréteget károsító gázt tartalmaz"]
["Méretek","Egység","","Magasság","mm","550"]
["","","","Szélesség","mm","658"]
["","","","Mélység","mm","289"]
["Tömeg","Egység","","","kg","28"]
["Kompresszor","Típus","","","","Hermetikus légterelő"]
["Üzemi tartomány","Hűtés","Környezeti","Min.","°C száraz hőm.","10"]
["","","","Max.","°C száraz hőm.","46"]
["","Fűtés","Környezeti","Min.","°C párás hőm.","-15"]
["","","","Max.","°C párás hőm.","18"]
["Hangnyomás szint","Hűtés","","Magas","dB(A)","46"]
["Hűtőközeg","Típus","","","","R-410A"]
["","Töltet","","","kg","0.74"]
["","Töltet","","","tCO2Eq","1.5"]
["","GWP","","","","2087.5"]
["Áramellátás","fázis","","","","1~"]
["","Frekvencia","","","Hz","50"]
["","Feszültség","","","V","220-240"]