{"text_format":"2","workbook":"xls","n_sheets":1,"sheets":["Products"],"not_rendered":{"charts":0,"images":0,"macros":0,"external_links":1,"defined_names":0,"comments":0,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"run_cost":"one","rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900","formulas":"cached_only"}

{"sheet":"Products","index":0,"n_rows":56,"n_cols":11,"rows_kept":56,"cut":false,"hidden":false,"merged":[],"flags":["formulas_cached_only"]}
["PRODUCT NAME","RXS-F"]
[]
[]
[]
[]
["","","","","","RXS60F4V1B","RXS60F2V1B","RXS60F3V1B","RXS71FAV1B9","RXS71FV1B","RXS71FAV1B"]
["Hangnyomás szint","Fűtés","","Magas","dB(A)","49","","","52"]
["","","","Alacsony","dB(A)","46","","","49"]
["","Hűtés","","Alacsony","dB(A)","46","","","49"]
["","","","Magas","dB(A)","49","","","52"]
["Standard Accessories","Leeresztő aljzat","","","","1","","","1"]
["","Telepítési utasítás","","","","1","","","1"]
["Refrigerant","Charge","","","TCO2Eq","3.1","","","4.8"]
["","GWP","","","","2,087.5","","","2,087.5"]
["","Feltöltés","","","kg","1.5","","","2.3"]
["","Típus","","","","R-410A","","","R-410A"]
["Csőcsatlakozások","Szintkülönbség","IU - OU","Max.","m","20","","","20"]
["","További hűtőközeg utántöltés","","","kg/m","0,02 (10m-t meghaladó csőhosszhoz)","","","0,02 (10m-t meghaladó csőhosszhoz)"]
["Kompresszor","Típus","","","","Hermetikusan zárt lengő kompresszor","","","Hermetikusan zárt lengő kompresszor"]
["Méretek","Egység","","Szélesség","mm","825","","","900"]
["","","","Mélység","mm","300","","","320"]
["","","","Magasság","mm","735","","","770"]
["Tömeg","Egység","","","kg","48","","","71"]
["Power supply","fázis","","","","1~","","","1~"]
["","Frekvencia","","","Hz","50","","","50"]
["","Feszültség","","","V","220-240","","","220-240"]
["Notes","","","","","(1) - SL: A Légszállítási sebesség beállításának néma ventilátorszintje","(1) - 220V","","(1) - SL: A Légszállítási sebesség beállításának néma ventilátorszintje","(1) - 220V"]
["","","","","","(2) - Fluor-tartalmú, az ózonréteget károsító gázt tartalmaz","(2) - 230V","","(2) - Fluor-tartalmú, az ózonréteget károsító gázt tartalmaz","(2) - 230V"]
["Méretek","Egység","","Magasság","mm","","735","735","","770","770"]
["","","","Szélesség","mm","","825","825","","900","900"]
["","","","Mélység","mm","","300","300","","320","320"]
["Tömeg","Egység","","","kg","","48","48","","71","71"]
["Kompresszor","Típus","","","","","Hermetikusan zárt lengő kompresszor","Hermetikusan zárt lengő kompresszor","","Hermetikusan zárt lengő kompresszor","Hermetikusan zárt lengő kompresszor"]
["Üzemi tartomány","Hűtés","Környezeti","Min.","°C száraz hőm.","","-10","-10","","-10","-10"]
["","","","Max.","°C száraz hőm.","","46","46","","46","46"]
["","Fűtés","Környezeti","Min.","°C párás hőm.","","-15","-15","","-15","-15"]
["","","","Max.","°C párás hőm.","","18","20","","18","20"]
["Hangnyomás szint","Hűtés","","Magas","dB(A)","","49","49","","52","52"]
["","","","Alacsony","dB(A)","","46","46","","49","49"]
["","Fűtés","","Magas","dB(A)","","49","49","","52","52"]
["","","","Alacsony","dB(A)","","46","46","","49","49"]
["Hűtőközeg","Típus","","","","","R-410A","R-410A","","R-410A","R-410A"]
["","Töltet","","","kg","","1.5","1.5","","2.3","2.3"]
["","Töltet","","","tCO2Eq","","3.1","3.1","","4.8","4.8"]
["","GWP","","","","","2087.5","2087.5","","2087.5","2087.5"]
["Csőcsatlakozások","Csőhossz","Max.","OU - IU","m","","30","30","","30","30"]
["","További hűtőközeg utántöltés","","","kg/m","","0,02 (10m-t meghaladó csőhosszhoz)","0,02 (10m-t meghaladó csőhosszhoz)","","0,02 (10m-t meghaladó csőhosszhoz)","0,02 (10m-t meghaladó csőhosszhoz)"]
["","Szintkülönbség","IU - OU","Max.","m","","20","20","","20","20"]
["Standard Accessories","Installation manual","","","","","Installation manual","1","","Installation manual","1"]
["","Drain plug","","","","","Drain plug","","","Drain plug"]
["Áramellátás","fázis","","","","","1~","1~","","1~","1~"]
["","Frekvencia","","","Hz","","50","50","","50","50"]
["","Feszültség","","","V","","220-240","220-240","","220-240","220-240"]
["Notes","","","","","","(3) - 240V","","","(3) - 240V"]
["Standard Accessories","Drain socket","","","","","","1","","","1"]
["Sound power level","Hűtés","","","dB(A)","","","","65"]