{"text_format":"2","workbook":"xls","n_sheets":1,"sheets":["Products"],"not_rendered":{"charts":0,"images":0,"macros":0,"external_links":1,"defined_names":0,"comments":0,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"run_cost":"one","rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900","formulas":"cached_only"}

{"sheet":"Products","index":0,"n_rows":59,"n_cols":12,"rows_kept":59,"cut":false,"hidden":false,"merged":[],"flags":["formulas_cached_only"]}
["PRODUCT NAME","RXS-K"]
[]
[]
[]
[]
["","","","","","RXS20K3V1B","RXS20K2V1B","RXS25K3V1B","RXS25K2V1B","RXS35K2V1B","RXS42K2V1B","RXS50K2V1B"]
["Hangnyomás szint","Fűtés","","Magas","dB(A)","47","","47","","48","48","48"]
["","Hűtés","","Magas","dB(A)","46","","46","","48","48","48"]
["Standard Accessories","Csatlakozás (vízlevezetés)","","","","1","","1"]
["","Telepítési utasítás","","","","1","","1","","1","1","1"]
["Hűtőközeg","Charge","","","TCO2Eq","2.1","","2.1","","2.5","2.7","3.5"]
["","GWP","","","","2,087.5","","2,087.5","","2,087.5","2,087.5","2,087.5"]
["","Töltet","","","kg","1.0","","1.0","","1.2","1.3","1.7"]
["","Típus","","","","R-410A","","R-410A","","R-410A","R-410A","R-410A"]
["Ventilátormotor","Sebesség","Hűtés","Szuper alacsony","1/perc","780","","780","","780","790","670"]
["","","Fűtés","Szuper alacsony","1/perc","740","","740","","740","780","670"]
["Piping connections","Szintkülönbség","IU - OU","Max.","m","15","","15","","15","15","20"]
["","További hűtőközeg utántöltés","","","kg/m","0,02 (10m-t meghaladó csőhosszhoz)","","0,02 (10m-t meghaladó csőhosszhoz)","","0,02 (10m-t meghaladó csőhosszhoz)","0,02 (10m-t meghaladó csőhosszhoz)","0,02 (10m-t meghaladó csőhosszhoz)"]
["Kompresszor","Type","","","","Hermetikusan zárt lengő kompresszor","","Hermetikusan zárt lengő kompresszor","","Hermetikusan zárt lengő kompresszor","Hermetikusan zárt lengő kompresszor","Hermetikusan zárt lengő kompresszor"]
["Méretek","Berendezés","","Szélesség","mm","765","","765","","765","765","825"]
["","","","Mélység","mm","285","","285","","285","285","300"]
["","","","Magasság","mm","550","","550","","550","550","735"]
["Tömeg","Egység","","","kg","34","","34","","34","39","47"]
["Ventilátor","Légáramlási arány","Fűtés","Szuper alacsony","cfm","","","","","904","960","1,522"]
["","","Hűtés","Szuper alacsony","cfm","","","","","1,063","1,080","1,727"]
["Power supply","Phase","","","","1~","","1~","","1~","1~","1~"]
["","Frekvencia","","","Hz","50","","50","","50","50","50"]
["","Feszültség","","","V","220-240","","220-240","","220-240","220-240","220-240"]
["Notes","","","","","(1) - 220V","(1) - 220V","(1) - 220V","(1) - 220V","(1) - 220V","(1) - 220V","(1) - 220V"]
["","","","","","(2) - 230V","(2) - 230V","(2) - 230V","(2) - 230V","(2) - 230V","(2) - 230V","(2) - 230V"]
["","","","","","(3) - 240V","(3) - 240V","(3) - 240V","(3) - 240V","(3) - 240V","(3) - 240V","(3) - 240V"]
["","","","","","(4) - SL: A Légszállítási sebesség beállításának néma ventilátorszintje","","(4) - SL: A Légszállítási sebesség beállításának néma ventilátorszintje","","(4) - Fluor-tartalmú, az ózonréteget károsító gázt tartalmaz","(4) - Fluor-tartalmú, az ózonréteget károsító gázt tartalmaz","(4) - Fluor-tartalmú, az ózonréteget károsító gázt tartalmaz"]
["","","","","","(5) - Fluor-tartalmú, az ózonréteget károsító gázt tartalmaz","","(5) - Fluor-tartalmú, az ózonréteget károsító gázt tartalmaz"]
["Méretek","Egység","","Magasság","mm","","550","","550"]
["","","","Szélesség","mm","","765","","765"]
["","","","Mélység","mm","","285","","285"]
["Tömeg","Egység","","","kg","","34","","34"]
["Ventilátor motor","Sebesség","Hűtés","Szuper alacsony","1/perc","","780","","780"]
["","","Fűtés","Szuper alacsony","1/perc","","740","","740"]
["Kompresszor","Type","","","","","Hermetikusan zárt lengő kompresszor","","Hermetikusan zárt lengő kompresszor"]
["Üzemi tartomány","Hűtés","Környezeti","Min.","°C száraz hőm.","","-10","","-10"]
["","","","Max.","°C száraz hőm.","","46","","46"]
["","Fűtés","Környezeti","Min.","°C párás hőm.","","-15","","-15"]
["","","","Max.","°C párás hőm.","","18","","18"]
["Hangnyomás szint","Hűtés","","Magas","dB(A)","","46","","46"]
["","Fűtés","","Magas","dB(A)","","47","","47"]
["Hűtőközeg","Típus","","","","","R-410A","","R-410A"]
["","Töltet","","","kg","","1.0","","1.0"]
["","Töltet","","","tCO2Eq","","2.1","","2.1"]
["","GWP","","","","","2087.5","","2087.5"]
["Csőcsatlakozások","Csőhossz","Max.","OU - IU","m","","20","","20"]
["","További hűtőközeg utántöltés","","","kg/m","","0,02 (10m-t meghaladó csőhosszhoz)","","0,02 (10m-t meghaladó csőhosszhoz)"]
["","Szintkülönbség","IU - OU","Max.","m","","15","","15"]
["Standard Accessories","Installation manual","","","","","1","","1"]
["","Joint (drain)","","","","","1","","1"]
["Áramellátás","fázis","","","","","1~","","1~"]
["","Frekvencia","","","Hz","","50","","50"]
["","Feszültség","","","V","","220-240","","220-240"]
["Standard Accessories","Leeresztő csavar","","","","","","","","1","1","1"]