{"text_format":"2","workbook":"xls","n_sheets":1,"sheets":["Products"],"not_rendered":{"charts":0,"images":0,"macros":0,"external_links":1,"defined_names":0,"comments":0,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"run_cost":"one","rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900","formulas":"cached_only"}

{"sheet":"Products","index":0,"n_rows":73,"n_cols":11,"rows_kept":73,"cut":false,"hidden":false,"merged":[],"flags":["formulas_cached_only"]}
["PRODUCT NAME","RXS-L"]
[]
[]
[]
[]
["","","","","","RXS20L2V1B","RXS25L2V1B","RXS35L2V1B","RXS42L2V1B","RXS50L2V1B","RXS60L2V1B"]
["Hangnyomás szint","Fűtés","","Magas","dBA","47","47","48","48"]
["","Hűtés","","Magas","dBA","46","46","48","48"]
["Standard Accessories","Leeresztő sapka","","","","1","1","","1"]
["","Telepítési utasítás","","","","1","1","1","1"]
["","Hűtőközeg töltési címke","","","","1","1","1"]
["","Fluorinált káros gázokra vonatkozó többnyelvű címke","","","","1","1","Fluorinált káros gázokra vonatkozó többnyelvű címke"]
["Refrigerant","Charge","","","TCO2Eq","2.1","2.1","2.5","2.7"]
["","GWP","","","","2,087.5","2,087.5","2,087.5","2,087.5"]
["","Töltet","","","kg","1.0","1.0","1.20","1.3"]
["","Típus","","","","R-410A","R-410A","R-410A","R-410A"]
["Ventilátormotor","Sebesség","Hűtés","Szuper alacsony","ford./perc","780","780","780","790"]
["","","Fűtés","Szuper alacsony","ford./perc","740","740","740","780"]
["Üzemi tartomány","Hűtés","Környezeti","Max.","°C száraz hőm.","46","46","46","46"]
["","","","Min.","°C száraz hőm.","-10","-10","-10","-10"]
["","Fűtés","Környezeti","Max.","°C párás hőm.","18","18","18","18"]
["","","","Min.","°C párás hőm.","-15","-15","-15","-15"]
["Piping connections","Szintkülönbség","IU - OU","Max.","m","","","15"]
["","További hűtőközeg utántöltés","","","kg/m","","","0,020 (10m-t meghaladó csőhosszhoz)"]
["Méretek","Egység","","Szélesség","mm","765","765","765","765"]
["","","","Mélység","mm","285","285","285","285"]
["","","","Magasság","mm","550","550","550","550"]
["Compressor","Type","","","","Hermetikusan zárt lengő kompresszor","Hermetikusan zárt lengő kompresszor","Hermetikusan zárt lengő kompresszor","Hermetikusan zárt lengő kompresszor"]
["Tömeg","Egység","","","kg","34","34","34","39"]
["Ventilátor","Légszállítási sebesség","Fűtés","Szuper alacsony","cfm","904","904","904","960"]
["","","","Szuper alacsony","m³/perc","25.6","25.6","25.6","27.2"]
["","","Hűtés","Szuper alacsony","m³/perc","30.1","30.1","30.1","30.6"]
["","","","Szuper alacsony","cfm","1,063","1,063","1,063","1,080"]
["Power supply","Phase","","","","1~","1~","1~","1~"]
["","Frekvencia","","","Hz","50","50","50","50"]
["","Feszültség","","","V","220-240","220-240","220-240","220-240"]
["Notes","","","","","(1) - 220V","(1) - 220V","(1) - 220V","(1) - 220V","(1) - 220V"]
["","","","","","(2) - 230V","(2) - 230V","(2) - 230V","(2) - 230V","(2) - 230V"]
["","","","","","(3) - 240V","(3) - 240V","(3) - 240V","(3) - 240V","(3) - 240V"]
["","","","","","(4) - Fluor-tartalmú, az ózonréteget károsító gázt tartalmaz","(4) - Fluor-tartalmú, az ózonréteget károsító gázt tartalmaz","(4) - Fluor-tartalmú, az ózonréteget károsító gázt tartalmaz","(4) - Fluor-tartalmú, az ózonréteget károsító gázt tartalmaz"]
["Standard Accessories","Leeresztő csavar","","","","","","1"]
["Ventilátor","Légáramlási arány","Hűtés","Szuper alacsony","m³/perc","","","","","48.9","45.0"]
["","","Fűtés","Szuper alacsony","m³/perc","","","","","43.1","46.3"]
["","","","Szuper alacsony","cfm","","","","","1727","1589"]
["","","Fűtés","Szuper alacsony","cfm","","","","","1522","1635"]
["Méretek","Egység","","Magasság","mm","","","","","735","735"]
["","","","Szélesség","mm","","","","","825","825"]
["","","","Mélység","mm","","","","","300","300"]
["Tömeg","Egység","","","kg","","","","","47","48"]
["Ventilátor motor","Sebesség","Hűtés","Szuper alacsony","ford./perc","","","","","670"]
["","","Fűtés","Szuper alacsony","ford./perc","","","","","670"]
["Kompresszor","Típus","","","","","","","","Hermetikusan zárt lengő kompresszor","Hermetikusan zárt lengő kompresszor"]
["Üzemi tartomány","Hűtés","Környezeti","Min.","°C száraz hőm.","","","","","-10","-10"]
["","","","Max.","°C száraz hőm.","","","","","46","46"]
["","Fűtés","Környezeti","Min.","°C párás hőm.","","","","","-15","-15"]
["","","","Max.","°C párás hőm.","","","","","18","18"]
["Hangnyomás szint","Hűtés","","Magas","dBA","","","","","48","49"]
["","","","Alacsony","dBA","","","","","44","46"]
["","Fűtés","","Magas","dBA","","","","","48","49"]
["","","","Alacsony","dBA","","","","","45","46"]
["Hűtőközeg","Típus","","","","","","","","R-410A","R-410A"]
["","Töltet","","","kg","","","","","1.7","1.5"]
["","Töltet","","","tCO2Eq","","","","","3.5","3.1"]
["","GWP","","","","","","","","2087.5","2087.5"]
["Csőcsatlakozások","Csőhossz","Max.","OU - IU","m","","","","","30","30"]
["","További hűtőközeg utántöltés","","","kg/m","","","","","0,020 (10m-t meghaladó csőhosszhoz)","0,020 (10m-t meghaladó csőhosszhoz)"]
["","Szintkülönbség","IU - OU","Max.","m","","","","","20.0","20"]
["Standard Accessories","Installation manual","","","","","","","","1","1"]
["","Drain plug","","","","","","","","1","1"]
["Áramellátás","fázis","","","","","","","","1~","1~"]
["","Frekvencia","","","Hz","","","","","50","50"]
["","Feszültség","","","V","","","","","220-230-240","220-230-240"]
["Notes","","","","","","","","","","(1) - 230V"]