{"text_format":"2","workbook":"xls","n_sheets":1,"sheets":["Products"],"not_rendered":{"charts":0,"images":0,"macros":0,"external_links":1,"defined_names":0,"comments":0,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"run_cost":"one","rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900","formulas":"cached_only"}

{"sheet":"Products","index":0,"n_rows":36,"n_cols":6,"rows_kept":36,"cut":false,"hidden":false,"merged":[],"flags":["formulas_cached_only"]}
["PRODUCT NAME","RXTA-B"]
[]
[]
[]
[]
["","","","","","RXTA30B2V1B"]
["Méretek","Egység","","Magasság","mm","551"]
["","","","Szélesség","mm","763"]
["","","","Mélység","mm","312"]
["Tömeg","Egység","","","kg","38"]
["Ventilátor motor","Sebesség","Hűtés","Szuper alacsony","1/perc","450"]
["","","Fűtés","Szuper alacsony","1/perc","360"]
["Kompresszor","Típus","","","","Hermetikusan zárt lengő kompresszor"]
["Üzemi tartomány","Hűtés","Környezeti","Min.","°C száraz hőm.","-10"]
["","","","Max.","°C száraz hőm.","46"]
["","Fűtés","Környezeti","Min.","°C párás hőm.","-25"]
["","","","Max.","°C párás hőm.","18"]
["Hangnyomás szint","Hűtés","","Névl.","dB(A)","48"]
["","Fűtés","","Névl.","dB(A)","49"]
["Hűtőközeg","Típus","","","","R-32"]
["","Töltet","","","kg","1.1"]
["","Töltet","","","tCO2Eq","0.74"]
["","GWP","","","","675"]
["Csőcsatlakozások","Csőhossz","Max.","OU - IU","m","20"]
["","További hűtőközeg utántöltés","","","kg/m","0,02 (10m-t meghaladó csőhosszhoz)"]
["","Szintkülönbség","IU - OU","Max.","m","15"]
["Standard Accessories","Telepítési utasítás","","","","1"]
["","Hűtőközeg töltési címke","","","","1"]
["","Fluorinált káros gázokra vonatkozó többnyelvű címke","","","","1"]
["Energiatakarékossági besorolás","","","","","A+++ ~ D"]
["Áramellátás","fázis","","","","1~"]
["","Frekvencia","","","Hz","50"]
["","Feszültség","","","V","220-240"]
["Notes","","","","","(1) - Fluor-tartalmú, az ózonréteget károsító gázt tartalmaz"]
["","","","","","(2) - Az üzemi tartomány tekintetében ld. az önálló ábrát"]
["","","","","","(3) - Az elektromos adatokat lásd külön rajzokon"]