{"text_format":"2","workbook":"xls","n_sheets":1,"sheets":["Products"],"not_rendered":{"charts":0,"images":0,"macros":0,"external_links":1,"defined_names":0,"comments":0,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"run_cost":"one","rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900","formulas":"cached_only"}

{"sheet":"Products","index":0,"n_rows":32,"n_cols":9,"rows_kept":32,"cut":false,"hidden":false,"merged":[],"flags":["formulas_cached_only"]}
["PRODUCT NAME","RXV-AB"]
[]
[]
[]
[]
["","","","","","RXV25AV1B","RXV35AV1B","RXV50AV1B","RXV60AV1B"]
["Hangnyomás szint","Hűtés","","Névl.","dBA","","","","58"]
["Refrigerant","Charge","","","TCO2Eq","","","","4.3"]
["","GWP","","","","","","","2,087.5"]
["","Charge","","","kg","","","","2.05"]
["","Típus","","","","","","","R-410A"]
["Csőcsatlakozások","Szintkülönbség","IU - OU","Max.","m","","","","10"]
["Méretek","Egység","","Szélesség","mm","","","","980"]
["","","","Mélység","mm","","","","427"]
["","","","Magasság","mm","","","","790"]
["Tömeg","Egység","","","kg","","","","60"]
["Notes","","","","","","","","(1) - Fluor-tartalmú, az ózonréteget károsító gázt tartalmaz"]
["Méretek","Egység","","Magasság","mm","540","540","700"]
["","","","Szélesség","mm","776","776","955"]
["","","","Mélység","mm","320","320","396"]
["Tömeg","Egység","","","kg","28","29","45"]
["Üzemi tartomány","Hűtés","Környezeti","Min.","°C száraz hőm.","18","18","18"]
["","","","Max.","°C száraz hőm.","43","43","43"]
["","Fűtés","Környezeti","Min.","°C párás hőm.","-10","-10","-10"]
["","","","Max.","°C párás hőm.","24","24","24"]
["Hangnyomás szint","Hűtés","","Névl.","dBA","51","53","56"]
["Hűtőközeg","Típus","","","","R-410A","R-410A","R-410A"]
["","Töltet","","","kg","0.80","0.95","1.45"]
["","Töltet","","","tCO2Eq","1.7","2","3"]
["","GWP","","","","2087.5","2087.5","2087.5"]
["Csőcsatlakozások","Csőhossz","Max.","OU - IU","m","15","15","25"]
["","Szintkülönbség","IU - OU","Max.","m","10","10","10"]